IF 1(RR)

850

750

650 IF 2(RR)

50 -50

Plot file version 1 created 09-MAR-2004 16:59:44 J1126+45 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/13:04:18 to 00/13:05:28

ON - MC

IF 1(LL)

850

750

650 IF 2(LL)

50 0 ON - MC

IF 1(RR)

400

360

320 IF 2(RR)

10 -10 WB - MC

IF 1(LL)

420

380

340 IF 2(LL)

0 -20 WB - MC

IF 1(RR)

500

400 IF 2(RR)

20 -20 MC - NT

IF 1(LL)

400

300 IF 2(LL)

20 -20 MC - NT

IF 1(RR)

850

750

650 IF 2(RR)

100 0

Plot file version 2 created 09-MAR-2004 16:59:45 J1126+45 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/13:08:32 to 00/13:09:58

ON - MC

IF 1(LL)

800

700

600 IF 2(LL)

50 -50 ON - MC

IF 1(RR)

420

380

340 IF 2(RR)

5 -5 WB - MC

IF 1(LL)

380

340 IF 2(LL)

5 -5 WB - MC

IF 1(RR)

540 500 460 420 IF 2(RR)

10 -10 MC - NT

IF 1(LL)

460 420 380 340 IF 2(LL)

0 -40 MC - NT

IF 1(RR)

850

750

650 IF 2(RR)

50 -50

Plot file version 3 created 09-MAR-2004 16:59:45 J1126+45 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/13:13:02 to 00/13:14:28

ON - MC

IF 1(LL)

750

650

550 IF 2(LL)

50 -50 -150 ON - MC

IF 1(RR)

420

380

340 IF 2(RR)

5 -5 WB - MC

IF 1(LL)

420

380

340 IF 2(LL)

5 -5 WB - MC

IF 1(RR)

540 500 460 420 IF 2(RR)

0 -20 MC - NT

IF 1(LL)

450

350 IF 2(LL)

20 -20 MC - NT

IF 1(RR)

850

750

650 IF 2(RR)

40 0 -40

Plot file version 4 created 09-MAR-2004 16:59:45 J1126+45 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/13:17:32 to 00/13:18:58

ON - MC

IF 1(LL)

800

700

600 IF 2(LL)

60 20 -20 ON - MC

IF 1(RR)

360

320 IF 2(RR)

10 -10 WB - MC

IF 1(LL)

380

340

300 IF 2(LL)

5 -5 WB - MC

IF 1(RR)

560 520 480 440 IF 2(RR)

10 -10 MC - NT

IF 1(LL)

450

350 IF 2(LL)

20 -20 MC - NT

IF 1(RR)

4.4

4.0

3.6 IF 2(RR)

-15 -25

Plot file version 5 created 09-MAR-2004 16:59:45 J1625-25 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/13:23:32 to 00/13:24:58

ON - MC

IF 1(LL)

3.8

3.4 IF 2(LL)

-15 -25 ON - MC

IF 1(RR)

3.15

3.05

2.95 IF 2(RR)

-5 -10 WB - MC

IF 1(LL)

3.15

3.05

2.95 IF 2(LL)

-4 -8 WB - MC

IF 1(RR)

3.9

3.7 IF 2(RR)

16 12 MC - NT

IF 1(LL)

3.2

2.8

2.4 IF 2(LL)

18 14 10 MC - NT

IF 1(RR)

Channels

0 5 10 15

3.8

3.6

3.4

3.2 IF 2(RR)

0 5 10 15

26 22 18 MC - HH

IF 1(LL)

Channels

0 5 10 15

3.7

3.5 IF 2(LL)

0 5 10 15

25 15 MC - HH

IF 1(RR)

4.4

4.0

3.6 IF 2(RR)

15 5

Plot file version 6 created 09-MAR-2004 16:59:45 J1625-25 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/13:28:02 to 00/13:29:28

ON - MC

IF 1(LL)

4.0

3.6 IF 2(LL)

14 10 6 ON - MC

IF 1(RR)

3.05

2.95

2.85

IF 2(RR)

20 10 WB - MC

IF 1(LL)

3.10

3.00

2.90 IF 2(LL)

12 8 WB - MC

IF 1(RR)

4.0

3.8 IF 2(RR)

-6 -10 MC - NT

IF 1(LL)

3.2 2.8 2.4 IF 2(LL)

-8 -12 MC - NT

IF 1(RR)

Channels

0 5 10 15

3.7

3.5

3.3 IF 2(RR)

0 5 10 15

6 2 -2 MC - HH

IF 1(LL)

Channels

0 5 10 15

3.7

3.5

3.3 IF 2(LL)

0 5 10 15

0 -5 MC - HH

IF 1(RR)

3.20

3.10

3.00 IF 2(RR)

2 -2

Plot file version 7 created 09-MAR-2004 16:59:46 J1625-25 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/13:32:32 to 00/13:33:58

WB - MC

IF 1(LL)

3.1

2.9 IF 2(LL)

6 2 -2 WB - MC

IF 1(RR)

4.0

3.8 IF 2(RR)

12 8 MC - NT

IF 1(LL)

3.5

2.5 IF 2(LL)

18 14 10 MC - NT

IF 1(RR)

3.8

3.6

3.4 IF 2(RR)

25 15 5 MC - HH

IF 1(LL)

3.8

3.6

3.4 IF 2(LL)

15 5 MC - HH

IF 1(RR)

2.5

2.3 IF 2(RR)

-4 -8

Plot file version 8 created 09-MAR-2004 16:59:46 1504-166 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/13:35:53 to 00/13:40:37

ON - MC

IF 1(LL)

2.5

2.3

2.1 IF 2(LL)

-4 -8 ON - MC

IF 1(RR)

2.30

2.20 IF 2(RR)

-4 -8 WB - MC

IF 1(LL)

2.30

2.20 IF 2(LL)

-4 -8 WB - MC

IF 1(RR)

2.50

2.40

2.30

IF 2(RR)

5.4 5.0 MC - EF

IF 1(LL)

2.55

2.45

2.35

IF 2(LL)

5.0 4.0 MC - EF

IF 1(RR)

Channels

0 5 10 15

2.40

2.30 IF 2(RR)

0 5 10 15

-14 -18 MC - NT

IF 1(LL)

Channels

0 5 10 15

1.8

1.4 IF 2(LL)

0 5 10 15

-14 -18 MC - NT

IF 1(RR)

Channels

0 5 10 15

820 780 740 IF 2(RR)

0 5 10 15

-40 -60 MC - HH

IF 1(LL)

850

750 IF 2(LL)

-20 -60

Plot file version 9 created 09-MAR-2004 16:59:47 1504-166 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/13:35:53 to 00/13:40:37

MC - HH

IF 1(RR)

3.50

3.40

3.30 IF 2(RR)

0 -4

Plot file version 10 created 09-MAR-2004 16:59:47 J1625-25 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/13:42:34 to 00/13:43:44

WB - MC

IF 1(LL)

3.45

3.35

3.25

IF 2(LL)

0 -4 WB - MC

IF 1(RR)

3.8

3.6 IF 2(RR)

8.5 7.5 6.5 MC - EF

IF 1(LL)

3.90

3.80

3.70 IF 2(LL)

8.5 7.5 MC - EF

IF 1(RR)

4.2

4.0

3.8 IF 2(RR)

7 5 3 MC - NT

IF 1(LL)

3.4

3.0

2.6

2.2 IF 2(LL)

6 2 MC - NT

IF 1(RR)

Channels

0 5 10 15

3.4

3.0 IF 2(RR)

0 5 10 15

40 30 MC - HH

IF 1(LL)

Channels

0 5 10 15

3.6 3.2 2.8 2.4 IF 2(LL) 0 5 10 15

40 20 MC - HH

IF 1(RR)

3.1

2.9 IF 2(RR)

6 2 -2

Plot file version 11 created 09-MAR-2004 16:59:47 J1625-25 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/13:46:48 to 00/13:50:44

WB - MC

IF 1(LL)

3.15

3.05

2.95

IF 2(LL)

2 -2 WB - MC

IF 1(RR)

3.75

3.65

3.55 IF 2(RR)

1.0 0.0 MC - EF

IF 1(LL)

3.85

3.75

3.65

3.55

IF 2(LL)

2 0 MC - EF

IF 1(RR)

4.2 4.0 3.8 3.6 IF 2(RR)

10 0 MC - NT

IF 1(LL)

4.0

3.0

2.0 IF 2(LL)

90 70 MC - NT

IF 1(RR)

Channels

0 5 10 15

3.7

3.5

3.3 IF 2(RR) 0 5 10 15

10 6 2 MC - HH

IF 1(LL)

Channels

0 5 10 15

3.7

3.5

3.3 IF 2(LL)

0 5 10 15

8 4 MC - HH

IF 1(RR)

1.20

1.10 IF 2(RR)

5 -5 -15

Plot file version 12 created 09-MAR-2004 16:59:47 J1625-25 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/13:53:48 to 00/13:55:14

WB - MC

IF 1(LL)

1.25

1.15 IF 2(LL)

-10 -30 WB - MC

IF 1(RR)

4.3

4.1

3.9 IF 2(RR)

70 50 MC - NT

IF 1(RR)

2.45

2.35

2.25 IF 2(RR)

0 -4 -8

Plot file version 15 created 09-MAR-2004 16:59:48 1504-166 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/14:10:45 to 00/14:14:55

ON - MC

IF 1(LL)

2.40

2.30

2.20

2.10 IF 2(LL)

-6 -10 ON - MC

IF 1(RR)

2.20

2.10 IF 2(RR)

-6 -10 WB - MC

IF 1(LL)

2.15

2.05 IF 2(LL)

-8 -12 WB - MC

IF 1(RR)

2.45

2.35

2.25 IF 2(RR)

7 5 MC - EF

IF 1(LL)

2.40

2.30

2.20

IF 2(LL)

7 5 MC - EF

IF 1(RR)

Channels

0 5 10 15

2.40

2.30

2.20 IF 2(RR) 0 5 10 15

-11 -13 -15 MC - NT

IF 1(LL)

Channels

0 5 10 15

1.8

1.4 IF 2(LL)

0 5 10 15

-12 -16 MC - NT

IF 1(RR)

Channels

0 5 10 15

800

700 IF 2(RR)

0 5 10 15

-30 -50 MC - HH

IF 1(LL)

850

750 IF 2(LL)

-20 -60

Plot file version 16 created 09-MAR-2004 16:59:49 1504-166 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/14:10:45 to 00/14:14:55

MC - HH

IF 1(RR)

0.9

0.7 IF 2(RR)

20 -20 -60

Plot file version 17 created 09-MAR-2004 16:59:49 J1126+45 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/14:20:06 to 00/14:21:32

ON - MC

IF 1(LL)

800

600 IF 2(LL)

40 0 -40 ON - MC

IF 1(RR)

360

320 IF 2(RR)

2 -2 -6 MC - EF

IF 1(LL)

400

360

320 IF 2(LL)

5 -5 MC - EF

IF 1(RR)

600

500 IF 2(RR)

10 -10 MC - NT

IF 1(LL)

500

400

300 IF 2(LL)

20 -20 MC - NT

IF 1(RR)

0.9

0.7 IF 2(RR)

100 -100

Plot file version 18 created 09-MAR-2004 16:59:49 J1126+45 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/14:24:36 to 00/14:26:02

ON - MC

IF 1(LL)

800

700 IF 2(LL)

100 -100

ON - MC

IF 1(RR)

380

360

340

320 IF 2(RR)

5 -5 MC - EF

IF 1(LL)

370

350

330 IF 2(LL)

5 -5 MC - EF

IF 1(RR)

650

550

450 IF 2(RR)

0 -20 MC - NT

IF 1(LL)

550

450

350 IF 2(LL)

20 -20 MC - NT

IF 1(RR)

0.9

0.7 IF 2(RR)

100 -100

Plot file version 19 created 09-MAR-2004 16:59:50 J1126+45 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/14:29:06 to 00/14:30:32

ON - MC

IF 1(LL)

800

600 IF 2(LL)

100 -100

ON - MC

IF 1(RR)

380

340

300 IF 2(RR)

4 0 -4 MC - EF

IF 1(LL)

380

340

300 IF 2(LL)

5 -5 MC - EF

IF 1(RR)

550

450 IF 2(RR)

10 -10 MC - NT

IF 1(LL)

550

450

350 IF 2(LL)

10 -10 MC - NT

IF 1(RR)

8.5 8.3 8.1 7.9 IF 2(RR)

0.5 -0.5 -1.5

Plot file version 20 created 09-MAR-2004 16:59:50 4C39.25 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/14:33:05 to 00/14:37:47

ON - MC

IF 1(LL)

8.0

7.6

7.2 IF 2(LL)

1 -1 ON - MC

IF 1(RR)

400

300

200 IF 2(RR)

300 100 WB - MC

IF 1(LL)

300

200 IF 2(LL)

200 0 WB - MC

IF 1(RR)

6.6

6.4

6.2 IF 2(RR)

2.4 2.0 1.6 MC - EF

IF 1(LL)

6.7 6.5 6.3 6.1 IF 2(LL)

3.0 2.0 MC - EF

IF 1(RR)

Channels

0 5 10 15

650 550 450 350 IF 2(RR)

0 5 10 15

300 100 MC - NT

IF 1(LL)

Channels

0 5 10 15

550

450

350 IF 2(LL) 0 5 10 15

100 -100

MC - NT

IF 1(LL)

Channels

0 5 10 15

3.5

2.5 IF 2(LL) 0 5 10 15

300 100 MC - UR

IF 1(RR)

1.1

0.9 IF 2(RR)

-10 -30

Plot file version 21 created 09-MAR-2004 16:59:51 J1924+15 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/14:50:11 to 00/14:51:21

ON - MC

IF 1(LL)

1.2

1.0

0.8 IF 2(LL)

0 -20 ON - MC

IF 1(RR)

760

720

680 IF 2(RR)

0 -4 -8 WB - MC

IF 1(LL)

740

700 IF 2(LL)

15 5 -5 WB - MC

IF 1(RR)

740

700 IF 2(RR)

6 2 MC - EF

IF 1(LL)

740

700 IF 2(LL)

5 -5 MC - EF

IF 1(RR)

Channels

0 5 10 15

850

750

650 IF 2(RR)

0 5 10 15

10 0 MC - NT

IF 1(LL)

Channels

0 5 10 15

650

550

450 IF 2(LL)

0 5 10 15

0 -20 MC - NT

IF 1(LL)

Channels

0 5 10 15

2.6

2.2

1.8 IF 2(LL)

0 5 10 15

100 -100

MC - UR

IF 1(RR)

800

700

600 IF 2(RR)

100 -100

Plot file version 22 created 09-MAR-2004 16:59:51 J1922+08 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/14:54:25 to 00/14:55:51

ON - MC

IF 1(LL)

850 750 650 550 IF 2(LL)

100 -100

ON - MC

IF 1(RR)

260 240 220 200 IF 2(RR)

40 0 WB - MC

IF 1(LL)

260 240 220 200 IF 2(LL)

10 -10 WB - MC

IF 1(RR)

220

200

180 IF 2(RR)

-50 -60 MC - EF

IF 1(LL)

220

200

180 IF 2(LL)

-5 -15 MC - EF

IF 1(RR)

Channels

0 5 10 15

400

360

320

280 IF 2(RR) 0 5 10 15

40 0 -40 MC - NT

IF 1(LL)

Channels

0 5 10 15

340

300

260 IF 2(LL) 0 5 10 15

60 20 MC - NT

IF 1(LL)

Channels

0 5 10 15

2.4

2.0

1.6 IF 2(LL) 0 5 10 15

300 100 MC - UR

IF 1(RR)

650

550 IF 2(RR)

150 50 -50

Plot file version 23 created 09-MAR-2004 16:59:52 J1922+08 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/14:54:25 to 00/14:55:51

MC - HH

IF 1(RR)

1.2

1.0

0.8 IF 2(RR)

20 -20

Plot file version 24 created 09-MAR-2004 16:59:52 J1924+15 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/14:55:55 to 00/14:57:21

ON - MC

IF 1(LL)

1.3 1.1 0.9 0.7 IF 2(LL)

20 -20 -60 ON - MC

IF 1(RR)

760

720

680 IF 2(RR)

0 -10 WB - MC

IF 1(LL)

760 720 680 IF 2(LL)

0 -40 WB - MC

IF 1(RR)

800

760

720

680 IF 2(RR)

-10 -14 -18 MC - EF

IF 1(LL)

760

720

680 IF 2(LL)

140 100 MC - EF

IF 1(RR)

Channels

0 5 10 15

800

700

600 IF 2(RR) 0 5 10 15

5 -5 MC - NT

IF 1(LL)

Channels

0 5 10 15

600

400 IF 2(LL)

0 5 10 15

110 90 70 MC - NT

IF 1(RR)

Channels

0 5 10 15

650

550 IF 2(RR) 0 5 10 15

100 -100

MC - HH

IF 1(RR)

900 800 700 600 IF 2(RR)

100 -100

Plot file version 25 created 09-MAR-2004 16:59:52 J1922+08 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/15:00:25 to 00/15:01:51

ON - MC

IF 1(RR)

240 220

200 IF 2(RR)

-20 -60 WB - MC

IF 1(LL)

240

220 200 IF 2(LL)

20 0 WB - MC

IF 1(RR)

200

160 IF 2(RR)

35 25 15 MC - EF

IF 1(LL)

210

190

170 IF 2(LL)

-10 -30 MC - EF

IF 1(RR)

380

340 IF 2(RR)

80 40 MC - NT

IF 1(LL)

Channels

0 5 10 15

350

250 IF 2(LL)

0 5 10 15

100 0 MC - NT

IF 1(RR)

Channels

0 5 10 15

750

650

550 IF 2(RR)

0 5 10 15

300 100 MC - HH

IF 1(RR)

1.0

0.8 IF 2(RR)

20 0

Plot file version 26 created 09-MAR-2004 16:59:52 J1924+15 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/15:01:55 to 00/15:03:21

ON - MC

IF 1(LL)

1.00

0.90

0.80

IF 2(LL)

-40 -80 ON - MC

IF 1(RR)

800

700 IF 2(RR)

18 14 10 WB - MC

IF 1(LL)

780

740

700 IF 2(LL)

-20 -30 WB - MC

IF 1(RR)

740

700

660 IF 2(RR)

0 -4 MC - EF

IF 1(LL)

740

700

660 IF 2(LL)

50 30 MC - EF

IF 1(RR)

Channels

0 5 10 15

750

650 IF 2(RR)

0 5 10 15

-4 -8 -12 MC - NT

IF 1(LL)

Channels

0 5 10 15

600

400 IF 2(LL)

0 5 10 15

0 -40 MC - NT

IF 1(RR)

Channels

0 5 10 15

700

600 IF 2(RR)

0 5 10 15

100 -100

MC - HH

IF 1(RR)

1.0

0.8 IF 2(RR)

0 -20

Plot file version 27 created 09-MAR-2004 16:59:53 J1924+15 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/15:06:25 to 00/15:07:51

ON - MC

IF 1(LL)

1.05

0.95

0.85

0.75

IF 2(LL)

0 -20 ON - MC

IF 1(RR)

680

640

600 IF 2(RR)

2 -2 -6 WB - MC

IF 1(LL)

720 680 640 IF 2(LL)

0 -5 WB - MC

IF 1(RR)

740

700

660 IF 2(RR)

4 0 MC - EF

IF 1(LL)

740

700 IF 2(LL)

6 2 -2 MC - EF

IF 1(RR)

Channels

0 5 10 15

750

650 IF 2(RR)

0 5 10 15

2 -2 -6 MC - NT

IF 1(LL)

Channels

0 5 10 15

750 650 550 450 IF 2(LL)

0 5 10 15

0 -10 MC - NT

IF 1(RR)

Channels

0 5 10 15

800

700

600

500 IF 2(RR)

0 5 10 15

50 -50 MC - HH

IF 1(LL)

800

700

600 IF 2(LL)

100 -100

Plot file version 30 created 09-MAR-2004 16:59:54 J1924+15 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/15:10:55 to 00/15:12:21

MC - HH

IF 1(RR)

850

750

650

550 IF 2(RR)

100 -100

Plot file version 31 created 09-MAR-2004 16:59:54 J1922+08 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/15:12:25 to 00/15:13:51

ON - MC

IF 1(LL)

850 750 650 550 IF 2(LL)

200 0 ON - MC

IF 1(RR)

220

180 IF 2(RR)

100 60 WB - MC

IF 1(LL)

280

240

200 IF 2(LL)

200 100 WB - MC

IF 1(RR)

240

200

160 IF 2(RR)

110 90 MC - EF

IF 1(LL)

220 200 180 160 IF 2(LL)

120 80 MC - EF

IF 1(RR)

Channels

0 5 10 15

420 380 340 300 IF 2(RR) 0 5 10 15

150 100 MC - NT

IF 1(LL)

Channels

0 5 10 15

350

250 IF 2(LL) 0 5 10 15

180 140 100 MC - NT

IF 1(RR)

Channels

0 5 10 15

750

650

550

450 IF 2(RR) 0 5 10 15

100 -100 MC - HH

IF 1(LL)

750

650

550 IF 2(LL)

250 150 50

Plot file version 32 created 09-MAR-2004 16:59:54 J1922+08 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/15:12:25 to 00/15:13:51

MC - HH

IF 1(RR)

1.0

0.8 IF 2(RR)

0 -20

Plot file version 33 created 09-MAR-2004 16:59:54 J1924+15 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/15:13:55 to 00/15:15:21

ON - MC

IF 1(LL)

950 850 750 650 IF 2(LL)

20 -20 ON - MC

IF 1(RR)

740

700

660 IF 2(RR)

5 -5 WB - MC

IF 1(LL)

760

720

680 IF 2(LL)

10 0 WB - MC

IF 1(RR)

760

720

680 IF 2(RR)

0 -10 MC - EF

IF 1(LL)

780 740 700 660 IF 2(LL)

0 -4 -8 MC - EF

IF 1(RR)

Channels

0 5 10 15

800

760

720 IF 2(RR)

0 5 10 15

0 -10 MC - NT

IF 1(LL)

Channels

0 5 10 15

600

500

400 IF 2(LL)

0 5 10 15

10 -10 MC - NT

IF 1(RR)

Channels

0 5 10 15

700

600

500 IF 2(RR)

0 5 10 15

50 -50 -150

MC - HH

IF 1(LL)

700

600

500 IF 2(LL)

100 -100

Plot file version 34 created 09-MAR-2004 16:59:55 J1924+15 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/15:13:55 to 00/15:15:21

MC - HH

IF 1(RR)

1.2

1.0

0.8 IF 2(RR)

0 -20

Plot file version 35 created 09-MAR-2004 16:59:55 J1924+15 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/15:18:25 to 00/15:19:51

ON - MC

IF 1(LL)

1.0

0.8 IF 2(LL)

10 -10 ON - MC

IF 1(RR)

800 760 720 680 IF 2(RR)

5 -5 WB - MC

IF 1(LL)

740

700

660 IF 2(LL)

0 -4 -8 WB - MC

IF 1(RR)

780

740

700 IF 2(RR)

10 6 2 MC - EF

IF 1(LL)

800

700 IF 2(LL)

14 10 MC - EF

IF 1(RR)

Channels

0 5 10 15

780

740

700 IF 2(RR) 0 5 10 15

6 2 -2 MC - NT

IF 1(LL)

Channels

0 5 10 15

650

550

450 IF 2(LL)

0 5 10 15

5 -5 MC - NT

IF 1(RR)

Channels

0 5 10 15

800 700 600 500 IF 2(RR)

0 5 10 15

100 -100

MC - HH

IF 1(LL)

850 750 650 550 IF 2(LL)

50 -50 -150

Plot file version 36 created 09-MAR-2004 16:59:55 J1924+15 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/15:18:25 to 00/15:19:51

MC - HH

IF 1(RR)

1.2

1.0

0.8 IF 2(RR)

0 -20

Plot file version 37 created 09-MAR-2004 16:59:55 J1924+15 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/15:22:55 to 00/15:24:21

ON - MC

IF 1(LL)

0.95

0.85

0.75 IF 2(LL)

10 -10 ON - MC

IF 1(RR)

780

740

700 IF 2(RR)

6 2 -2 WB - MC

IF 1(LL)

800

700 IF 2(LL)

5 -5 WB - MC

IF 1(RR)

740

700 IF 2(RR)

-4 -8 MC - EF

IF 1(LL)

800 760 720 680 IF 2(LL)

-4 -8 MC - EF

IF 1(RR)

Channels

0 5 10 15

800 760 720 680 IF 2(RR)

0 5 10 15

5 -5 MC - NT

IF 1(LL)

Channels

0 5 10 15

650

550

450 IF 2(LL)

0 5 10 15

5 -5 MC - NT

IF 1(RR)

Channels

0 5 10 15

750

650

550 IF 2(RR)

0 5 10 15

100 -100

MC - HH

IF 1(LL)

800

700

600 IF 2(LL)

100 -100

Plot file version 38 created 09-MAR-2004 16:59:55 J1924+15 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/15:22:55 to 00/15:24:21

MC - HH

IF 1(RR)

0.9

0.7 IF 2(RR)

10 -10

Plot file version 39 created 09-MAR-2004 16:59:56 J1924+15 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/15:27:25 to 00/15:28:51

ON - MC

IF 1(LL)

0.9

0.7 IF 2(LL)

10 -10 ON - MC

IF 1(RR)

760

720

680 IF 2(RR)

4 0 -4 WB - MC

IF 1(LL)

740

700

660 IF 2(LL)

2 -2 WB - MC

IF 1(RR)

740

700

660 IF 2(RR)

4 0 MC - EF

IF 1(LL)

760

720

680 IF 2(LL)

2 -2 MC - EF

IF 1(RR)

Channels

0 5 10 15

800

700 IF 2(RR) 0 5 10 15

15 5 MC - NT

IF 1(LL)

Channels

0 5 10 15

650

550

450 IF 2(LL)

0 5 10 15

10 0 MC - NT

IF 1(RR)

9.0

8.6

8.2 IF 2(RR)

1 -1

Plot file version 40 created 09-MAR-2004 16:59:56 3C454.3 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/15:33:11 to 00/15:37:51

ON - MC

IF 1(LL)

8.6 8.2 7.8 7.4 IF 2(LL)

-1.0 -2.0

ON - MC

IF 1(RR)

12.0

11.6

11.2 IF 2(RR)

2 -2 WB - MC

IF 1(LL)

11.8

11.4

11.0

IF 2(LL)

2 -2 WB - MC

IF 1(RR)

11.6

11.2

10.8 IF 2(RR)

-0.8 -1.2 -1.6

MC - EF

IF 1(LL)

11.6

11.2

10.8 IF 2(LL)

-1.5

-2.5

MC - EF

IF 1(RR)

Channels

0 5 10 15

11.4

11.0

IF 2(RR)

0 5 10 15

2 0 MC - NT

IF 1(LL)

Channels

0 5 10 15

9

7 IF 2(LL)

0 5 10 15

3 1 MC - NT

IF 1(LL)

Channels

0 5 10 15

1.30

1.20 IF 2(LL)

0 5 10 15

5 -5 MC - SH

IF 1(RR)

1.15

1.05

0.95

0.85 IF 2(RR)

0 -20

Plot file version 41 created 09-MAR-2004 16:59:57 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/15:53:00 to 00/15:54:10

ON - MC

IF 1(LL)

1.2

1.0

0.8 IF 2(LL)

20 -20 ON - MC

IF 1(RR)

940 900 860 820 IF 2(RR)

0 -4 MC - EF

IF 1(LL)

900

860

820 IF 2(LL)

2 -2 -6 MC - EF

IF 1(LL)

1.0

0.8

0.6 IF 2(LL)

200 0 MC - SH

IF 1(RR)

1.10

1.00

0.90

0.80

IF 2(RR)

10 -10

Plot file version 42 created 09-MAR-2004 16:59:57 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/15:57:14 to 00/15:58:40

ON - MC

IF 1(LL)

1.05

0.95

0.85 IF 2(LL)

0 -20 ON - MC

IF 1(RR)

240

200

160 IF 2(RR)

100 -100

WB - MC

IF 1(LL)

240

200

160 IF 2(LL)

200 0 WB - MC

IF 1(RR)

900

860 IF 2(RR)

-2 -6 MC - EF

IF 1(LL)

920

880

840 IF 2(LL)

0 -4 MC - EF

IF 1(RR)

Channels

0 5 10 15

1.05

0.95 IF 2(RR)

0 5 10 15

0 -4 -8 MC - NT

IF 1(LL)

Channels

0 5 10 15

900 800 700 600 IF 2(LL)

0 5 10 15

10 -10 MC - NT

IF 1(LL)

950

850

750

650 IF 2(LL)

200 0

Plot file version 45 created 09-MAR-2004 16:59:59 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/16:06:14 to 00/16:07:40

MC - SH

IF 1(RR)

4.3

4.1

3.9 IF 2(RR)

7 5

Plot file version 46 created 09-MAR-2004 16:59:59 J0102+58 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/16:10:16 to 00/16:12:56

ON - MC

IF 1(LL)

4.0

3.6 IF 2(LL)

6 2 ON - MC

IF 1(RR)

4.20

4.10

4.00

3.90 IF 2(RR)

4 0 WB - MC

IF 1(LL)

4.2

4.0

3.8 IF 2(LL)

4 0 WB - MC

IF 1(RR)

4.15

4.05

3.95

3.85 IF 2(RR)

-1.8 -2.2 -2.6

MC - EF

IF 1(LL)

4.1

3.9 IF 2(LL)

-2.0

-3.0

MC - EF

IF 1(RR)

Channels

0 5 10 15

4.40

4.30

4.20

4.10 IF 2(RR) 0 5 10 15

-1 -3 MC - NT

IF 1(LL)

Channels

0 5 10 15

3.6 3.2 2.8 2.4 IF 2(LL)

0 5 10 15

2 -2 MC - NT

IF 1(LL)

Channels

0 5 10 15

4.0

3.6 IF 2(LL)

0 5 10 15

2 -2 -6 MC - UR

IF 1(LL)

3.2

3.0

2.8 IF 2(LL)

-2 -6

Plot file version 47 created 09-MAR-2004 17:00:00 J0102+58 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/16:10:16 to 00/16:12:56

MC - SH

IF 1(RR)

1.10

1.00

0.90 IF 2(RR)

0 -20

Plot file version 48 created 09-MAR-2004 17:00:00 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/16:14:40 to 00/16:15:52

ON - MC

IF 1(LL)

1.00

0.90

0.80 IF 2(LL)

0 -20 ON - MC

IF 1(RR)

240

200

160 IF 2(RR)

200 0 WB - MC

IF 1(LL)

240

200

160 IF 2(LL)

100 -100

WB - MC

IF 1(RR)

940

900

860 IF 2(RR)

8 6 MC - EF

IF 1(LL)

920 880 840 800 IF 2(LL)

10 6 MC - EF

IF 1(RR)

Channels

0 5 10 15

1.10

1.00

0.90 IF 2(RR)

0 5 10 15

5 -5 MC - NT

IF 1(LL)

Channels

0 5 10 15

900 800 700 600 IF 2(LL)

0 5 10 15

5 -5 MC - NT

IF 1(LL)

Channels

0 5 10 15

2.2

1.8 IF 2(LL)

0 5 10 15

100 -100

MC - UR

IF 1(LL)

950 850 750 650 IF 2(LL)

200 0

Plot file version 49 created 09-MAR-2004 17:00:00 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/16:14:40 to 00/16:15:52

MC - SH

IF 1(RR)

1.05

0.95

0.85 IF 2(RR)

10 -10 -30

Plot file version 50 created 09-MAR-2004 17:00:00 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/16:18:56 to 00/16:20:22

ON - MC

IF 1(LL)

0.9

0.7 IF 2(LL)

20 -20 ON - MC

IF 1(RR)

900

860

820 IF 2(RR)

1 -1 MC - EF

IF 1(LL)

920

880

840 IF 2(LL)

2 -2 MC - EF

IF 1(RR)

1.10

1.00

0.90

IF 2(RR)

5 -5 MC - NT

IF 1(LL)

800

600 IF 2(LL)

5 -5 MC - NT

IF 1(RR)

1.10

1.00

0.90

0.80

IF 2(RR)

10 -10

Plot file version 51 created 09-MAR-2004 17:00:00 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/16:23:26 to 00/16:24:52

ON - MC

IF 1(LL)

1.00

0.90

0.80 IF 2(LL)

20 0 ON - MC

IF 1(RR)

880

840

800 IF 2(RR)

0 -4 MC - EF

IF 1(LL)

880

840

800 IF 2(LL)

0 -4 MC - EF

IF 1(RR)

1.10

1.00

0.90 IF 2(RR)

0 -10 MC - NT

IF 1(LL)

800

600 IF 2(LL)

-5 -15 MC - NT

IF 1(RR)

1.0

0.8 IF 2(RR)

-10 -30

Plot file version 52 created 09-MAR-2004 17:00:00 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/16:27:56 to 00/16:29:22

ON - MC

IF 1(LL)

1.00

0.90

0.80 IF 2(LL)

0 -20 ON - MC

IF 1(RR)

880

840

800 IF 2(RR)

6 4 MC - EF

IF 1(LL)

900

860

820

780 IF 2(LL)

6 2 -2 MC - EF

IF 1(RR)

1.05

0.95 IF 2(RR)

10 0 MC - NT

IF 1(LL)

800

600 IF 2(LL)

10 -10 MC - NT

IF 1(LL)

Channels

0 5 10 15

2.4

2.0

1.6 IF 2(LL)

0 5 10 15

100 -100

MC - UR

IF 1(LL)

Channels

0 5 10 15

1.0

0.8

0.6 IF 2(LL)

0 5 10 15

300 100 MC - SH

IF 1(RR)

4.3

4.1

3.9 IF 2(RR)

4 2

Plot file version 53 created 09-MAR-2004 17:00:01 J0102+58 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/16:31:59 to 00/16:34:39

ON - MC

IF 1(LL)

4.0

3.8

3.6 IF 2(LL)

5 3 1 ON - MC

IF 1(RR)

3.65

3.55

3.45

3.35 IF 2(RR)

4 0 WB - MC

IF 1(LL)

3.60

3.50

3.40 IF 2(LL)

6 2 WB - MC

IF 1(RR)

3.95

3.85

3.75

IF 2(RR)

-1.6 -2.0 -2.4

MC - EF

IF 1(LL)

3.95

3.85

3.75 IF 2(LL)

-1.0 -2.0

MC - EF

IF 1(RR)

Channels

0 5 10 15

4.35

4.25

4.15

4.05 IF 2(RR) 0 5 10 15

-2 -4 MC - NT

IF 1(LL)

Channels

0 5 10 15

3.6 3.2 2.8 2.4 IF 2(LL)

0 5 10 15

0 -4 MC - NT

IF 1(LL)

Channels

0 5 10 15

4.0

3.6 IF 2(LL) 0 5 10 15

5 -5 MC - UR

IF 1(LL)

2.9

2.7 IF 2(LL)

0 -4

Plot file version 54 created 09-MAR-2004 17:00:02 J0102+58 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/16:31:59 to 00/16:34:39

MC - SH

IF 1(RR)

1.15

1.05

0.95

0.85 IF 2(RR)

0 -20

Plot file version 55 created 09-MAR-2004 17:00:02 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/16:36:25 to 00/16:37:35

ON - MC

IF 1(LL)

1.10

1.00

0.90

0.80 IF 2(LL)

10 -10 -30 ON - MC

IF 1(RR)

900

860

820 IF 2(RR)

4 0 MC - EF

IF 1(LL)

880

840

800 IF 2(LL)

4 0 MC - EF

IF 1(RR)

1.15

1.05

0.95

0.85

IF 2(RR)

10 0 MC - NT

IF 1(LL)

800

600 IF 2(LL)

5 -5 MC - NT

IF 1(LL)

Channels

0 5 10 15

2.6

2.2

1.8 IF 2(LL)

0 5 10 15

300 100 MC - UR

IF 1(LL)

Channels

0 5 10 15

800

600 IF 2(LL) 0 5 10 15

300 100 MC - SH

IF 1(RR)

1.05

0.95

0.85 IF 2(RR)

0 -20

Plot file version 56 created 09-MAR-2004 17:00:02 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/16:40:39 to 00/16:42:05

ON - MC

IF 1(LL)

0.95

0.85

0.75 IF 2(LL)

10 -10 -30 ON - MC

IF 1(RR)

300

200 IF 2(RR)

300 100 WB - MC

IF 1(LL)

240

200

160 IF 2(LL)

100 -100

WB - MC

IF 1(RR)

940

900

860 IF 2(RR)

8 6 MC - EF

IF 1(LL)

920

880

840 IF 2(LL)

12 8 4 MC - EF

IF 1(RR)

Channels

0 5 10 15

1.05

0.95 IF 2(RR)

0 5 10 15

6 2 -2 MC - NT

IF 1(LL)

Channels

0 5 10 15

800

600 IF 2(LL)

0 5 10 15

10 0 MC - NT

IF 1(LL)

Channels

0 5 10 15

2.6

2.2

1.8 IF 2(LL)

0 5 10 15

100 -100

MC - UR

IF 1(LL)

700

500 IF 2(LL)

200 0

Plot file version 57 created 09-MAR-2004 17:00:03 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/16:40:39 to 00/16:42:05

MC - SH

IF 1(RR)

1.00

0.90

0.80

IF 2(RR)

15 5 -5

Plot file version 60 created 09-MAR-2004 17:00:04 J1924+15 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/16:57:36 to 00/16:58:46

ON - MC

IF 1(LL)

1.05

0.95

0.85 IF 2(LL)

10 -10 ON - MC

IF 1(RR)

760 720 680 640 IF 2(RR)

10 0 WB - MC

IF 1(LL)

700

660 IF 2(LL)

4 0 WB - MC

IF 1(RR)

750

730

710 IF 2(RR)

-3 -5 MC - EF

IF 1(LL)

730 710 690 670 IF 2(LL)

-1 -3 -5 MC - EF

IF 1(RR)

Channels

0 5 10 15

850

750

650 IF 2(RR)

0 5 10 15

-5 -15 MC - NT

IF 1(LL)

Channels

0 5 10 15

650

550

450 IF 2(LL)

0 5 10 15

-5 -15 MC - NT

IF 1(LL)

Channels

0 5 10 15

2.4

2.0

1.6 IF 2(LL)

0 5 10 15

100 -100 MC - UR

IF 1(RR)

900

800

700

600 IF 2(RR)

150 50 -50

Plot file version 61 created 09-MAR-2004 17:00:04 J1924+15 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/16:57:36 to 00/16:58:46

MC - HH

IF 1(LL)

800

700

600 IF 2(LL)

100 -100 MC - HH

IF 1(RR)

800

700

600 IF 2(RR)

100 -100

Plot file version 62 created 09-MAR-2004 17:00:04 J1922+08 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/17:01:50 to 00/17:03:16

ON - MC

IF 1(LL)

800

700

600 IF 2(LL)

100 -100 ON - MC

IF 1(RR)

240

200 IF 2(RR)

0 -40 WB - MC

IF 1(LL)

250

230

210

190 IF 2(LL)

0 -40 WB - MC

IF 1(RR)

210

190

170 IF 2(RR)

5 -5 MC - EF

IF 1(LL)

210

190

170 IF 2(LL)

0 -20 MC - EF

IF 1(RR)

Channels

0 5 10 15

380

340

300 IF 2(RR) 0 5 10 15

80 40 MC - NT

IF 1(LL)

Channels

0 5 10 15

350

250 IF 2(LL) 0 5 10 15

100 0 MC - NT

IF 1(LL)

Channels

0 5 10 15

4

2

0 IF 2(LL)

0 5 10 15

200 0 MC - UR

IF 1(RR)

1.1

0.9

0.7 IF 2(RR)

30 10 -10

Plot file version 63 created 09-MAR-2004 17:00:05 J1924+15 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/17:03:20 to 00/17:04:46

ON - MC

IF 1(LL)

1.0

0.8 IF 2(LL)

-100

-140

ON - MC

IF 1(RR)

700

600 IF 2(RR)

12 8 WB - MC

IF 1(LL)

660

620 IF 2(LL)

160 120 WB - MC

IF 1(RR)

760

720

680 IF 2(RR)

-6 -10 -14 MC - EF

IF 1(LL)

700

660

620 IF 2(LL)

45 35 MC - EF

IF 1(RR)

Channels

0 5 10 15

800

700 IF 2(RR)

0 5 10 15

-10 -20 MC - NT

IF 1(LL)

Channels

0 5 10 15

750 650

550 450 IF 2(LL) 0 5 10 15

200 160 MC - NT

IF 1(RR)

850

750

650 IF 2(RR)

200 0

Plot file version 64 created 09-MAR-2004 17:00:06 J1922+08 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/17:07:50 to 00/17:09:16

ON - MC

IF 1(LL)

750

650

550 IF 2(LL)

50 -50 -150

ON - MC

IF 1(RR)

220

180 IF 2(RR)

0 -40 WB - MC

IF 1(LL)

260

220

180 IF 2(LL)

20 -20 WB - MC

IF 1(RR)

200

180

160 IF 2(RR)

15 5 MC - EF

IF 1(LL)

210

190

170 IF 2(LL)

-5 -15 -25 MC - EF

IF 1(RR)

Channels

0 5 10 15

420

380

340

300 IF 2(RR)

0 5 10 15

80 40 MC - NT

IF 1(LL)

Channels

0 5 10 15

350

250 IF 2(LL)

0 5 10 15

100 0 MC - NT

IF 1(RR)

1.05

0.95

0.85

0.75

IF 2(RR)

60 20 -20

Plot file version 65 created 09-MAR-2004 17:00:06 J1924+15 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/17:09:20 to 00/17:10:46

ON - MC

IF 1(LL)

1.00

0.90

0.80

IF 2(LL)

40 0 -40 ON - MC

IF 1(RR)

680

640

600 IF 2(RR)

2 -2 WB - MC

IF 1(LL)

680

640

600 IF 2(LL)

20 -20 WB - MC

IF 1(RR)

760

720

680 IF 2(RR)

6 2 MC - EF

IF 1(LL)

760

720

680 IF 2(LL)

50 30 MC - EF

IF 1(RR)

Channels

0 5 10 15

750

650 IF 2(RR)

0 5 10 15

-6 -10 -14 MC - NT

IF 1(LL)

Channels

0 5 10 15

650

550

450 IF 2(LL)

0 5 10 15

50 -50 MC - NT

IF 1(RR)

Channels

0 5 10 15

800

700

600 IF 2(RR)

0 5 10 15

0 -40 -80 MC - HH

IF 1(RR)

1.00

0.90

0.80

IF 2(RR)

10 -10

Plot file version 66 created 09-MAR-2004 17:00:07 J1924+15 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/17:13:50 to 00/17:15:16

ON - MC

IF 1(LL)

1.00

0.90

0.80 IF 2(LL)

10 -10 ON - MC

IF 1(RR)

760 720 680 640 IF 2(RR)

2 -2 -6 WB - MC

IF 1(LL)

740

700

660

620 IF 2(LL)

2 -2 -6 WB - MC

IF 1(RR)

740

700

660 IF 2(RR)

10 6 2 MC - EF

IF 1(LL)

720 680 640 600 IF 2(LL)

7 5 3 MC - EF

IF 1(RR)

Channels

0 5 10 15

800

760

720

680 IF 2(RR)

0 5 10 15

0 -10 MC - NT

IF 1(LL)

Channels

0 5 10 15

600

500

400 IF 2(LL)

0 5 10 15

5 -5 -15 MC - NT

IF 1(RR)

Channels

0 5 10 15

700

600 IF 2(RR)

0 5 10 15

40 0 -40 MC - HH

IF 1(LL)

850

750

650 IF 2(LL)

300 100

Plot file version 67 created 09-MAR-2004 17:00:07 J1924+15 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/17:13:50 to 00/17:15:16

MC - HH

IF 1(RR)

1.0

0.8 IF 2(RR)

10 -10

Plot file version 68 created 09-MAR-2004 17:00:07 J1924+15 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/17:18:20 to 00/17:19:46

ON - MC

IF 1(LL)

1.0

0.8 IF 2(LL)

10 -10 ON - MC

IF 1(RR)

660

620

580 IF 2(RR)

5 -5 WB - MC

IF 1(LL)

660

620

580 IF 2(LL)

2 -2 -6 WB - MC

IF 1(RR)

760

720

680 IF 2(RR)

6 2 -2 MC - EF

IF 1(LL)

740

700

660 IF 2(LL)

4 0 -4 MC - EF

IF 1(RR)

Channels

0 5 10 15

850

750

650 IF 2(RR) 0 5 10 15

0 -10 MC - NT

IF 1(LL)

Channels

0 5 10 15

700 600 500

400 IF 2(LL)

0 5 10 15

5 -5 -15 MC - NT

IF 1(RR)

Channels

0 5 10 15

750

650

550 IF 2(RR)

0 5 10 15

50 -50 MC - HH

IF 1(LL)

850

750

650

550 IF 2(LL)

50 -50

Plot file version 69 created 09-MAR-2004 17:00:08 J1924+15 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/17:18:20 to 00/17:19:46

MC - HH

IF 1(RR)

800

700

600 IF 2(RR)

100 -100

Plot file version 70 created 09-MAR-2004 17:00:08 J1922+08 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/17:19:50 to 00/17:21:16

ON - MC

IF 1(LL)

0.9

0.7

0.5 IF 2(LL)

300 100 ON - MC

IF 1(RR)

260

220

180 IF 2(RR)

250 150 WB - MC

IF 1(LL)

250

150 IF 2(LL)

300 200 WB - MC

IF 1(RR)

200

160 IF 2(RR)

110 90 MC - EF

IF 1(RR)

420 380 340 300 IF 2(RR)

200 150 MC - NT

IF 1(LL)

Channels

0 5 10 15

450

350

250 IF 2(LL)

0 5 10 15

300 100 MC - NT

IF 1(RR)

Channels

0 5 10 15

800

700

600 IF 2(RR)

0 5 10 15

100 -100

MC - HH

IF 1(RR)

1.15

1.05

0.95

0.85 IF 2(RR)

0 -20

Plot file version 71 created 09-MAR-2004 17:00:09 J1924+15 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/17:21:20 to 00/17:22:46

ON - MC

IF 1(RR)

660

620

580 IF 2(RR)

0 -4 -8 WB - MC

IF 1(RR)

800

760

720 IF 2(RR)

8 4 MC - EF

IF 1(RR)

800

700 IF 2(RR)

0 -10 MC - NT

IF 1(RR)

750

650

550 IF 2(RR)

60 20 -20 MC - HH

IF 1(RR)

1.05

0.95

0.85

IF 2(RR)

10 -10

Plot file version 72 created 09-MAR-2004 17:00:09 J1924+15 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/17:25:50 to 00/17:27:16

ON - MC

IF 1(LL)

1.0

0.8 IF 2(LL)

20 0 ON - MC

IF 1(RR)

730 710 690 670 IF 2(RR)

2 -2 -6 WB - MC

IF 1(LL)

700

600 IF 2(LL)

2 -2 -6 WB - MC

IF 1(RR)

760

720

680 IF 2(RR)

10 6 MC - EF

IF 1(LL)

740

700

660 IF 2(LL)

44 40 MC - EF

IF 1(RR)

Channels

0 5 10 15

800

700 IF 2(RR)

0 5 10 15

5 -5 MC - NT

IF 1(LL)

Channels

0 5 10 15

650

550

450 IF 2(LL)

0 5 10 15

60 40 MC - NT

IF 1(RR)

Channels

0 5 10 15

750

650

550 IF 2(RR)

0 5 10 15

100 -100

MC - HH

IF 1(LL)

800

700

600 IF 2(LL)

0 -100

Plot file version 75 created 09-MAR-2004 17:00:11 J1924+15 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/17:30:20 to 00/17:31:46

MC - HH

IF 1(RR)

1.05

0.95

0.85 IF 2(RR)

10 -10

Plot file version 76 created 09-MAR-2004 17:00:11 J1924+15 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/17:34:50 to 00/17:36:16

ON - MC

IF 1(LL)

1.05

0.95

0.85

0.75

IF 2(LL)

-10 -30 ON - MC

IF 1(RR)

720

680

640 IF 2(RR)

12 8 4 WB - MC

IF 1(LL)

740 700 660 620 IF 2(LL)

0 -10 WB - MC

IF 1(RR)

780

740

700 IF 2(RR)

-4 -8 -12 MC - EF

IF 1(LL)

760

720 680 640 IF 2(LL)

12 8 MC - EF

IF 1(RR)

Channels

0 5 10 15

800

700

600 IF 2(RR)

0 5 10 15

0 -10 MC - NT

IF 1(LL)

Channels

0 5 10 15

700

600

500

400 IF 2(LL)

0 5 10 15

10 0 MC - NT

IF 1(LL)

Channels

0 5 10 15

2.6

2.2

1.8 IF 2(LL)

0 5 10 15

100 -100 MC - UR

IF 1(RR)

750

650 IF 2(RR)

100 -100

Plot file version 77 created 09-MAR-2004 17:00:12 J1924+15 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/17:34:50 to 00/17:36:16

MC - HH

IF 1(LL)

0.9

0.7 IF 2(LL)

200 0 MC - HH

IF 1(RR)

11.2

10.8

10.4 IF 2(RR)

3 1

Plot file version 78 created 09-MAR-2004 17:00:12 3C454.3 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/17:41:46 to 00/17:46:28

ON - MC

IF 1(LL)

10.5

9.5 IF 2(LL)

3 1 ON - MC

IF 1(RR)

10.6

10.2

9.8 IF 2(RR)

4 0 WB - MC

IF 1(LL)

10.8

10.4

10.0 IF 2(LL)

6 2 WB - MC

IF 1(RR)

10.8

10.4

10.0

IF 2(RR)

-4.6 -5.0 -5.4

MC - EF

IF 1(LL)

10.8

10.4

10.0

9.6 IF 2(LL)

-6 -8 MC - EF

IF 1(RR)

Channels

0 5 10 15

10.0

9.6 IF 2(RR)

0 5 10 15

10 8 MC - NT

IF 1(LL)

Channels

0 5 10 15

8.0

7.0

6.0 IF 2(LL)

0 5 10 15

11 9 7 MC - NT

IF 1(LL)

Channels

0 5 10 15

3.7 3.5 3.3 3.1 IF 2(LL) 0 5 10 15

10 0 MC - UR

IF 1(LL)

1.90

1.80

1.70

1.60 IF 2(LL)

4 0

Plot file version 79 created 09-MAR-2004 17:00:13 3C454.3 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/17:41:46 to 00/17:46:28

MC - SH

IF 1(RR)

5.3

5.1 IF 2(RR)

3 1 MC - HH

IF 1(LL)

5.5

5.3

5.1 IF 2(LL)

-1 -3 -5 MC - HH

IF 1(RR)

1.0

0.8 IF 2(RR)

10 -10 -30

Plot file version 80 created 09-MAR-2004 17:00:13 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/17:52:53 to 00/17:54:07

ON - MC

IF 1(LL)

0.9

0.7 IF 2(LL)

10 -10 ON - MC

IF 1(RR)

900 860 820 780 IF 2(RR)

5 -5 WB - MC

IF 1(LL)

850

750 IF 2(LL)

0 -5 WB - MC

IF 1(RR)

1.0

0.8 IF 2(RR)

0 -20 MC - NT

IF 1(LL)

900

700

500 IF 2(LL)

100 60 MC - NT

IF 1(LL)

Channels

0 5 10 15

2.4

2.0

1.6 IF 2(LL)

0 5 10 15

100 -100

MC - UR

IF 1(LL)

Channels

0 5 10 15

1.0

0.8

0.6 IF 2(LL)

0 5 10 15

100 -100

MC - SH

IF 1(RR)

1.05

0.95

0.85 IF 2(RR)

20 -20

Plot file version 81 created 09-MAR-2004 17:00:14 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/17:57:11 to 00/17:58:37

ON - MC

IF 1(LL)

950

850

750 IF 2(LL)

10 -10 ON - MC

IF 1(RR)

900 860 820 IF 2(RR)

6 2 -2 WB - MC

IF 1(LL)

900

800 IF 2(LL)

6 2 -2 WB - MC

IF 1(RR)

920

880

840 IF 2(RR)

0 -4 MC - EF

IF 1(LL)

900

860

820 IF 2(LL)

2 -2 MC - EF

IF 1(RR)

Channels

0 5 10 15

1.00

0.90 IF 2(RR)

0 5 10 15

0 -10 MC - NT

IF 1(LL)

Channels

0 5 10 15

850 750 650 550 IF 2(LL)

0 5 10 15

0 -10 MC - NT

IF 1(RR)

1.00

0.90

0.80

IF 2(RR)

0 -20

Plot file version 82 created 09-MAR-2004 17:00:14 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/18:01:41 to 00/18:03:07

ON - MC

IF 1(LL)

1.00

0.90

0.80 IF 2(LL)

10 -10 ON - MC

IF 1(RR)

900

860

820

780 IF 2(RR)

2 -2 -6 WB - MC

IF 1(LL)

860

820 IF 2(LL)

5 -5 WB - MC

IF 1(RR)

900

800 IF 2(RR)

4 0 MC - EF

IF 1(LL)

900

860

820

780 IF 2(LL)

3 1 MC - EF

IF 1(RR)

Channels

0 5 10 15

1.00

0.90 IF 2(RR)

0 5 10 15

5 -5 MC - NT

IF 1(LL)

Channels

0 5 10 15

800

600 IF 2(LL)

0 5 10 15

5 -5 MC - NT

IF 1(RR)

1.0

0.8 IF 2(RR)

20 -20

Plot file version 83 created 09-MAR-2004 17:00:15 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/18:06:11 to 00/18:07:37

ON - MC

IF 1(LL)

0.95

0.85

0.75 IF 2(LL)

0 -20 ON - MC

IF 1(RR)

900

860

820 IF 2(RR)

0 -4 -8 WB - MC

IF 1(LL)

920

880

840

800 IF 2(LL)

-2 -6 WB - MC

IF 1(RR)

880

840

800 IF 2(RR)

1 -1 MC - EF

IF 1(LL)

880

840

800 IF 2(LL)

2 -2 MC - EF

IF 1(RR)

Channels

0 5 10 15

1.00

0.90

IF 2(RR)

0 5 10 15

10 0 MC - NT

IF 1(LL)

Channels

0 5 10 15

800

600 IF 2(LL)

0 5 10 15

10 6 2 MC - NT

IF 1(LL)

Channels

0 5 10 15

2.2

1.8 IF 2(LL)

0 5 10 15

100 -100

MC - UR

IF 1(LL)

850

750

650 IF 2(LL)

200 0

Plot file version 84 created 09-MAR-2004 17:00:16 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/18:06:11 to 00/18:07:37

MC - SH

IF 1(RR)

4.5

4.3

4.1

3.9 IF 2(RR)

4 0

Plot file version 85 created 09-MAR-2004 17:00:16 J0102+58 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/18:09:50 to 00/18:12:32

ON - MC

IF 1(LL)

4.3

4.1

3.9

3.7 IF 2(LL)

2 0 ON - MC

IF 1(RR)

4.15

4.05

3.95

3.85

IF 2(RR)

4 0 WB - MC

IF 1(LL)

4.1

3.9 IF 2(LL)

2 -2 WB - MC

IF 1(RR)

3.9

3.7 IF 2(RR)

0.4 0.0 -0.4

MC - EF

IF 1(LL)

4.0

3.8 IF 2(LL)

0.5 -0.5

MC - EF

IF 1(RR)

Channels

0 5 10 15

4.25

4.15

4.05 IF 2(RR)

0 5 10 15

0 -2 MC - NT

IF 1(LL)

Channels

0 5 10 15

3.6

3.2

2.8

2.4 IF 2(LL)

0 5 10 15

-1 -3 MC - NT

IF 1(LL)

Channels

0 5 10 15

4.0

3.6

3.2 IF 2(LL)

0 5 10 15

2 -2 -6 MC - UR

IF 1(LL)

3.2

3.0 IF 2(LL)

2 -2

Plot file version 86 created 09-MAR-2004 17:00:17 J0102+58 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/18:09:50 to 00/18:12:32

MC - SH

IF 1(RR)

1.0

0.8 IF 2(RR)

20 -20

Plot file version 87 created 09-MAR-2004 17:00:17 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/18:14:40 to 00/18:15:52

ON - MC

IF 1(LL)

950

850

750 IF 2(LL)

10 -10 ON - MC

IF 1(RR)

850

750 IF 2(RR)

5 -5 WB - MC

IF 1(LL)

880 840 800 760 IF 2(LL)

0 -10 WB - MC

IF 1(RR)

860

820

780 IF 2(RR)

-2 -6 MC - EF

IF 1(LL)

860

820

780 IF 2(LL)

4 0 MC - EF

IF 1(RR)

Channels

0 5 10 15

1.05

0.95

0.85 IF 2(RR) 0 5 10 15

5 0 MC - NT

IF 1(LL)

Channels

0 5 10 15

800

600 IF 2(LL)

0 5 10 15

10 -10 MC - NT

IF 1(LL)

Channels

0 5 10 15

2.1

1.9 1.7 IF 2(LL) 0 5 10 15

300 100 MC - UR

IF 1(RR)

1.00

0.90

0.80 IF 2(RR)

0 -20

Plot file version 90 created 09-MAR-2004 17:00:18 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/18:23:26 to 00/18:24:52

ON - MC

IF 1(LL)

0.95

0.85

0.75 IF 2(LL)

20 -20 ON - MC

IF 1(RR)

860 820 780 740 IF 2(RR)

-6 -10 WB - MC

IF 1(LL)

820

780

740 IF 2(LL)

6 2 -2 WB - MC

IF 1(RR)

1.00

0.90 IF 2(RR)

15 5 MC - NT

IF 1(LL)

800

600 IF 2(LL)

5 -5 MC - NT

IF 1(RR)

1.00

0.90

0.80 IF 2(RR)

10 -10

Plot file version 91 created 09-MAR-2004 17:00:19 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/18:27:56 to 00/18:29:22

ON - MC

IF 1(LL)

1.05

0.95

0.85

0.75 IF 2(LL)

0 -20 ON - MC

IF 1(RR)

800

700 IF 2(RR)

0 -4 -8 WB - MC

IF 1(LL)

820

780

740 IF 2(LL)

-2 -6 -10 WB - MC

IF 1(RR)

1.00

0.90 IF 2(RR)

6 2 MC - NT

IF 1(LL)

800

600 IF 2(LL)

10 0 MC - NT

IF 1(LL)

Channels

0 5 10 15

2.4

2.0

1.6 IF 2(LL)

0 5 10 15

200 0 MC - UR

IF 1(LL)

Channels

0 5 10 15

800

700

600 IF 2(LL)

0 5 10 15

100 -100

MC - SH

IF 1(RR)

4.5

4.3

4.1 IF 2(RR)

1 -1

Plot file version 92 created 09-MAR-2004 17:00:20 J0102+58 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/18:31:36 to 00/18:34:16

ON - MC

IF 1(LL)

4.1

3.9

3.7 IF 2(LL)

1 -1 ON - MC

IF 1(RR)

4.1

3.9 IF 2(RR)

2 -2 WB - MC

IF 1(LL)

4.2

4.0 IF 2(LL)

2 -2 WB - MC

IF 1(RR)

4.25

4.15

4.05

3.95 IF 2(RR)

-1 -3 MC - NT

IF 1(LL)

3.6 3.2 2.8 2.4 IF 2(LL)

0 -2 MC - NT

IF 1(LL)

Channels

0 5 10 15

4.2

3.8 IF 2(LL)

0 5 10 15

0 -5 MC - UR

IF 1(LL)

Channels

0 5 10 15

3.2

3.0 IF 2(LL)

0 5 10 15

0 -4 MC - SH

IF 1(RR)

1.05

0.95

0.85 IF 2(RR)

10 -10

Plot file version 93 created 09-MAR-2004 17:00:21 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/18:36:25 to 00/18:37:37

ON - MC

IF 1(LL)

950

850

750 IF 2(LL)

10 -10 -30 ON - MC

IF 1(RR)

860

820 IF 2(RR)

2 -2 -6 WB - MC

IF 1(LL)

940

900

860

820 IF 2(LL)

-5 -15 WB - MC

IF 1(RR)

1.00

0.90

IF 2(RR)

5 -5 MC - NT

IF 1(LL)

900

700

500 IF 2(LL)

5 -5 MC - NT

IF 1(LL)

Channels

0 5 10 15

2.6 2.2 1.8 1.4 IF 2(LL)

0 5 10 15

200 0 MC - UR

IF 1(LL)

Channels

0 5 10 15

800

600 IF 2(LL)

0 5 10 15

300 100 MC - SH

IF 1(RR)

1.0

0.8 IF 2(RR)

0 -10

Plot file version 94 created 09-MAR-2004 17:00:22 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/18:40:41 to 00/18:42:07

ON - MC

IF 1(LL)

0.9

0.7 IF 2(LL)

20 -20 ON - MC

IF 1(RR)

880 840 800 760 IF 2(RR)

-4 -8 WB - MC

IF 1(LL)

880

840

800 IF 2(LL)

5 -5 WB - MC

IF 1(RR)

1.00

0.90

IF 2(RR)

4 0 -4 MC - NT

IF 1(LL)

900 800 700 600 IF 2(LL)

6 2 -2 MC - NT

IF 1(LL)

Channels

0 5 10 15

2.4

2.0

1.6 IF 2(LL)

0 5 10 15

100 -100

MC - UR

IF 1(LL)

Channels

0 5 10 15

800

600 IF 2(LL)

0 5 10 15

100 -100

MC - SH

IF 1(RR)

4.6

4.4

4.2 IF 2(RR)

4 0

Plot file version 95 created 09-MAR-2004 17:00:23 J0102+58 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/18:44:21 to 00/18:46:01

ON - MC

IF 1(LL)

4.3

4.1

3.9

3.7 IF 2(LL)

-12 -16 -20 ON - MC

IF 1(RR)

4.1

3.9 IF 2(RR)

3 1 -1 WB - MC

IF 1(LL)

4.2

4.0 IF 2(LL)

2 -2 WB - MC

IF 1(RR)

4.25

4.15

4.05

3.95 IF 2(RR)

1 -1 MC - NT

IF 1(LL)

3.6

3.2

2.8

2.4 IF 2(LL)

2 -2 MC - NT

IF 1(LL)

Channels

0 5 10 15

4.2 3.8 3.4 3.0 IF 2(LL) 0 5 10 15

0 -10 MC - UR

IF 1(LL)

Channels

0 5 10 15

3.4

3.2

3.0 IF 2(LL) 0 5 10 15

20 0 MC - SH

IF 1(RR)

1.0

0.8 IF 2(RR)

10 -10 -30

Plot file version 96 created 09-MAR-2004 17:00:23 J1924+15 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/18:57:55 to 00/18:59:05

ON - MC

IF 1(LL)

1.00

0.90

0.80 IF 2(LL)

10 -10 ON - MC

IF 1(RR)

700

660

620 IF 2(RR)

6 2 -2 WB - MC

IF 1(LL)

700 660 620 580 IF 2(LL)

5 -5 WB - MC

IF 1(RR)

800

700 IF 2(RR)

-5 -15 MC - NT

IF 1(LL)

700

500 IF 2(LL)

0 -20 MC - NT

IF 1(LL)

Channels

0 5 10 15

2.4

2.0

1.6 IF 2(LL)

0 5 10 15

300 100 MC - UR

IF 1(RR)

Channels

0 5 10 15

1.0

0.8

0.6 IF 2(RR)

0 5 10 15

100 -100

MC - HH

IF 1(LL)

Channels

0 5 10 15

1.0

0.6 IF 2(LL)

0 5 10 15

200 0 MC - HH

IF 1(RR)

950

850

750

650 IF 2(RR)

100 -100

Plot file version 97 created 09-MAR-2004 17:00:24 J1922+08 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/19:02:09 to 00/19:03:35

ON - MC

IF 1(LL)

850

750

650 IF 2(LL)

100 -100

ON - MC

IF 1(RR)

250 230 210 190 IF 2(RR)

20 -20 WB - MC

IF 1(LL)

250

230

210 IF 2(LL)

20 -20 WB - MC

IF 1(RR)

450

350 IF 2(RR)

50 -50 MC - NT

IF 1(LL)

400

300 IF 2(LL)

100 60 20 MC - NT

IF 1(RR)

1.00

0.90

0.80

IF 2(RR)

10 -10

Plot file version 98 created 09-MAR-2004 17:00:25 J1924+15 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/19:03:39 to 00/19:05:05

ON - MC

IF 1(LL)

1.1

0.9

0.7 IF 2(LL)

10 -10 ON - MC

IF 1(RR)

640

600

560 IF 2(RR)

10 0 WB - MC

IF 1(LL)

620

580

540 IF 2(LL)

8 4 WB - MC

IF 1(RR)

900

800

700 IF 2(RR)

-15 -25 MC - NT

IF 1(LL)

700

600

500 400 IF 2(LL)

-10 -30 MC - NT

IF 1(RR)

950 850 750 650 IF 2(RR)

100 -100

Plot file version 99 created 09-MAR-2004 17:00:26 J1922+08 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/19:08:09 to 00/19:09:35

ON - MC

IF 1(LL)

900

800

700

600 IF 2(LL)

100 -100

ON - MC

IF 1(RR)

230

210

190 IF 2(RR)

30 10 -10 WB - MC

IF 1(LL)

240

200 IF 2(LL)

0 -40 WB - MC

IF 1(RR)

400

300 IF 2(RR)

100 0 MC - NT

IF 1(LL)

400 360 320 280 IF 2(LL)

200 0 MC - NT

IF 1(RR)

1.0

0.8 IF 2(RR)

10 -10

Plot file version 100 created 09-MAR-2004 17:00:26 J1924+15 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/19:09:39 to 00/19:11:05

ON - MC

IF 1(LL)

1.10

1.00

0.90

0.80 IF 2(LL)

10 -10 ON - MC

IF 1(RR)

540

500

460 IF 2(RR)

5 0 WB - MC

IF 1(LL)

580

540

500

460 IF 2(LL)

-10 -30 WB - MC

IF 1(RR)

800

700 IF 2(RR)

-10 -20 MC - NT

IF 1(LL)

750

650

550

450 IF 2(LL)

0 -20 MC - NT

IF 1(RR)

1.05

0.95

0.85 IF 2(RR)

0 -20

Plot file version 101 created 09-MAR-2004 17:00:27 J1924+15 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/19:14:09 to 00/19:15:35

ON - MC

IF 1(LL)

1.05

0.95

0.85

0.75 IF 2(LL)

10 -10 ON - MC

IF 1(RR)

700 660 620 580 IF 2(RR)

0 -10 WB - MC

IF 1(LL)

660

620

580 IF 2(LL)

5 -5 WB - MC

IF 1(RR)

750

650 IF 2(RR)

0 -10 MC - NT

IF 1(LL)

650

550

450 IF 2(LL)

5 -5 -15 MC - NT

IF 1(RR)

1.00

0.90

0.80

IF 2(RR)

0 -20

Plot file version 102 created 09-MAR-2004 17:00:28 J1924+15 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/19:18:39 to 00/19:20:05

ON - MC

IF 1(LL)

1.0

0.8 IF 2(LL)

20 -20 ON - MC

IF 1(RR)

720

680

640 IF 2(RR)

2 -2 -6 WB - MC

IF 1(LL)

700 660 620 580 IF 2(LL)

0 -10 WB - MC

IF 1(RR)

800

700 IF 2(RR)

0 -10 MC - NT

IF 1(LL)

600

400 IF 2(LL)

5 -5 -15 MC - NT

IF 1(RR)

1.05

0.95

0.85 IF 2(RR)

10 -10

Plot file version 105 created 09-MAR-2004 17:00:30 J1924+15 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/19:26:09 to 00/19:27:35

ON - MC

IF 1(LL)

1.10

1.00

0.90

0.80 IF 2(LL)

20 -20 ON - MC

IF 1(RR)

680

640

600 IF 2(RR)

-5 -15 WB - MC

IF 1(LL)

680

640

600 IF 2(LL)

0 -10 WB - MC

IF 1(RR)

720

680 IF 2(RR)

-8 -12 MC - EF

IF 1(LL)

740

700

660 IF 2(LL)

-18 -22 MC - EF

IF 1(RR)

Channels

0 5 10 15

800

700 IF 2(RR)

0 5 10 15

0 -10 MC - NT

IF 1(LL)

Channels

0 5 10 15

750 650 550 450 IF 2(LL)

0 5 10 15

5 -5 -15 MC - NT

IF 1(RR)

1.15

1.05

0.95

0.85 IF 2(RR)

-10 -30

Plot file version 106 created 09-MAR-2004 17:00:31 J1924+15 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/19:30:39 to 00/19:32:05

ON - MC

IF 1(LL)

1.10

1.00

0.90

0.80

IF 2(LL)

30 10 -10 ON - MC

IF 1(RR)

700

660

620

580 IF 2(RR)

0 -4 -8 WB - MC

IF 1(LL)

680 640 600 560 IF 2(LL)

0 -10 WB - MC

IF 1(RR)

120

80 IF 2(RR)

300 100 MC - EF

IF 1(LL)

120

100 IF 2(LL)

100 -100 MC - EF

IF 1(RR)

Channels

0 5 10 15

800

700 IF 2(RR)

0 5 10 15

10 0 MC - NT

IF 1(LL)

Channels

0 5 10 15

650

550

450 IF 2(LL)

0 5 10 15

0 -10 MC - NT

IF 1(RR)

1.2

1.0

0.8 IF 2(RR)

10 -10

Plot file version 107 created 09-MAR-2004 17:00:32 J1924+15 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/19:35:09 to 00/19:36:35

ON - MC

IF 1(LL)

1.1

0.9

0.7 IF 2(LL)

10 -10 ON - MC

IF 1(RR)

700 660 620 580 IF 2(RR)

0 -10 WB - MC

IF 1(LL)

680

640

600 IF 2(LL)

0 -4 -8 WB - MC

IF 1(RR)

120

100

80 IF 2(RR)

100 -100 MC - EF

IF 1(LL)

130

110

90 IF 2(LL)

100 -100 MC - EF

IF 1(RR)

Channels

0 5 10 15

900

800

700 IF 2(RR)

0 5 10 15

-5 -15 MC - NT

IF 1(LL)

Channels

0 5 10 15

700 600 500 400 IF 2(LL)

0 5 10 15

-10 -20 MC - NT

IF 1(RR)

Channels

0 5 10 15

0.95

0.85

0.75

IF 2(RR)

0 5 10 15

100 -100 MC - HH

IF 1(LL)

1.0

0.8 IF 2(LL)

100 -100

Plot file version 108 created 09-MAR-2004 17:00:33 J1924+15 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/19:35:09 to 00/19:36:35

MC - HH

IF 1(RR)

9.8

9.4

9.0 IF 2(RR)

5.5 4.5

Plot file version 109 created 09-MAR-2004 17:00:33 3C454.3 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/19:42:01 to 00/19:46:41

ON - MC

IF 1(LL)

9.2

8.8

8.4 IF 2(LL)

4 2 ON - MC

IF 1(RR)

8.4

8.0

7.6 IF 2(RR)

4 0 WB - MC

IF 1(LL)

8.4 8.2 8.0 7.8 IF 2(LL)

4 0 WB - MC

IF 1(RR)

8.9 8.7 8.5 8.3 IF 2(RR)

-6.8 -7.2

MC - EF

IF 1(LL)

8.8

8.4 IF 2(LL)

-6.0 -7.0 MC - EF

IF 1(RR)

Channels

0 5 10 15

8.4

8.0 IF 2(RR)

0 5 10 15

13 11 MC - NT

IF 1(LL)

Channels

0 5 10 15

7.0

6.0

5.0 IF 2(LL)

0 5 10 15

14 12 MC - NT

IF 1(LL)

Channels

0 5 10 15

3.2

3.0

2.8 IF 2(LL) 0 5 10 15

0 -20 MC - UR

IF 1(RR)

4.6

4.4

4.2 IF 2(RR)

6 4

Plot file version 110 created 09-MAR-2004 17:00:34 3C454.3 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/19:42:01 to 00/19:46:41

MC - HH

IF 1(LL)

4.7

4.5

4.3 IF 2(LL)

6 2 MC - HH

IF 1(RR)

1.3 1.1 0.9 0.7 IF 2(RR)

20 -20

Plot file version 111 created 09-MAR-2004 17:00:34 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/19:55:19 to 00/19:56:29

ON - MC

IF 1(LL)

1.1

0.9

0.7 IF 2(LL)

80 40 0 ON - MC

IF 1(RR)

900

800 IF 2(RR)

4 0 -4 WB - MC

IF 1(LL)

900 860 820 780 IF 2(LL)

5 -5 WB - MC

IF 1(RR)

1.4

1.0

0.6 IF 2(RR)

50 -50 MC - NT

IF 1(LL)

800

400

0 IF 2(LL)

-60 -100 -140

MC - NT

IF 1(LL)

Channels

0 5 10 15

3.0

2.0 IF 2(LL)

0 5 10 15

300 100 MC - UR

IF 1(RR)

Channels

0 5 10 15

1.0

0.8

0.6 IF 2(RR)

0 5 10 15

300 100 MC - HH

IF 1(LL)

Channels

0 5 10 15

1.1 0.9 0.7 0.5 IF 2(LL) 0 5 10 15

100 -100

MC - HH

IF 1(RR)

1.00

0.90

0.80 IF 2(RR)

20 -20

Plot file version 112 created 09-MAR-2004 17:00:35 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/19:59:33 to 00/20:00:59

ON - MC

IF 1(LL)

1.00

0.90

0.80

0.70 IF 2(LL)

20 -20 ON - MC

IF 1(RR)

900

800 IF 2(RR)

2 -2 -6 WB - MC

IF 1(LL)

900

800 IF 2(LL)

2 -2 -6 WB - MC

IF 1(RR)

920

880

840 IF 2(RR)

4 0 MC - EF

IF 1(LL)

920

880

840 IF 2(LL)

1 -1 MC - EF

IF 1(RR)

Channels

0 5 10 15

1.00

0.90 IF 2(RR)

0 5 10 15

5 -5 MC - NT

IF 1(LL)

Channels

0 5 10 15

800

600 IF 2(LL)

0 5 10 15

0 -10 MC - NT

IF 1(LL)

Channels

0 5 10 15

750

650

550 IF 2(LL)

0 5 10 15

100 -100

MC - SH

IF 1(RR)

1.10

1.00

0.90

0.80

IF 2(RR)

10 -10

Plot file version 113 created 09-MAR-2004 17:00:36 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/20:04:03 to 00/20:05:29

ON - MC

IF 1(LL)

0.95

0.85 IF 2(LL)

10 -10 ON - MC

IF 1(RR)

880

840

800 IF 2(RR)

2 -2 -6 WB - MC

IF 1(LL)

940 900 860 820 IF 2(LL)

4 0 -4 WB - MC

IF 1(RR)

880

840 IF 2(RR)

-2 -4 MC - EF

IF 1(LL)

900 880 860 840 IF 2(LL)

-2 -6 MC - EF

IF 1(RR)

Channels

0 5 10 15

0.95

0.85

IF 2(RR)

0 5 10 15

2 -2 -6 MC - NT

IF 1(LL)

Channels

0 5 10 15

850 750 650 550 IF 2(LL)

0 5 10 15

0 -4 -8 MC - NT

IF 1(RR)

1.0

0.8 IF 2(RR)

10 -10

Plot file version 114 created 09-MAR-2004 17:00:37 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/20:08:33 to 00/20:09:59

ON - MC

IF 1(LL)

0.9

0.7 IF 2(LL)

20 0 ON - MC

IF 1(RR)

920 880 840 800 IF 2(RR)

0 -4 WB - MC

IF 1(LL)

920

880

840 IF 2(LL)

2 -2 -6 WB - MC

IF 1(RR)

900

860 IF 2(RR)

2 -2 MC - EF

IF 1(LL)

920

880

840 IF 2(LL)

2 -2 MC - EF

IF 1(RR)

Channels

0 5 10 15

1.00

0.90 IF 2(RR)

0 5 10 15

6 2 -2 MC - NT

IF 1(LL)

Channels

0 5 10 15

800

600 IF 2(LL)

0 5 10 15

5 -5 MC - NT

IF 1(LL)

Channels

0 5 10 15

850

750

650 IF 2(LL)

0 5 10 15

100 -100

MC - SH

IF 1(RR)

4.8

4.6

4.4 IF 2(RR)

-1 -3

Plot file version 115 created 09-MAR-2004 17:00:38 J0102+58 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/20:12:10 to 00/20:14:52

ON - MC

IF 1(LL)

4.5

4.3

4.1 IF 2(LL)

-1 -3 ON - MC

IF 1(RR)

4.3

4.1 IF 2(RR)

2 -2 WB - MC

IF 1(LL)

4.5

4.3

4.1 IF 2(LL)

2 -2 WB - MC

IF 1(RR)

4.3

4.1

3.9 IF 2(RR)

0.6 0.2 -0.2

MC - EF

IF 1(LL)

4.2

4.0 IF 2(LL)

0.5 -0.5

MC - EF

IF 1(RR)

Channels

0 5 10 15

4.3

4.1 IF 2(RR)

0 5 10 15

1 -1 MC - NT

IF 1(LL)

Channels

0 5 10 15

3.4 3.0 2.6 IF 2(LL)

0 5 10 15

2 -2 MC - NT

IF 1(LL)

Channels

0 5 10 15

3.4

3.2

3.0 IF 2(LL)

0 5 10 15

2 -2 MC - SH

IF 1(RR)

1.05

0.95

0.85 IF 2(RR)

10 -10

Plot file version 116 created 09-MAR-2004 17:00:39 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/20:17:01 to 00/20:18:13

ON - MC

IF 1(LL)

0.95

0.85

0.75 IF 2(LL)

10 -10 ON - MC

IF 1(RR)

900

860

820 IF 2(RR)

5 -5 WB - MC

IF 1(LL)

920

880

840 IF 2(LL)

5 -5 WB - MC

IF 1(RR)

940

900 IF 2(RR)

0 -2 MC - EF

IF 1(LL)

960

920 IF 2(LL)

1 -1 MC - EF

IF 1(RR)

Channels

0 5 10 15

1.05

0.95

0.85

IF 2(RR)

0 5 10 15

5 -5 MC - NT

IF 1(LL)

Channels

0 5 10 15

850

750

650

550 IF 2(LL)

0 5 10 15

10 -10 MC - NT

IF 1(LL)

Channels

0 5 10 15

800

600 IF 2(LL)

0 5 10 15

300 100 MC - SH

IF 1(RR)

0.95

0.85 IF 2(RR)

10 -10

Plot file version 117 created 09-MAR-2004 17:00:40 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/20:21:17 to 00/20:22:43

ON - MC

IF 1(LL)

0.95

0.85

0.75 IF 2(LL)

10 -10 ON - MC

IF 1(RR)

880

840

800 IF 2(RR)

5 -5 WB - MC

IF 1(LL)

900

800 IF 2(LL)

2 -2 -6 WB - MC

IF 1(RR)

920

880 IF 2(RR)

0 -2 MC - EF

IF 1(LL)

940

900

860 IF 2(LL)

0 -4 MC - EF

IF 1(RR)

Channels

0 5 10 15

0.95

0.85 IF 2(RR) 0 5 10 15

2 -2 -6 MC - NT

IF 1(LL)

Channels

0 5 10 15

850 750 650 550 IF 2(LL)

0 5 10 15

0 -10 MC - NT

IF 1(RR)

4.8

4.6

4.4 IF 2(RR)

-1 -3 -5

Plot file version 120 created 09-MAR-2004 17:00:43 J0102+58 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/20:33:56 to 00/20:36:36

ON - MC

IF 1(LL)

4.5

4.3

4.1 IF 2(LL)

0 -4 ON - MC

IF 1(RR)

4.1

3.9 IF 2(RR)

2 -2 WB - MC

IF 1(LL)

4.25

4.15

4.05

3.95 IF 2(LL)

2 -2 WB - MC

IF 1(RR)

4.3

4.1 IF 2(RR)

0.4 0.0 MC - EF

IF 1(LL)

4.5

4.3

4.1 IF 2(LL)

0.5 -0.5 MC - EF

IF 1(RR)

Channels

0 5 10 15

4.30

4.20

4.10

4.00

IF 2(RR)

0 5 10 15

0 -2 MC - NT

IF 1(LL)

Channels

0 5 10 15

3.5

2.5 IF 2(LL) 0 5 10 15

0 -2 MC - NT

IF 1(LL)

Channels

0 5 10 15

3.3

3.1

2.9 IF 2(LL) 0 5 10 15

2 -2 MC - SH

IF 1(RR)

1.1

0.9

0.7 IF 2(RR)

20 -20

Plot file version 121 created 09-MAR-2004 17:00:44 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/20:38:46 to 00/20:39:58

ON - MC

IF 1(LL)

900

800

700 IF 2(LL)

0 -40 ON - MC

IF 1(RR)

860

820

780 IF 2(RR)

4 0 -4 WB - MC

IF 1(LL)

850

750 IF 2(LL)

5 -5 WB - MC

IF 1(RR)

940

900

860 IF 2(RR)

0 -4 MC - EF

IF 1(LL)

940

900

860 IF 2(LL)

1 -1 -3 MC - EF

IF 1(RR)

Channels

0 5 10 15

1.00

0.90 IF 2(RR)

0 5 10 15

5 -5 MC - NT

IF 1(LL)

Channels

0 5 10 15

850 750 650 550 IF 2(LL)

0 5 10 15

0 -10 MC - NT

IF 1(LL)

Channels

0 5 10 15

800

700

600 IF 2(LL)

0 5 10 15

200 0 MC - SH

IF 1(RR)

1.10

1.00

0.90

0.80 IF 2(RR)

30 10 -10

Plot file version 122 created 09-MAR-2004 17:00:45 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/20:43:02 to 00/20:44:28

ON - MC

IF 1(LL)

1.0

0.8 IF 2(LL)

20 0 ON - MC

IF 1(RR)

840

800

760 IF 2(RR)

-2 -6 WB - MC

IF 1(LL)

860

820

780

740 IF 2(LL)

0 -4 -8 WB - MC

IF 1(RR)

960

920

880 IF 2(RR)

1 -1 -3 MC - EF

IF 1(LL)

940

900 IF 2(LL)

0 -2 MC - EF

IF 1(RR)

Channels

0 5 10 15

1.00

0.90

IF 2(RR)

0 5 10 15

8 4 0 MC - NT

IF 1(LL)

Channels

0 5 10 15

700

500 IF 2(LL)

0 5 10 15

5 -5 MC - NT

IF 1(LL)

Channels

0 5 10 15

2.0

1.6 IF 2(LL)

0 5 10 15

200 0 MC - UR

IF 1(LL)

900

700

500 IF 2(LL)

200 0

Plot file version 123 created 09-MAR-2004 17:00:46 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/20:43:02 to 00/20:44:28

MC - SH

IF 1(RR)

4.7

4.5

4.3 IF 2(RR)

-4 -6

Plot file version 124 created 09-MAR-2004 17:00:46 J0102+58 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/20:46:38 to 00/20:48:22

ON - MC

IF 1(LL)

4.6

4.4

4.2

4.0 IF 2(LL)

-2 -6 ON - MC

IF 1(RR)

4.1

3.9 IF 2(RR)

2 -2 WB - MC

IF 1(LL)

4.25

4.15

4.05

3.95

IF 2(LL)

2 -2 WB - MC

IF 1(RR)

4.4

4.2 IF 2(RR)

0.0 -0.5

MC - EF

IF 1(LL)

4.50

4.40

4.30

4.20 IF 2(LL)

0.5 -0.5 -1.5

MC - EF

IF 1(RR)

Channels

0 5 10 15

4.20

4.10

4.00 IF 2(RR)

0 5 10 15

0 -4 MC - NT

IF 1(LL)

Channels

0 5 10 15

3.6 3.2 2.8 2.4 IF 2(LL) 0 5 10 15

0 -4 MC - NT

IF 1(LL)

Channels

0 5 10 15

4.4

4.0

3.6 IF 2(LL) 0 5 10 15

5 -5 MC - UR

IF 1(LL)

3.2

3.0 IF 2(LL)

2 -2

Plot file version 125 created 09-MAR-2004 17:00:47 J0102+58 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/20:46:38 to 00/20:48:22

MC - SH

IF 1(RR)

0.9

0.7 IF 2(RR)

0 -40

Plot file version 126 created 09-MAR-2004 17:00:47 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/20:51:08 to 00/20:51:42

ON - MC

IF 1(LL)

1.0

0.8

0.6 IF 2(LL)

30 10 -10 ON - MC

IF 1(RR)

860 820 780 740 IF 2(RR)

5 -5 WB - MC

IF 1(LL)

800

700 IF 2(LL)

4 0 -4 WB - MC

IF 1(RR)

1.02

0.98

0.94

0.90

IF 2(RR)

2 -2 MC - EF

IF 1(LL)

1.02

0.98

0.94

0.90 IF 2(LL)

0 -4 MC - EF

IF 1(RR)

Channels

0 5 10 15

1.0

0.8 IF 2(RR)

0 5 10 15

5 -5 MC - NT

IF 1(LL)

Channels

0 5 10 15

700

500 IF 2(LL)

0 5 10 15

10 -10 MC - NT

IF 1(LL)

Channels

0 5 10 15

900

700

500 IF 2(LL)

0 5 10 15

100 -100

MC - SH

IF 1(RR)

1.00

0.90

0.80

0.70

IF 2(RR)

10 -10

Plot file version 127 created 09-MAR-2004 17:00:48 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/20:54:46 to 00/20:56:12

ON - MC

IF 1(LL)

900

800

700 IF 2(LL)

10 -10 ON - MC

IF 1(RR)

850

750 IF 2(RR)

5 -5 WB - MC

IF 1(LL)

840

800

760 IF 2(LL)

0 -4 -8 WB - MC

IF 1(RR)

1.00

0.96

0.92

0.88

IF 2(RR)

10 -10 MC - EF

IF 1(LL)

960

920

880 IF 2(LL)

10 -10 MC - EF

IF 1(RR)

Channels

0 5 10 15

1.05

0.95

0.85 IF 2(RR)

0 5 10 15

5 -5 MC - NT

IF 1(LL)

Channels

0 5 10 15

800

600 IF 2(LL)

0 5 10 15

5 -5 MC - NT

IF 1(LL)

Channels

0 5 10 15

2.4

2.0

1.6 IF 2(LL) 0 5 10 15

100 -100

MC - UR

IF 1(RR)

1.05

0.95

0.85 IF 2(RR)

0 -20

Plot file version 128 created 09-MAR-2004 17:00:49 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/20:59:16 to 00/21:00:42

ON - MC

IF 1(LL)

0.95

0.85

0.75 IF 2(LL)

10 -10 ON - MC

IF 1(RR)

800

760

720 IF 2(RR)

0 -4 WB - MC

IF 1(LL)

800

760

720 IF 2(LL)

5 -5 WB - MC

IF 1(RR)

960

920

880 IF 2(RR)

4 0 MC - EF

IF 1(LL)

980

940

900 IF 2(LL)

1 -1 MC - EF

IF 1(RR)

Channels

0 5 10 15

1.05

0.95

0.85 IF 2(RR)

0 5 10 15

4 0 -4 MC - NT

IF 1(LL)

Channels

0 5 10 15

800

600 IF 2(LL)

0 5 10 15

0 -4 -8 MC - NT

IF 1(RR)

1.00

0.90

0.80 IF 2(RR)

0 -20

Plot file version 129 created 09-MAR-2004 17:00:50 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/21:03:46 to 00/21:05:12

ON - MC

IF 1(LL)

0.95

0.85 IF 2(LL)

10 -10 ON - MC

IF 1(RR)

900

800 IF 2(RR)

5 -5 WB - MC

IF 1(LL)

820

780

740 IF 2(LL)

0 -4 WB - MC

IF 1(RR)

960

920

880 IF 2(RR)

4 0 -4 MC - EF

IF 1(LL)

1.00

0.96

0.92 IF 2(LL)

2 -2 MC - EF

IF 1(RR)

Channels

0 5 10 15

0.95

0.85

IF 2(RR)

0 5 10 15

0 -5 MC - NT

IF 1(LL)

Channels

0 5 10 15

850

750

650

550 IF 2(LL) 0 5 10 15

0 -10 MC - NT

IF 1(RR)

1.05

0.95

0.85 IF 2(RR)

10 -10

Plot file version 130 created 09-MAR-2004 17:00:51 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/21:09:08 to 00/21:10:18

ON - MC

IF 1(LL)

1.0

0.8 IF 2(LL)

0 -20 ON - MC

IF 1(RR)

880 840 800 760 IF 2(RR)

2 -2 -6 WB - MC

IF 1(LL)

900 860 820 780 IF 2(LL)

5 -5 WB - MC

IF 1(RR)

960

920

880 IF 2(RR)

3 1 -1 MC - EF

IF 1(LL)

0.98

0.94

0.90

IF 2(LL)

2 -2 MC - EF

IF 1(RR)

Channels

0 5 10 15

1.05

0.95

0.85

IF 2(RR)

0 5 10 15

10 -10 MC - NT

IF 1(LL)

Channels

0 5 10 15

700

500 IF 2(LL) 0 5 10 15

10 -10 -30 MC - NT

IF 1(RR)

0.95

0.85

IF 2(RR)

10 -10

Plot file version 131 created 09-MAR-2004 17:00:52 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/21:13:23 to 00/21:14:49

ON - MC

IF 1(LL)

0.95

0.85

0.75 IF 2(LL)

0 -20 ON - MC

IF 1(RR)

880

840

800 IF 2(RR)

4 0 -4 WB - MC

IF 1(LL)

880

840

800 IF 2(LL)

4 0 -4 WB - MC

IF 1(RR)

940

900 IF 2(RR)

1 -1 MC - EF

IF 1(LL)

0.98

0.94

0.90

IF 2(LL)

1 -1 MC - EF

IF 1(RR)

Channels

0 5 10 15

0.95

0.85 IF 2(RR)

0 5 10 15

0 -10 MC - NT

IF 1(LL)

Channels

0 5 10 15

850 750 650 550 IF 2(LL)

0 5 10 15

0 -10 MC - NT

IF 1(RR)

1.05

0.95

0.85

0.75 IF 2(RR)

10 -10

Plot file version 132 created 09-MAR-2004 17:00:53 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/21:18:11 to 00/21:19:19

ON - MC

IF 1(LL)

950

850

750 IF 2(LL)

20 -20 ON - MC

IF 1(RR)

880

840

800 IF 2(RR)

5 -5 WB - MC

IF 1(LL)

900

860

820

780 IF 2(LL)

5 -5 WB - MC

IF 1(RR)

960 940 920 IF 2(RR)

2 -2 MC - EF

IF 1(LL)

960

920 IF 2(LL)

2 -2 MC - EF

IF 1(RR)

Channels

0 5 10 15

1.00

0.90 IF 2(RR)

0 5 10 15

5 -5 -15 MC - NT

IF 1(LL)

Channels

0 5 10 15

850 750 650 550 IF 2(LL) 0 5 10 15

10 -10 MC - NT

IF 1(RR)

1.0

0.8 IF 2(RR)

20 -20

Plot file version 135 created 09-MAR-2004 17:00:56 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/21:32:00 to 00/21:33:26

ON - MC

IF 1(LL)

0.9

0.7 IF 2(LL)

10 -10 ON - MC

IF 1(RR)

860

820

780 IF 2(RR)

5 -5 WB - MC

IF 1(LL)

880

840

800 IF 2(LL)

5 -5 WB - MC

IF 1(RR)

960

920

880 IF 2(RR)

-4 -6 MC - EF

IF 1(LL)

980

940

900 IF 2(LL)

-1 -3 -5 MC - EF

IF 1(RR)

Channels

0 5 10 15

1.00

0.96

0.92

0.88 IF 2(RR)

0 5 10 15

-4 -8 -12 MC - NT

IF 1(LL)

Channels

0 5 10 15

800

600 IF 2(LL)

0 5 10 15

0 -10 MC - NT

IF 1(RR)

1.0

0.8 IF 2(RR)

0 -20

Plot file version 136 created 09-MAR-2004 17:00:58 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/21:36:45 to 00/21:37:55

ON - MC

IF 1(LL)

1.1

0.9

0.7 IF 2(LL)

20 -20 ON - MC

IF 1(RR)

900

800 IF 2(RR)

4 0 -4 WB - MC

IF 1(LL)

880 840 800 760 IF 2(LL)

5 -5 WB - MC

IF 1(RR)

980

940

900 IF 2(RR)

-2 -6 MC - EF

IF 1(LL)

960

920

880 IF 2(LL)

0 -4 MC - EF

IF 1(RR)

Channels

0 5 10 15

1.0

0.8 IF 2(RR)

0 5 10 15

80 40 MC - NT

IF 1(LL)

Channels

0 5 10 15

0.9

0.7

0.5 IF 2(LL) 0 5 10 15

55 45 MC - NT

IF 1(RR)

1.15

1.05

0.95

0.85 IF 2(RR)

0 -20

Plot file version 137 created 09-MAR-2004 17:00:59 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/21:40:59 to 00/21:42:25

ON - MC

IF 1(LL)

1.00

0.90

0.80 IF 2(LL)

10 -10 ON - MC

IF 1(RR)

880 840 800 760 IF 2(RR)

2 -2 -6 WB - MC

IF 1(LL)

860

820

780 IF 2(LL)

2 -2 -6 WB - MC

IF 1(RR)

940

900 IF 2(RR)

4 0 MC - EF

IF 1(LL)

960

920

880 IF 2(LL)

2 0 MC - EF

IF 1(RR)

Channels

0 5 10 15

1.00

0.90 IF 2(RR)

0 5 10 15

4 0 -4 MC - NT

IF 1(LL)

Channels

0 5 10 15

900

700

500 IF 2(LL) 0 5 10 15

10 0 MC - NT

IF 1(RR)

1.20

1.10

1.00

0.90

IF 2(RR)

10 -10

Plot file version 138 created 09-MAR-2004 17:01:00 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/21:45:29 to 00/21:46:55

ON - MC

IF 1(LL)

1.05

0.95

0.85 IF 2(LL)

20 -20 ON - MC

IF 1(RR)

900

800 IF 2(RR)

4 0 WB - MC

IF 1(LL)

860

820

780 IF 2(LL)

6 2 -2 WB - MC

IF 1(RR)

980

940

900 IF 2(RR)

-1 -3 MC - EF

IF 1(LL)

960

920

880 IF 2(LL)

0 -4 MC - EF

IF 1(RR)

Channels

0 5 10 15

900

800 IF 2(RR)

0 5 10 15

4 0 -4 MC - NT

IF 1(LL)

Channels

0 5 10 15

700

500 IF 2(LL)

0 5 10 15

0 -10 MC - NT

IF 1(RR)

1.10

1.00

0.90

0.80 IF 2(RR)

30 10 -10

Plot file version 139 created 09-MAR-2004 17:01:01 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/21:49:59 to 00/21:51:25

ON - MC

IF 1(LL)

1.0

0.8 IF 2(LL)

10 -10 ON - MC

IF 1(RR)

840

800

760 IF 2(RR)

0 -4 WB - MC

IF 1(LL)

880 840 800 760 IF 2(LL)

2 -2 -6 WB - MC

IF 1(RR)

970 950 930 910 IF 2(RR)

4 2 MC - EF

IF 1(LL)

960

920

880 IF 2(LL)

4 0 MC - EF

IF 1(RR)

Channels

0 5 10 15

960

920

880 IF 2(RR) 0 5 10 15

4 0 -4 MC - NT

IF 1(LL)

Channels

0 5 10 15

700

500 IF 2(LL)

0 5 10 15

5 -5 MC - NT

IF 1(RR)

1.1

0.9 IF 2(RR)

10 -10

Plot file version 140 created 09-MAR-2004 17:01:02 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/21:55:19 to 00/21:56:29

ON - MC

IF 1(LL)

1.10

1.00

0.90

0.80

IF 2(LL)

20 -20 ON - MC

IF 1(RR)

950

850

750 IF 2(RR)

5 -5 WB - MC

IF 1(LL)

850

750 IF 2(LL)

4 0 -4 WB - MC

IF 1(RR)

980 960 940 920 IF 2(RR)

0 -2 MC - EF

IF 1(LL)

960

920

880 IF 2(LL)

2 -2 MC - EF

IF 1(RR)

Channels

0 5 10 15

1.05

0.95

0.85 IF 2(RR) 0 5 10 15

5 -5 MC - NT

IF 1(LL)

Channels

0 5 10 15

700

500 IF 2(LL)

0 5 10 15

10 -10 MC - NT

IF 1(RR)

1.1

0.9 IF 2(RR)

0 -20

Plot file version 141 created 09-MAR-2004 17:01:03 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/21:59:33 to 00/22:00:59

ON - MC

IF 1(LL)

1.0

0.8 IF 2(LL)

20 -20 ON - MC

IF 1(RR)

860

820

780 IF 2(RR)

0 -4 WB - MC

IF 1(LL)

860

820

780

740 IF 2(LL)

5 -5 WB - MC

IF 1(RR)

960

920

880 IF 2(RR)

0 -2 MC - EF

IF 1(LL)

960

920

880 IF 2(LL)

0 -4 MC - EF

IF 1(RR)

Channels

0 5 10 15

950

850 IF 2(RR)

0 5 10 15

5 -5 MC - NT

IF 1(LL)

Channels

0 5 10 15

850 750 650 550 IF 2(LL)

0 5 10 15

5 0 MC - NT

IF 1(RR)

1.10

1.00

0.90 IF 2(RR)

10 -10

Plot file version 142 created 09-MAR-2004 17:01:04 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/22:04:03 to 00/22:05:29

ON - MC

IF 1(LL)

1.05

0.95

0.85

IF 2(LL)

20 -20 ON - MC

IF 1(RR)

900 860 820 780 IF 2(RR)

2 -2 -6 WB - MC

IF 1(LL)

840

800

760 IF 2(LL)

5 -5 WB - MC

IF 1(RR)

0.98

0.94

0.90

IF 2(RR)

2 0 MC - EF

IF 1(LL)

960

920

880 IF 2(LL)

3 1 MC - EF

IF 1(RR)

Channels

0 5 10 15

1.05

0.95

0.85 IF 2(RR) 0 5 10 15

5 -5 MC - NT

IF 1(LL)

Channels

0 5 10 15

750

650

550 IF 2(LL)

0 5 10 15

0 -10 MC - NT

IF 1(RR)

1.15

1.05

0.95

0.85 IF 2(RR)

20 -20

Plot file version 143 created 09-MAR-2004 17:01:05 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/22:08:33 to 00/22:09:59

ON - MC

IF 1(LL)

1.00

0.90 IF 2(LL)

20 -20 ON - MC

IF 1(RR)

880

840

800

760 IF 2(RR)

2 -2 WB - MC

IF 1(LL)

880

840

800 IF 2(LL)

5 -5 WB - MC

IF 1(RR)

980

940

900 IF 2(RR)

2 -2 MC - EF

IF 1(LL)

960

920

880 IF 2(LL)

0 -4 MC - EF

IF 1(RR)

Channels

0 5 10 15

0.95

0.85 IF 2(RR) 0 5 10 15

5 -5 MC - NT

IF 1(LL)

Channels

0 5 10 15

700

500 IF 2(LL) 0 5 10 15

5 -5 MC - NT

IF 1(RR)

1.15

1.05

0.95

0.85

IF 2(RR)

0 -40

Plot file version 144 created 09-MAR-2004 17:01:07 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/22:13:03 to 00/22:14:29

ON - MC

IF 1(LL)

1.0

0.8 IF 2(LL)

20 -20 ON - MC

IF 1(RR)

850

750 IF 2(RR)

2 -2 -6 WB - MC

IF 1(LL)

880

840

800

760 IF 2(LL)

2 -2 -6 WB - MC

IF 1(RR)

1.00

0.96

0.92 IF 2(RR)

10 0 MC - EF

IF 1(LL)

960

920

880 IF 2(LL)

0 -2 MC - EF

IF 1(RR)

Channels

0 5 10 15

960 920 880 840 IF 2(RR)

0 5 10 15

4 0 MC - NT

IF 1(LL)

Channels

0 5 10 15

700

500 IF 2(LL)

0 5 10 15

10 0 MC - NT

IF 1(RR)

1.1

0.9 IF 2(RR)

10 -10

Plot file version 145 created 09-MAR-2004 17:01:08 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/22:17:33 to 00/22:18:59

ON - MC

IF 1(LL)

1.05

0.95

0.85 IF 2(LL)

10 -10 ON - MC

IF 1(RR)

920 880 840 800 IF 2(RR)

-5 -15 WB - MC

IF 1(LL)

920

880

840

800 IF 2(LL)

4 0 -4 WB - MC

IF 1(RR)

100

80 IF 2(RR)

300 100 MC - EF

IF 1(LL)

100

80 IF 2(LL)

100 -100

MC - EF

IF 1(RR)

Channels

0 5 10 15

1.00

0.90

0.80

IF 2(RR)

0 5 10 15

5 0 MC - NT

IF 1(LL)

Channels

0 5 10 15

700

500 IF 2(LL)

0 5 10 15

5 -5 MC - NT

IF 1(LL)

Channels

0 5 10 15

2.4

2.0

1.6 IF 2(LL)

0 5 10 15

100 -100

MC - UR

IF 1(LL)

800

600 IF 2(LL)

300 100

Plot file version 146 created 09-MAR-2004 17:01:09 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/22:17:33 to 00/22:18:59

MC - SH

IF 1(RR)

4.2

4.0

3.8

3.6 IF 2(RR)

5 -5

Plot file version 147 created 09-MAR-2004 17:01:09 J0102+58 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/22:22:49 to 00/22:24:29

ON - MC

IF 1(LL)

3.6

3.2 IF 2(LL)

0 -4 -8 ON - MC

IF 1(RR)

4.3

4.1

3.9 IF 2(RR)

2 -2 WB - MC

IF 1(LL)

4.40

4.30

4.20

4.10 IF 2(LL)

0 -4 WB - MC

IF 1(RR)

4.4

4.2 IF 2(RR)

1 -1 MC - EF

IF 1(LL)

4.4

4.2 IF 2(LL)

1.5 0.5 MC - EF

IF 1(RR)

Channels

0 5 10 15

4.2

4.0 IF 2(RR)

0 5 10 15

0 -2 MC - NT

IF 1(LL)

Channels

0 5 10 15

3.6 3.2 2.8 2.4 IF 2(LL)

0 5 10 15

2 -2 MC - NT

IF 1(LL)

Channels

0 5 10 15

4.2

3.8 IF 2(LL)

0 5 10 15

5 0 MC - UR

IF 1(LL)

800

600 IF 2(LL)

200 0

Plot file version 150 created 09-MAR-2004 17:01:11 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/22:28:09 to 00/22:29:23

MC - SH

IF 1(RR)

1.10

1.00

0.90 IF 2(RR)

20 -20

Plot file version 151 created 09-MAR-2004 17:01:12 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/22:32:27 to 00/22:33:53

ON - MC

IF 1(LL)

1.2

1.0

0.8 IF 2(LL)

20 -20 ON - MC

IF 1(RR)

900

860

820

780 IF 2(RR)

6 2 -2 WB - MC

IF 1(LL)

880 840 800 760 IF 2(LL)

4 0 -4 WB - MC

IF 1(RR)

0.98

0.94

0.90

IF 2(RR)

2 0 MC - EF

IF 1(LL)

960

920

880 IF 2(LL)

4 0 -4 MC - EF

IF 1(RR)

Channels

0 5 10 15

0.95

0.85 IF 2(RR)

0 5 10 15

6 2 -2 MC - NT

IF 1(LL)

Channels

0 5 10 15

850 750 650 550 IF 2(LL)

0 5 10 15

5 -5 MC - NT

IF 1(LL)

Channels

0 5 10 15

2.2

1.8 IF 2(LL)

0 5 10 15

200 0 MC - UR

IF 1(LL)

900 800 700 600 IF 2(LL)

100 -100

Plot file version 152 created 09-MAR-2004 17:01:13 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/22:32:27 to 00/22:33:53

MC - SH

IF 1(RR)

4.3 4.1 3.9 3.7 IF 2(RR)

2 -2

Plot file version 153 created 09-MAR-2004 17:01:13 J0102+58 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/22:38:42 to 00/22:40:18

ON - MC

IF 1(LL)

3.7

3.5 IF 2(LL)

0 -4 ON - MC

IF 1(RR)

4.2

4.0 IF 2(RR)

0 -4 WB - MC

IF 1(LL)

4.4

4.2

4.0 IF 2(LL)

0 -4 WB - MC

IF 1(RR)

4.2

4.0 IF 2(RR)

0 -2 MC - NT

IF 1(LL)

3.6 3.2 2.8 2.4 IF 2(LL)

2 -2 MC - NT

IF 1(LL)

Channels

0 5 10 15

4.6

4.2

3.8 IF 2(LL)

0 5 10 15

5 -5 MC - UR

IF 1(LL)

Channels

0 5 10 15

3.1

2.9 IF 2(LL)

0 5 10 15

0 -4 MC - SH

IF 1(RR)

340

300

260

220 IF 2(RR)

20 -20 -60

Plot file version 154 created 09-MAR-2004 17:01:14 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/22:40:22 to 00/22:41:48

WB - MC

IF 1(LL)

300

260 IF 2(LL)

0 -40 WB - MC

IF 1(RR)

1.10

1.00

0.90

0.80 IF 2(RR)

-40 -80 MC - NT

IF 1(LL)

800

600

400 IF 2(LL)

-45 -55 -65 MC - NT

IF 1(RR)

1.20

1.10

1.00

0.90 IF 2(RR)

20 -20

Plot file version 155 created 09-MAR-2004 17:01:15 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/22:44:52 to 00/22:46:18

ON - MC

IF 1(LL)

1.0

0.8 IF 2(LL)

40 0 -40 ON - MC

IF 1(RR)

850

750 IF 2(RR)

-2 -6 WB - MC

IF 1(LL)

860

820

780 IF 2(LL)

0 -4 -8 WB - MC

IF 1(RR)

950

850 IF 2(RR)

5 -5 MC - NT

IF 1(LL)

800

700

600

500 IF 2(LL)

0 -10 MC - NT

IF 1(RR)

1.7 1.5 1.3 1.1 IF 2(RR)

40 0 -40

Plot file version 156 created 09-MAR-2004 17:01:16 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/22:49:22 to 00/22:50:48

ON - MC

IF 1(LL)

1.15

1.05

0.95 IF 2(LL)

20 -20 ON - MC

IF 1(RR)

860

820

780

740 IF 2(RR)

4 0 -4 WB - MC

IF 1(LL)

840

800

760 IF 2(LL)

2 -2 -6 WB - MC

IF 1(RR)

1.00

0.96

0.92

IF 2(RR)

3 1 -1 MC - EF

IF 1(LL)

960

920

880 IF 2(LL)

2 -2 MC - EF

IF 1(RR)

Channels

0 5 10 15

940 900 860 820 IF 2(RR)

0 5 10 15

5 -5 MC - NT

IF 1(LL)

Channels

0 5 10 15

700

500 IF 2(LL)

0 5 10 15

5 -5 MC - NT

IF 1(RR)

1.5

1.3

1.1 IF 2(RR)

-50 -150

Plot file version 157 created 09-MAR-2004 17:01:18 J0244+62 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/22:52:22 to 00/22:53:18

ON - MC

IF 1(LL)

1.1

0.9 IF 2(LL)

40 0 -40 ON - MC

IF 1(RR)

900

800 IF 2(RR)

4 0 -4 WB - MC

IF 1(LL)

900 860 820 780 IF 2(LL)

5 -5 WB - MC

IF 1(RR)

0.98

0.94 IF 2(RR)

0 -4 MC - EF

IF 1(LL)

0.98

0.94

0.90 IF 2(LL)

2 -2 MC - EF

IF 1(RR)

Channels

0 5 10 15

1.00

0.90

0.80 IF 2(RR)

0 5 10 15

5 -5 MC - NT

IF 1(LL)

Channels

0 5 10 15

700

500 IF 2(LL)

0 5 10 15

5 -5 MC - NT

IF 1(RR)

1.8

1.4 IF 2(RR)

100 -100

Plot file version 158 created 09-MAR-2004 17:01:20 J1126+45 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/23:00:50 to 00/23:02:00

ON - MC

IF 1(LL)

1.3

1.1

0.9 IF 2(LL)

300 200 ON - MC

IF 1(RR)

1.2

1.0

0.8 IF 2(RR)

100 -100

MC - NT

IF 1(LL)

1.0

0.8

0.6 IF 2(LL)

100 -100

MC - NT

IF 1(RR)

400

200

0 IF 2(RR)

100 -100

Plot file version 159 created 09-MAR-2004 17:01:42 J1146+39 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/23:07:44 to 00/23:10:24

MC - EF

IF 1(RR)

380 340 300 260 IF 2(RR)

10 -10 -30

Plot file version 160 created 09-MAR-2004 17:01:56 J1126+45 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/23:11:39 to 00/23:12:49

MC - EF

IF 1(RR)

900 800 700 600 IF 2(RR)

50 -50 MC - NT

IF 1(RR)

340

300

260 IF 2(RR)

20 -20

Plot file version 161 created 09-MAR-2004 17:02:04 J1126+45 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/23:15:53 to 00/23:17:19

MC - EF

IF 1(RR)

700

600 IF 2(RR)

20 -20 MC - NT

IF 1(RR)

380 340 300 260 IF 2(RR)

-50 -150

Plot file version 162 created 09-MAR-2004 17:02:13 J1126+45 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/23:20:23 to 00/23:21:49

MC - EF

IF 1(RR)

700

500 IF 2(RR)

50 0 MC - NT

IF 1(RR)

360

320

280 IF 2(RR)

10 -10

Plot file version 165 created 09-MAR-2004 17:02:45 J1126+45 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/23:30:29 to 00/23:31:39

MC - EF

IF 1(LL)

360

320

280 IF 2(LL)

0 -20 MC - EF

IF 1(RR)

650

550 IF 2(RR)

20 -20 MC - NT

IF 1(LL)

650

550

450 IF 2(LL)

20 -20 MC - NT

IF 1(RR)

340

300

260 IF 2(RR)

20 0

Plot file version 166 created 09-MAR-2004 17:02:55 J1126+45 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/23:34:43 to 00/23:36:09

MC - EF

IF 1(LL)

400

300

200 IF 2(LL)

100 0 MC - EF

IF 1(RR)

750

650

550 IF 2(RR)

20 -20 MC - NT

IF 1(LL)

650

550

450 IF 2(LL)

0 -100

MC - NT

IF 1(RR)

400 360 320 280 IF 2(RR)

10 -10

Plot file version 167 created 09-MAR-2004 17:03:03 J1126+45 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/23:39:13 to 00/23:40:39

MC - EF

IF 1(RR)

750

650

550 IF 2(RR)

20 -20 MC - NT

IF 1(RR)

400

300 IF 2(RR)

15 5 -5

Plot file version 168 created 09-MAR-2004 17:03:11 J1126+45 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/23:43:43 to 00/23:45:09

MC - EF

IF 1(RR)

750

650

550 IF 2(RR)

20 -20 MC - NT

IF 1(LL)

1.5 1.3 1.1 0.9 IF 2(LL)

100 -100

Plot file version 169 created 09-MAR-2004 17:03:17 J1146+39 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/23:46:23 to 00/23:49:03

ON - MC

IF 1(RR)

420

380 IF 2(RR)

10 -10 MC - EF

IF 1(LL)

480

440

400

360 IF 2(LL)

10 -10 -30 MC - EF

IF 1(RR)

1.4

1.2

1.0 IF 2(RR)

100 -100

MC - NT

IF 1(LL)

1.2

1.0

0.8 IF 2(LL)

100 -100

MC - NT

IF 1(LL)

1.1

0.9

0.7 IF 2(LL)

40 0 -40

Plot file version 170 created 09-MAR-2004 17:03:29 J1126+45 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/23:50:19 to 00/23:51:29

ON - MC

IF 1(RR)

320

280 IF 2(RR)

10 -10 MC - EF

IF 1(LL)

340

300

260 IF 2(LL)

20 -20 MC - EF

IF 1(RR)

750 650 550 450 IF 2(RR)

10 -10 MC - NT

IF 1(LL)

550

450 IF 2(LL)

50 -50 MC - NT

IF 1(LL)

0.9

0.7 IF 2(LL)

100 -100

Plot file version 171 created 09-MAR-2004 17:03:36 J1126+45 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/23:54:33 to 00/23:55:59

ON - MC

IF 1(RR)

340

300

260 IF 2(RR)

20 -20 MC - EF

IF 1(LL)

400

300 IF 2(LL)

150 50 -50 MC - EF

IF 1(RR)

700

600

500 IF 2(RR)

20 -20 MC - NT

IF 1(LL)

600

400 IF 2(LL)

50 -50 MC - NT

IF 1(RR)

380

340

300 IF 2(RR)

10 -10

Plot file version 172 created 09-MAR-2004 17:03:44 J1126+45 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/23:59:03 to 01/00:00:29

MC - EF

IF 1(LL)

350 330 310 290 IF 2(LL)

10 -10 MC - EF

IF 1(RR)

650

550 IF 2(RR)

20 -20 MC - NT

IF 1(RR)

340

300 IF 2(RR)

0 -10

Plot file version 173 created 09-MAR-2004 17:03:51 J1126+45 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 01/00:03:33 to 01/00:04:59

MC - EF

IF 1(LL)

360

320

280 IF 2(LL)

5 -5 MC - EF

IF 1(RR)

600

500 IF 2(RR)

20 -20 MC - NT

IF 1(RR)

380

340

300

260 IF 2(RR)

20 0

Plot file version 174 created 09-MAR-2004 17:03:57 J1126+45 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 01/00:08:03 to 01/00:09:29

MC - EF

IF 1(LL)

360

320

280 IF 2(LL)

140 100 MC - EF

IF 1(RR)

750

650

550 IF 2(RR)

10 -10 MC - NT

IF 1(LL)

600

500

400 IF 2(LL)

60 20 -20 MC - NT

IF 1(LL)

1.00

0.90

0.80

0.70 IF 2(LL)

100 -100

MC - SH

IF 1(RR)

460

420

380 IF 2(RR)

5 -5 -15

Plot file version 175 created 09-MAR-2004 17:04:05 J1146+39 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 01/00:10:43 to 01/00:13:53

MC - EF

IF 1(LL)

460

420

380 IF 2(LL)

0 -10 MC - EF

IF 1(RR)

950

850 IF 2(RR)

0 -10 MC - NT

IF 1(LL)

800

700

600 IF 2(LL)

5 -5 -15 MC - NT

IF 1(LL)

1.10

1.00

0.90

IF 2(LL)

10 -10 MC - SH

IF 1(RR)

350

250 IF 2(RR)

20 0

Plot file version 176 created 09-MAR-2004 17:04:14 J1126+45 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 01/00:15:25 to 01/00:16:21

MC - EF

IF 1(LL)

360

320

280 IF 2(LL)

15 5 -5 MC - EF

IF 1(RR)

600

500 IF 2(RR)

20 -20 MC - NT

IF 1(LL)

600

500

400 IF 2(LL)

50 -50 MC - NT

IF 1(RR)

360

320

280 IF 2(RR)

15 5 -5

Plot file version 177 created 09-MAR-2004 17:04:19 J1126+45 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 01/00:19:25 to 01/00:20:51

MC - EF

IF 1(LL)

380

340

300 IF 2(LL)

-120

-160

MC - EF

IF 1(RR)

650

550

450 IF 2(RR)

10 -10 MC - NT

IF 1(LL)

500

400 IF 2(LL)

100 60 20 MC - NT

IF 1(LL)

0.95

0.85

0.75 IF 2(LL)

100 -100

MC - SH

IF 1(RR)

380

340

300 IF 2(RR)

15 5 -5

Plot file version 180 created 09-MAR-2004 17:04:38 J1126+45 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 01/00:30:16 to 01/00:31:42

MC - EF

IF 1(LL)

450

350

250 IF 2(LL)

80 40 MC - EF

IF 1(RR)

550

450 IF 2(RR)

40 0 MC - NT

IF 1(LL)

550

450 350 IF 2(LL)

120 80 40 MC - NT

IF 1(RR)

360

320

280 IF 2(RR)

-10 -30

Plot file version 181 created 09-MAR-2004 17:04:43 J1126+45 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 01/00:34:46 to 01/00:36:12

MC - EF

IF 1(LL)

380

340

300 IF 2(LL)

-80 -100 MC - EF

IF 1(RR)

550

450 IF 2(RR)

0 -40 MC - NT

IF 1(LL)

500

400 IF 2(LL)

60 20 -20 MC - NT

IF 1(LL)

950 850 750 650 IF 2(LL)

200 0 MC - SH

IF 1(RR)

520

480

440 IF 2(RR)

5 -5

Plot file version 182 created 09-MAR-2004 17:04:49 J1146+39 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 01/00:37:25 to 01/00:40:07

MC - EF

IF 1(LL)

500

460

420 IF 2(LL)

5 -5 MC - EF

IF 1(RR)

950

850

750 IF 2(RR)

5 -5 MC - NT

IF 1(LL)

750

650

550 IF 2(LL)

5 -5 MC - NT

IF 1(LL)

1.10

1.00

0.90 IF 2(LL)

20 -20 MC - SH

IF 1(RR)

340

300 IF 2(RR)

15 5

Plot file version 183 created 09-MAR-2004 17:04:55 J1126+45 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 01/00:41:24 to 01/00:42:34

MC - EF

IF 1(LL)

380

340

300 IF 2(LL)

15 5 MC - EF

IF 1(RR)

600

500 IF 2(RR)

30 10 -10 MC - NT

IF 1(LL)

500

400 IF 2(LL)

20 -20 MC - NT

IF 1(LL)

0.9

0.7 IF 2(LL)

200 0 MC - SH

IF 1(RR)

360

320

280 IF 2(RR)

0 -10

Plot file version 184 created 09-MAR-2004 17:04:59 J1126+45 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 01/00:45:38 to 01/00:47:04

MC - EF

IF 1(LL)

350

250 IF 2(LL)

120 80 40 MC - EF

IF 1(RR)

600 560 520 480 IF 2(RR)

30 10 -10 MC - NT

IF 1(LL)

550

450

350 IF 2(LL)

0 -100

MC - NT

IF 1(RR)

380

340

300 IF 2(RR)

5 -5

Plot file version 185 created 09-MAR-2004 17:05:02 J1126+45 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 01/00:50:08 to 01/00:51:34

MC - EF

IF 1(LL)

360

340

320 IF 2(LL)

0 -4 -8 MC - EF

IF 1(RR)

650

550

450 IF 2(RR)

0 -20 MC - NT

IF 1(LL)

540 500 460 420 IF 2(LL)

5 -5 MC - NT

IF 1(RR)

340

300 IF 2(RR)

0 -10

Plot file version 186 created 09-MAR-2004 17:05:06 J1126+45 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 01/00:54:38 to 01/00:56:04

MC - EF

IF 1(LL)

350

250 IF 2(LL)

-40 -60 MC - EF

IF 1(RR)

550

450 IF 2(RR)

10 -10 MC - NT

IF 1(LL)

600

500

400 IF 2(LL)

100 60 MC - NT

IF 1(RR)

340

300 IF 2(RR)

25 15

Plot file version 187 created 09-MAR-2004 17:05:10 J1126+45 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 01/00:59:08 to 01/01:00:34

MC - EF

IF 1(LL)

380

340

300 IF 2(LL)

80 60 MC - EF

IF 1(RR)

550

450 IF 2(RR)

20 0 MC - NT

IF 1(LL)

500

400 IF 2(LL)

200 100 MC - NT

IF 1(LL)

0.9

0.7 IF 2(LL)

100 -100

MC - SH

IF 1(RR)

540

500 IF 2(RR)

2 -2 -6

Plot file version 188 created 09-MAR-2004 17:05:13 J1146+39 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 01/01:01:49 to 01/01:03:29

MC - EF

IF 1(LL)

580

540

500 IF 2(LL)

5 -5 MC - EF

IF 1(RR)

800

700 IF 2(RR)

10 -10 MC - NT

IF 1(LL)

750 650 550 450 IF 2(LL)

30 10 -10 MC - NT

IF 1(LL)

1.00

0.90

0.80

IF 2(LL)

20 -20 MC - SH

IF 1(RR)

340

300 IF 2(RR)

10 0

Plot file version 189 created 09-MAR-2004 17:05:16 J1126+45 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 01/01:04:45 to 01/01:05:55

MC - EF

IF 1(LL)

400

360

320 IF 2(LL)

5 -5 MC - EF

IF 1(RR)

700

600

500

400 IF 2(RR)

50 30 MC - NT

IF 1(LL)

1.0

0.8

0.6 IF 2(LL)

200 0 MC - SH

IF 1(RR)

340

300 IF 2(RR)

2 -2 -6

Plot file version 190 created 09-MAR-2004 17:05:19 J1126+45 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 01/01:08:59 to 01/01:10:25

MC - EF

IF 1(LL)

450

350

250 IF 2(LL)

-50 -70 -90 MC - EF

IF 1(RR)

550

450 IF 2(RR)

10 -10 MC - NT

IF 1(RR)

600

560

520 IF 2(RR)

2 -2

Plot file version 191 created 09-MAR-2004 17:05:22 J1146+39 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 01/01:10:29 to 01/01:13:25

MC - EF

IF 1(LL)

620 580 540 500 IF 2(LL)

2 -2 -6 MC - EF

IF 1(RR)

850

750 IF 2(RR)

5 -5 MC - NT

IF 1(LL)

700

600

500 IF 2(LL)

0 -10 MC - NT

IF 1(LL)

3.0

2.6

2.2 IF 2(LL)

100 -100

MC - UR

IF 1(LL)

0.95

0.85 IF 2(LL)

10 -10 MC - SH

IF 1(RR)

360

340

320 IF 2(RR)

2 -2

Plot file version 192 created 09-MAR-2004 17:05:26 J1126+45 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 01/01:13:29 to 01/01:16:55

MC - EF

IF 1(LL)

350

330

310 IF 2(LL)

0 -4 MC - EF

IF 1(RR)

580 540 500 460 IF 2(RR)

10 -10 MC - NT

IF 1(LL)

500

400 IF 2(LL)

20 0 MC - NT

IF 1(RR)

380

360

340

320 IF 2(RR)

0 -4 -8

Plot file version 195 created 09-MAR-2004 17:05:33 J1126+45 eh015a.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH Calibrated with CL # 3 and BP # 1 (BP mode 1)

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 01/01:28:59 to 01/01:30:25

MC - EF

IF 1(LL)

370

350

330 IF 2(LL)

5 -5 MC - EF

IF 1(RR)

540 500 460 IF 2(RR)

20 -20 MC - NT