IF 1(RR)

2.8

2.4

2.0

1.6 IF 2(RR)

200 -200

Plot file version 1 created 02-JUL-2004 12:44:09 0234+285 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/09:00:12 to 00/09:09:58

JV - MC

IF 1(LL)

9

7

5 IF 2(LL)

200 -200 JV - MC

IF 1(RR)

22

18

14 IF 2(RR)

200 -200 JB - MC

IF 1(LL)

18

14

10 IF 2(LL)

200 -200 JB - MC

IF 1(RR)

4.5

3.5

2.5 IF 2(RR)

200 -200 ON - MC

IF 1(LL)

4.5

3.5

2.5 IF 2(LL)

200 -200 ON - MC

IF 1(RR)

Channels

0 5 10 15

11.0

10.0 9.0 8.0 IF 2(RR)

0 5 10 15

200 -200 MC - NT

IF 1(LL)

Channels

0 5 10 15

9

7 IF 2(LL)

0 5 10 15

200 -200 MC - NT

IF 1(RR)

2.0

1.6

1.2 IF 2(RR)

200 -200

Plot file version 2 created 02-JUL-2004 12:44:10 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed

Timerange: 00/09:20:14 to 00/09:21:58

JV - MC

IF 1(LL)

2.5

1.5 IF 2(LL)

200 -200 JV - MC

IF 1(RR)

5.0

4.0

3.0 IF 2(RR)

200 -200 JB - MC

IF 1(LL)

4.5

3.5

2.5 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

1.8

1.4

1.0 IF 2(RR)

200 -200 ON - MC

IF 1(LL)

1.5

1.3

1.1 IF 2(LL)

200 -200 ON - MC

IF 1(RR)

Channels

0 5 10 15

3.0

2.6

2.2 IF 2(RR)

0 5 10 15

200 -200

MC - NT

IF 1(LL)

Channels

0 5 10 15

2.6

2.2

1.8 IF 2(LL)

0 5 10 15

200 -200 MC - NT

IF 1(RR)

2.4 2.0 1.6 1.2 IF 2(RR)

200 -200

Plot file version 3 created 02-JUL-2004 12:44:10 J0122+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed

Timerange: 00/09:22:02 to 00/09:24:58

JV - MC

IF 1(LL)

2.5

1.5 IF 2(LL)

200 -200

JV - MC

IF 1(RR)

7.5

6.5

5.5 4.5 IF 2(RR)

200 -200

JB - MC

IF 1(LL)

5

3 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

1.6

1.2 IF 2(RR)

200 -200

ON - MC

IF 1(LL)

1.6

1.2 IF 2(LL)

200 -200

ON - MC

IF 1(RR)

Channels

0 5 10 15

3.6 3.2 2.8 2.4 IF 2(RR)

0 5 10 15

200 -200

MC - NT

IF 1(LL)

Channels

0 5 10 15

3.0

2.0 IF 2(LL)

0 5 10 15

200 -200

MC - NT

IF 1(RR)

2.0

1.0 IF 2(RR)

200 -200

Plot file version 4 created 02-JUL-2004 12:44:10 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/09:25:02 to 00/09:26:58

JV - MC

IF 1(LL)

2.5

1.5 IF 2(LL)

200 -200

JV - MC

IF 1(RR)

1.8

1.4

1.0 IF 2(RR)

200 -200

JB - MC

IF 1(LL)

1.4

1.2

1.0 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

1.8

1.4

1.0 IF 2(RR)

200 -200

ON - MC

IF 1(LL)

1.7 1.5 1.3 1.1 IF 2(LL)

200 -200

ON - MC

IF 1(RR)

Channels

0 5 10 15

2.8

2.4 IF 2(RR)

0 5 10 15

200 -200

MC - NT

IF 1(LL)

Channels

0 5 10 15

2.8

2.4

2.0 IF 2(LL)

0 5 10 15

200 -200

MC - NT

IF 1(RR)

2.0

1.0 IF 2(RR)

200 -200

Plot file version 5 created 02-JUL-2004 12:44:10 J0122+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/09:27:02 to 00/09:29:58

JV - MC

IF 1(LL)

3.0

2.0 IF 2(LL)

200 -200

JV - MC

IF 1(RR)

7.5 6.5 5.5 4.5 IF 2(RR)

200 -200

JB - MC

IF 1(LL)

5

3 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

1.6

1.2 IF 2(RR)

200 -200

ON - MC

IF 1(LL)

1.6

1.2 IF 2(LL)

200 -200

ON - MC

IF 1(RR)

Channels

0 5 10 15

3.4

3.0 2.6 IF 2(RR)

0 5 10 15

200 -200

MC - NT

IF 1(LL)

Channels

0 5 10 15

3.4 3.0 2.6 2.2 IF 2(LL)

0 5 10 15

200 -200

MC - NT

IF 1(RR)

2.0

1.6

1.2 IF 2(RR)

200 -200

Plot file version 6 created 02-JUL-2004 12:44:10 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed

Timerange: 00/09:30:02 to 00/09:34:57

JV - MC

IF 1(LL)

2.5

1.5 IF 2(LL)

200 -200

JV - MC

IF 1(RR)

5.5

4.5

3.5 IF 2(RR)

200 -200

JB - MC

IF 1(LL)

4.5

3.5

2.5 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

1.6

1.2 IF 2(RR)

200 -200

ON - MC

IF 1(LL)

2.0

1.6

1.2 IF 2(LL)

200 -200

ON - MC

IF 1(RR)

Channels

0 5 10 15

2.8

2.4

2.0 IF 2(RR)

0 5 10 15

200 -200

MC - NT

IF 1(LL)

Channels

0 5 10 15

3.0

2.6

2.2

1.8 IF 2(LL)

0 5 10 15

200 -200

MC - NT

IF 1(RR)

2.4 2.0 1.6 1.2 IF 2(RR)

200 -200

Plot file version 7 created 02-JUL-2004 12:44:10 J0122+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/09:35:01 to 00/09:37:57

JV - MC

IF 1(LL)

2.5

1.5 IF 2(LL)

200 -200

JV - MC

IF 1(RR)

6.5 5.5 4.5 IF 2(RR)

200 -200

JB - MC

IF 1(LL)

6.5 5.5 4.5 3.5 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

13

11

9 IF 2(RR)

200 -200

EF - MC

IF 1(LL)

12

8 IF 2(LL)

200 -200

EF - MC

IF 1(RR)

Channels

0 5 10 15

2.2

1.8

1.4 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

2.0

1.6

1.2 IF 2(LL)

0 5 10 15

200 -200

ON - MC

IF 1(RR)

Channels

0 5 10 15

3.6

3.2

2.8

2.4 IF 2(RR)

0 5 10 15

200 -200

MC - NT

IF 1(LL)

3.0

2.0 IF 2(LL)

200 -200

Plot file version 8 created 02-JUL-2004 12:44:10 J0122+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/09:35:01 to 00/09:37:57

MC - NT

IF 1(RR)

2.0

1.0 IF 2(RR)

200 -200

Plot file version 9 created 02-JUL-2004 12:44:10 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/09:38:01 to 00/09:39:57

JV - MC

IF 1(LL)

2.6 2.2 1.8 1.4 IF 2(LL)

200 -200

JV - MC

IF 1(RR)

1.5

1.3

1.1

0.9 IF 2(RR)

200 -200

JB - MC

IF 1(LL)

1.4

1.2

1.0 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

11

9

7 IF 2(RR)

200 -200

EF - MC

IF 1(LL)

12

10

8

6 IF 2(LL)

200 -200

EF - MC

IF 1(RR)

Channels

0 5 10 15

2.0

1.6

1.2 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

2.0

1.6

1.2 IF 2(LL)

0 5 10 15

200 -200

ON - MC

IF 1(RR)

Channels

0 5 10 15

3.0

2.6

2.2 IF 2(RR)

0 5 10 15

200 -200

MC - NT

IF 1(LL)

2.6

2.2

1.8 IF 2(LL)

200 -200

Plot file version 10 created 02-JUL-2004 12:44:10 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/09:38:01 to 00/09:39:57

MC - NT

IF 1(RR)

2.4 2.0 1.6 1.2 IF 2(RR)

200 -200

Plot file version 11 created 02-JUL-2004 12:44:10 J0122+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/09:40:01 to 00/09:42:57

JV - MC

IF 1(LL)

3.0

2.0 IF 2(LL)

200 -200

JV - MC

IF 1(RR)

7.0

6.0

5.0

4.0 IF 2(RR)

200 -200

JB - MC

IF 1(LL)

6.0 5.0 4.0 3.0 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

15 13 11 9 IF 2(RR)

200 -200

EF - MC

IF 1(LL)

12

8 IF 2(LL)

200 -200

EF - MC

IF 1(RR)

Channels

0 5 10 15

2.2

1.8

1.4 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

2.2

1.8

1.4 IF 2(LL)

0 5 10 15

200 -200

ON - MC

IF 1(RR)

Channels

0 5 10 15

3.6

3.2

2.8 IF 2(RR)

0 5 10 15

200 -200

MC - NT

IF 1(LL)

3.0

2.0 IF 2(LL)

200 -200

Plot file version 12 created 02-JUL-2004 12:44:10 J0122+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/09:40:01 to 00/09:42:57

MC - NT

IF 1(RR)

2.2 1.8 1.4 1.0 IF 2(RR)

200 -200

Plot file version 15 created 02-JUL-2004 12:44:10 J0122+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/09:45:01 to 00/09:47:57

JV - MC

IF 1(LL)

3.0

2.0 IF 2(LL)

200 -200 JV - MC

IF 1(RR)

7.0

6.0

5.0

4.0 IF 2(RR)

200 -200 JB - MC

IF 1(LL)

6.0 5.0 4.0 3.0 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

13 11 9 IF 2(RR)

200 -200 EF - MC

IF 1(LL)

14 12 10 8 IF 2(LL)

200 -200 EF - MC

IF 1(RR)

Channels

0 5 10 15

2.2

1.8

1.4 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

2.0

1.6

1.2 IF 2(LL)

0 5 10 15

200 -200 ON - MC

IF 1(RR)

Channels

0 5 10 15

3.4

3.0

2.6 IF 2(RR)

0 5 10 15

200 -200 MC - NT

IF 1(LL)

3.4 3.0 2.6 2.2 IF 2(LL)

200 -200

Plot file version 16 created 02-JUL-2004 12:44:10 J0122+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/09:45:01 to 00/09:47:57

MC - NT

IF 1(RR)

2.2 1.8 1.4 1.0 IF 2(RR)

200 -200

Plot file version 17 created 02-JUL-2004 12:44:10 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/09:48:01 to 00/09:49:57

JV - MC

IF 1(LL)

2.5

1.5 IF 2(LL)

200 -200 JV - MC

IF 1(RR)

1.6 1.4 1.2 1.0 IF 2(RR)

200 -200 JB - MC

IF 1(LL)

1.4

1.2

1.0 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

11

9

7 IF 2(RR)

200 -200 EF - MC

IF 1(LL)

12 10 8 6 IF 2(LL)

200 -200 EF - MC

IF 1(RR)

Channels

0 5 10 15

1.8

1.4

1.0 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

1.6

1.2 IF 2(LL)

0 5 10 15

200 -200 ON - MC

IF 1(RR)

Channels

0 5 10 15

3.0

2.6

2.2 IF 2(RR)

0 5 10 15

200 -200 MC - NT

IF 1(LL)

2.8

2.4

2.0 IF 2(LL)

200 -200

Plot file version 18 created 02-JUL-2004 12:44:10 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/09:48:01 to 00/09:49:57

MC - NT

IF 1(RR)

1.8

1.4

1.0 IF 2(RR)

200 -200

Plot file version 19 created 02-JUL-2004 12:44:10 J0122+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/09:50:01 to 00/09:52:57

JV - MC

IF 1(LL)

3.0 2.6 2.2 1.8 IF 2(LL)

200 -200

JV - MC

IF 1(RR)

7.0

6.0

5.0

4.0 IF 2(RR)

200 -200 JB - MC

IF 1(LL)

6.0 5.0 4.0 3.0 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

13 11 9 IF 2(RR)

200 -200

EF - MC

IF 1(LL)

12

8 IF 2(LL)

200 -200 EF - MC

IF 1(RR)

Channels

0 5 10 15

2.2

1.8

1.4 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

2.0

1.6

1.2 IF 2(LL)

0 5 10 15

200 -200

ON - MC

IF 1(RR)

Channels

0 5 10 15

3.8

3.4

3.0

2.6 IF 2(RR)

0 5 10 15

200 -200 MC - NT

IF 1(LL)

3.0

2.6

2.2 IF 2(LL)

200 -200

Plot file version 20 created 02-JUL-2004 12:44:10 J0122+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/09:50:01 to 00/09:52:57

MC - NT

IF 1(RR)

2.4 2.0 1.6 1.2 IF 2(RR)

200 -200

Plot file version 21 created 02-JUL-2004 12:44:10 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/09:53:01 to 00/09:57:58

JV - MC

IF 1(LL)

2.5

1.5 IF 2(LL)

200 -200

JV - MC

IF 1(RR)

5.5

4.5

3.5 IF 2(RR)

200 -200

JB - MC

IF 1(LL)

4.5

3.5

2.5 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

11

9

7 IF 2(RR)

200 -200

EF - MC

IF 1(LL)

12 10 8 6 IF 2(LL)

200 -200

EF - MC

IF 1(RR)

Channels

0 5 10 15

1.6

1.2 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

1.6

1.2 IF 2(LL)

0 5 10 15

200 -200

ON - MC

IF 1(RR)

Channels

0 5 10 15

3.0

2.6

2.2 IF 2(RR)

0 5 10 15

200 -200

MC - NT

IF 1(LL)

2.6

2.2

1.8 IF 2(LL)

200 -200

Plot file version 22 created 02-JUL-2004 12:44:11 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/09:53:01 to 00/09:57:58

MC - NT

IF 1(RR)

2.4 2.0 1.6 1.2 IF 2(RR)

200 -200

Plot file version 23 created 02-JUL-2004 12:44:11 J0122+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/09:58:02 to 00/10:00:58

JV - MC

IF 1(LL)

2.8 2.4 2.0 1.6 IF 2(LL)

200 -200

JV - MC

IF 1(RR)

7.0 6.0 5.0 4.0 IF 2(RR)

200 -200

JB - MC

IF 1(LL)

6.5

5.5 4.5 3.5 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

13 11 9 IF 2(RR)

200 -200

EF - MC

IF 1(LL)

12

8 IF 2(LL)

200 -200

EF - MC

IF 1(RR)

Channels

0 5 10 15

2.2

1.8

1.4 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

2.2

1.8

1.4 IF 2(LL)

0 5 10 15

200 -200

ON - MC

IF 1(RR)

Channels

0 5 10 15

3.4

3.0

2.6 IF 2(RR)

0 5 10 15

200 -200

MC - NT

IF 1(LL)

3.0 2.6 2.2 IF 2(LL)

200 -200

Plot file version 24 created 02-JUL-2004 12:44:11 J0122+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/09:58:02 to 00/10:00:58

MC - NT

IF 1(RR)

2.2 1.8 1.4 1.0 IF 2(RR)

200 -200

Plot file version 25 created 02-JUL-2004 12:44:11 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/10:01:02 to 00/10:02:58

JV - MC

IF 1(LL)

2.5

1.5 IF 2(LL)

200 -200

JV - MC

IF 1(RR)

1.4

1.2

1.0 IF 2(RR)

200 -200

JB - MC

IF 1(LL)

1.4

1.0 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

11

9

7 IF 2(RR)

200 -200

EF - MC

IF 1(LL)

12 10 8 6 IF 2(LL)

200 -200

EF - MC

IF 1(RR)

Channels

0 5 10 15

1.8

1.4

1.0 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

1.6

1.2 IF 2(LL)

0 5 10 15

200 -200

ON - MC

IF 1(RR)

Channels

0 5 10 15

3.0

2.6

2.2 IF 2(RR)

0 5 10 15

200 -200

MC - NT

IF 1(LL)

2.8

2.4

2.0 IF 2(LL)

200 -200

Plot file version 26 created 02-JUL-2004 12:44:11 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/10:01:02 to 00/10:02:58

MC - NT

IF 1(RR)

2.2

1.8

1.4

1.0 IF 2(RR)

200 -200

Plot file version 27 created 02-JUL-2004 12:44:11 J0122+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/10:03:02 to 00/10:05:58

JV - MC

IF 1(LL)

3.0

2.0 IF 2(LL)

200 -200

JV - MC

IF 1(RR)

6.5

5.5

4.5 IF 2(RR)

200 -200

JB - MC

IF 1(LL)

5

3 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

13

11

9 IF 2(RR)

200 -200

EF - MC

IF 1(LL)

12

8 IF 2(LL)

200 -200

EF - MC

IF 1(RR)

Channels

0 5 10 15

2.0

1.6

1.2 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

2.0

1.6

1.2 IF 2(LL)

0 5 10 15

200 -200

ON - MC

IF 1(RR)

Channels

0 5 10 15

3.4

3.0

2.6 IF 2(RR)

0 5 10 15

200 -200

MC - NT

IF 1(LL)

2.6

2.2

1.8 IF 2(LL)

200 -200

Plot file version 30 created 02-JUL-2004 12:44:11 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/10:06:02 to 00/10:07:58

MC - NT

IF 1(RR)

2.0

1.0 IF 2(RR)

200 -200

Plot file version 31 created 02-JUL-2004 12:44:11 J0122+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/10:08:02 to 00/10:10:58

JV - MC

IF 1(LL)

2.5

1.5 IF 2(LL)

200 -200 JV - MC

IF 1(RR)

7.0 6.0 5.0 4.0 IF 2(RR)

200 -200 JB - MC

IF 1(LL)

6.5 5.5 4.5 3.5 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

15

13

11

9 IF 2(RR)

200 -200 EF - MC

IF 1(LL)

12

8 IF 2(LL)

200 -200 EF - MC

IF 1(RR)

Channels

0 5 10 15

2.0

1.6

1.2 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

2.0

1.6

1.2 IF 2(LL)

0 5 10 15

200 -200 ON - MC

IF 1(RR)

Channels

0 5 10 15

3.4

3.0

2.6 IF 2(RR)

0 5 10 15

200 -200 MC - NT

IF 1(LL)

3.4 3.0 2.6 2.2 IF 2(LL)

200 -200

Plot file version 32 created 02-JUL-2004 12:44:11 J0122+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/10:08:02 to 00/10:10:58

MC - NT

IF 1(RR)

2.0

1.0 IF 2(RR)

200 -200

Plot file version 33 created 02-JUL-2004 12:44:11 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/10:11:02 to 00/10:12:58

JV - MC

IF 1(LL)

2.6

2.2

1.8

1.4 IF 2(LL)

200 -200 JV - MC

IF 1(RR)

1.4

1.2

1.0 IF 2(RR)

200 -200

JB - MC

IF 1(LL)

1.6 1.4 1.2 1.0 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

11

9

7 IF 2(RR)

200 -200 EF - MC

IF 1(LL)

12

10

8

6 IF 2(LL)

200 -200

EF - MC

IF 1(RR)

Channels

0 5 10 15

2.0

1.6

1.2 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

2.0

1.6

1.2 IF 2(LL)

0 5 10 15

200 -200 ON - MC

IF 1(RR)

2.0

1.6 1.2 IF 2(RR)

200 -200

Plot file version 34 created 02-JUL-2004 12:44:11 J0122+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/10:13:02 to 00/10:15:58

JV - MC

IF 1(LL)

2.5

1.5 IF 2(LL)

200 -200

JV - MC

IF 1(RR)

6.0

5.0

4.0 IF 2(RR)

200 -200 JB - MC

IF 1(LL)

6.0 5.0 4.0 3.0 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

13 11 9 IF 2(RR)

200 -200

EF - MC

IF 1(LL)

12

8 IF 2(LL)

200 -200 EF - MC

IF 1(RR)

Channels

0 5 10 15

2.0

1.6

1.2 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

2.0

1.6

1.2 IF 2(LL)

0 5 10 15

200 -200

ON - MC

IF 1(RR)

2.0

1.6

1.2 IF 2(RR)

200 -200

Plot file version 35 created 02-JUL-2004 12:44:11 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/10:16:02 to 00/10:20:58

JV - MC

IF 1(LL)

2.6

2.2

1.8

1.4 IF 2(LL)

200 -200

JV - MC

IF 1(RR)

5.5

4.5

3.5 IF 2(RR)

200 -200

JB - MC

IF 1(LL)

4.5

3.5

2.5 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

11

9

7 IF 2(RR)

200 -200

EF - MC

IF 1(LL)

10

8

6 IF 2(LL)

200 -200

EF - MC

IF 1(RR)

Channels

0 5 10 15

1.8 1.6 1.4 1.2 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

1.6

1.2 IF 2(LL)

0 5 10 15

200 -200

ON - MC

IF 1(RR)

Channels

0 5 10 15

2.8

2.4 IF 2(RR)

0 5 10 15

200 -200

MC - NT

IF 1(LL)

2.8

2.4

2.0 IF 2(LL)

200 -200

Plot file version 36 created 02-JUL-2004 12:44:11 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/10:16:02 to 00/10:20:58

MC - NT

IF 1(RR)

2.0

1.6

1.2 IF 2(RR)

200 -200

Plot file version 37 created 02-JUL-2004 12:44:11 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/10:24:02 to 00/10:25:58

JV - MC

IF 1(LL)

2.5

1.5 IF 2(LL)

200 -200

JV - MC

IF 1(RR)

1.5

1.3

1.1 IF 2(RR)

200 -200

JB - MC

IF 1(LL)

1.4

1.2

1.0 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

11

9

7 IF 2(RR)

200 -200

EF - MC

IF 1(LL)

12

10

8

6 IF 2(LL)

200 -200

EF - MC

IF 1(RR)

Channels

0 5 10 15

1.6

1.2 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

1.6

1.2 IF 2(LL)

0 5 10 15

200 -200

ON - MC

IF 1(RR)

Channels

0 5 10 15

2.8

2.4

2.0 IF 2(RR)

0 5 10 15

200 -200

MC - NT

IF 1(LL)

2.6

2.2

1.8 IF 2(LL)

200 -200

Plot file version 38 created 02-JUL-2004 12:44:11 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/10:24:02 to 00/10:25:58

MC - NT

IF 1(RR)

2.0

1.0 IF 2(RR)

200 -200

Plot file version 39 created 02-JUL-2004 12:44:11 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed

Timerange: 00/10:29:02 to 00/10:30:58

JV - MC

IF 1(LL)

3.5

2.5

1.5 IF 2(LL)

200 -200

JV - MC

IF 1(RR)

5.5

4.5

3.5 IF 2(RR)

200 -200

JB - MC

IF 1(LL)

4.5

3.5

2.5 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

11

9

7 IF 2(RR)

200 -200

EF - MC

IF 1(LL)

10

8

6 IF 2(LL)

200 -200

EF - MC

IF 1(RR)

Channels

0 5 10 15

1.8

1.4 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

2.0

1.6

1.2 IF 2(LL)

0 5 10 15

200 -200

ON - MC

IF 1(RR)

Channels

0 5 10 15

3.0

2.6

2.2 IF 2(RR)

0 5 10 15

200 -200

MC - NT

IF 1(LL)

3.0 2.6 2.2 1.8 IF 2(LL)

200 -200

Plot file version 40 created 02-JUL-2004 12:44:11 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/10:29:02 to 00/10:30:58

MC - NT

IF 1(RR)

2.0

1.0 IF 2(RR)

200 -200

Plot file version 41 created 02-JUL-2004 12:44:11 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/10:34:02 to 00/10:35:58

JV - MC

IF 1(LL)

2.5

1.5 IF 2(LL)

200 -200

JV - MC

IF 1(RR)

1.5

1.3

1.1 IF 2(RR)

200 -200

JB - MC

IF 1(LL)

1.4

1.0 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

11

9

7 IF 2(RR)

200 -200

EF - MC

IF 1(LL)

12

10

8

6 IF 2(LL)

200 -200

EF - MC

IF 1(RR)

Channels

0 5 10 15

2.0

1.6

1.2 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

2.0

1.6

1.2 IF 2(LL)

0 5 10 15

200 -200

ON - MC

IF 1(RR)

Channels

0 5 10 15

2.8

2.4 IF 2(RR)

0 5 10 15

200 -200

MC - NT

IF 1(LL)

3.0

2.6

2.2 IF 2(LL)

200 -200

Plot file version 42 created 02-JUL-2004 12:44:11 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/10:34:02 to 00/10:35:58

MC - NT

IF 1(RR)

2.4 2.0 1.6 1.2 IF 2(RR)

200 -200

Plot file version 45 created 02-JUL-2004 12:44:11 J0122+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/10:44:02 to 00/10:46:58

JV - MC

IF 1(LL)

3.0

2.0 IF 2(LL)

200 -200 JV - MC

IF 1(RR)

7.0 6.0 5.0 4.0 IF 2(RR)

200 -200 JB - MC

IF 1(LL)

5

3 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

15 13 11 9 IF 2(RR)

200 -200 EF - MC

IF 1(LL)

12

8 IF 2(LL)

200 -200 EF - MC

IF 1(RR)

Channels

0 5 10 15

2.4

2.0

1.6 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

2.4

2.0

1.6 IF 2(LL)

0 5 10 15

200 -200 ON - MC

IF 1(RR)

Channels

0 5 10 15

3.6

3.2

2.8 IF 2(RR)

0 5 10 15

200 -200 MC - NT

IF 1(LL)

3.0

2.0 IF 2(LL)

200 -200

Plot file version 46 created 02-JUL-2004 12:44:12 J0122+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/10:44:02 to 00/10:46:58

MC - NT

IF 1(RR)

2.0

1.0 IF 2(RR)

200 -200

Plot file version 47 created 02-JUL-2004 12:44:12 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed

Timerange: 00/10:47:02 to 00/10:48:58

JV - MC

IF 1(LL)

2.5

1.5 IF 2(LL)

200 -200 JV - MC

IF 1(RR)

1.4

1.2

1.0 IF 2(RR)

200 -200 JB - MC

IF 1(LL)

1.4

1.2

1.0 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

11

9

7 IF 2(RR)

200 -200 EF - MC

IF 1(LL)

10

8

6 IF 2(LL)

200 -200 EF - MC

IF 1(RR)

Channels

0 5 10 15

2.0

1.6

1.2 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

2.2

1.8

1.4 IF 2(LL)

0 5 10 15

200 -200 ON - MC

IF 1(RR)

Channels

0 5 10 15

2.8

2.4

2.0 IF 2(RR)

0 5 10 15

200 -200 MC - NT

IF 1(LL)

2.8

2.4

2.0 IF 2(LL)

200 -200

Plot file version 48 created 02-JUL-2004 12:44:12 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/10:47:02 to 00/10:48:58

MC - NT

IF 1(RR)

2.4 2.0 1.6 1.2 IF 2(RR)

200 -200

Plot file version 49 created 02-JUL-2004 12:44:12 J0122+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed

Timerange: 00/10:49:02 to 00/10:51:58

JV - MC

IF 1(LL)

2.5

1.5 IF 2(LL)

200 -200

JV - MC

IF 1(RR)

7.0

6.0

5.0

4.0 IF 2(RR)

200 -200

JB - MC

IF 1(LL)

5

3 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

15 13 11 9 IF 2(RR)

200 -200

EF - MC

IF 1(LL)

12

8 IF 2(LL)

200 -200

EF - MC

IF 1(RR)

Channels

0 5 10 15

2.6 2.2 1.8 1.4 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

2.2

1.8

1.4 IF 2(LL)

0 5 10 15

200 -200

ON - MC

IF 1(RR)

Channels

0 5 10 15

3.4

3.0

2.6 IF 2(RR)

0 5 10 15

200 -200

MC - NT

IF 1(LL)

3.4 3.0 2.6 2.2 IF 2(LL)

200 -200

Plot file version 50 created 02-JUL-2004 12:44:12 J0122+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/10:49:02 to 00/10:51:58

MC - NT

IF 1(RR)

2.0

1.6

1.2 IF 2(RR)

200 -200

Plot file version 51 created 02-JUL-2004 12:44:12 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/10:52:02 to 00/10:53:58

JV - MC

IF 1(LL)

2.5

1.5 IF 2(LL)

200 -200

JV - MC

IF 1(RR)

5.5

4.5

3.5 IF 2(RR)

200 -200

JB - MC

IF 1(LL)

4.5

3.5

2.5 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

11

9

7 IF 2(RR)

200 -200

EF - MC

IF 1(LL)

12

10

8

6 IF 2(LL)

200 -200

EF - MC

IF 1(RR)

Channels

0 5 10 15

2.2

1.8

1.4 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

2.2 1.8 1.4 1.0 IF 2(LL)

0 5 10 15

200 -200

ON - MC

IF 1(RR)

Channels

0 5 10 15

3.0

2.6

2.2 IF 2(RR)

0 5 10 15

200 -200

MC - NT

IF 1(LL)

2.6

2.2

1.8 IF 2(LL)

200 -200

Plot file version 52 created 02-JUL-2004 12:44:12 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/10:52:02 to 00/10:53:58

MC - NT

IF 1(RR)

2.0

1.6

1.2 IF 2(RR)

200 -200

Plot file version 53 created 02-JUL-2004 12:44:12 J0122+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed

Timerange: 00/10:54:02 to 00/10:56:58

JV - MC

IF 1(LL)

2.5

1.5 IF 2(LL)

200 -200

JV - MC

IF 1(RR)

7.0 6.0 5.0 4.0 IF 2(RR)

200 -200

JB - MC

IF 1(LL)

5.5 4.5 3.5 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

15 13 11 9 IF 2(RR)

200 -200

EF - MC

IF 1(LL)

12

8 IF 2(LL)

200 -200

EF - MC

IF 1(RR)

Channels

0 5 10 15

2.4

2.0

1.6 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

2.2

1.8

1.4 IF 2(LL)

0 5 10 15

200 -200

ON - MC

IF 1(RR)

Channels

0 5 10 15

3.4

3.0

2.6 IF 2(RR)

0 5 10 15

200 -200

MC - NT

IF 1(LL)

3.4 3.0 2.6 2.2 IF 2(LL)

200 -200

Plot file version 54 created 02-JUL-2004 12:44:12 J0122+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/10:54:02 to 00/10:56:58

MC - NT

IF 1(RR)

2.0

1.0 IF 2(RR)

200 -200

Plot file version 55 created 02-JUL-2004 12:44:12 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/10:57:02 to 00/10:58:58

JV - MC

IF 1(LL)

2.6

2.2

1.8

1.4 IF 2(LL)

200 -200

JV - MC

IF 1(RR)

1.4

1.0 IF 2(RR)

200 -200

JB - MC

IF 1(LL)

1.6 1.4 1.2 1.0 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

11

9

7 IF 2(RR)

200 -200

EF - MC

IF 1(LL)

12

10

8

6 IF 2(LL)

200 -200

EF - MC

IF 1(RR)

Channels

0 5 10 15

2.0

1.6

1.2 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

1.8

1.4 IF 2(LL)

0 5 10 15

200 -200

ON - MC

IF 1(RR)

Channels

0 5 10 15

3.0

2.6

2.2 IF 2(RR)

0 5 10 15

200 -200

MC - NT

IF 1(LL)

3.0 2.6 2.2 1.8 IF 2(LL)

200 -200

Plot file version 56 created 02-JUL-2004 12:44:12 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/10:57:02 to 00/10:58:58

MC - NT

IF 1(RR)

2.0 1.6 1.2 IF 2(RR)

200 -200

Plot file version 57 created 02-JUL-2004 12:44:12 J0122+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/10:59:02 to 00/11:01:58

JV - MC

IF 1(LL)

3.0

2.0 IF 2(LL)

200 -200

JV - MC

IF 1(RR)

7.0

6.0

5.0

4.0 IF 2(RR)

200 -200

JB - MC

IF 1(LL)

6.0 5.0 4.0 3.0 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

15 13 11 9 IF 2(RR)

200 -200

EF - MC

IF 1(LL)

12

8 IF 2(LL)

200 -200

EF - MC

IF 1(RR)

Channels

0 5 10 15

2.2

1.8

1.4 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

2.2

1.8

1.4 IF 2(LL)

0 5 10 15

200 -200

ON - MC

IF 1(RR)

Channels

0 5 10 15

3.6

3.2

2.8

2.4 IF 2(RR)

0 5 10 15

200 -200

MC - NT

IF 1(LL)

2.8

2.4

2.0 IF 2(LL)

200 -200

Plot file version 60 created 02-JUL-2004 12:44:12 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/11:02:02 to 00/11:06:58

MC - NT

IF 1(RR)

2.0

1.0 IF 2(RR)

200 -200

Plot file version 61 created 02-JUL-2004 12:44:12 J0122+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/11:07:02 to 00/11:09:58

JV - MC

IF 1(LL)

3.0

2.0 IF 2(LL)

200 -200 JV - MC

IF 1(RR)

7.0

6.0

5.0

4.0 IF 2(RR)

200 -200 JB - MC

IF 1(LL)

6.0 5.0 4.0 3.0 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

15 13 11 9 IF 2(RR)

200 -200 EF - MC

IF 1(LL)

12

8 IF 2(LL)

200 -200 EF - MC

IF 1(RR)

Channels

0 5 10 15

2.2

1.8

1.4 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

2.2

1.8

1.4 IF 2(LL)

0 5 10 15

200 -200 ON - MC

IF 1(RR)

Channels

0 5 10 15

3.4

3.0

2.6 IF 2(RR)

0 5 10 15

200 -200 MC - NT

IF 1(LL)

3.4

3.0

2.6

2.2 IF 2(LL)

200 -200

Plot file version 62 created 02-JUL-2004 12:44:12 J0122+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/11:07:02 to 00/11:09:58

MC - NT

IF 1(RR)

1.8

1.4

1.0 IF 2(RR)

200 -200

Plot file version 63 created 02-JUL-2004 12:44:12 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed

Timerange: 00/11:10:02 to 00/11:11:58

JV - MC

IF 1(LL)

2.5

1.5 IF 2(LL)

200 -200

JV - MC

IF 1(RR)

1.4

1.2

1.0 IF 2(RR)

200 -200 JB - MC

IF 1(LL)

1.4

1.2

1.0 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

11

9

7 IF 2(RR)

200 -200

EF - MC

IF 1(LL)

12 10 8 6 IF 2(LL)

200 -200 EF - MC

IF 1(RR)

Channels

0 5 10 15

2.2

1.8

1.4 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

2.2

1.8

1.4 IF 2(LL)

0 5 10 15

200 -200

ON - MC

IF 1(RR)

Channels

0 5 10 15

3.0

2.6

2.2 IF 2(RR)

0 5 10 15

200 -200 MC - NT

IF 1(LL)

2.6

2.2

1.8 IF 2(LL)

200 -200

Plot file version 64 created 02-JUL-2004 12:44:12 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/11:10:02 to 00/11:11:58

MC - NT

IF 1(RR)

2.0

1.6

1.2 IF 2(RR)

200 -200

Plot file version 65 created 02-JUL-2004 12:44:12 J0122+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/11:12:02 to 00/11:14:58

JV - MC

IF 1(LL)

2.5

1.5 IF 2(LL)

200 -200

JV - MC

IF 1(RR)

7.0

6.0

5.0

4.0 IF 2(RR)

200 -200

JB - MC

IF 1(LL)

6.0 5.0 4.0 3.0 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

15 13 11 9 IF 2(RR)

200 -200

EF - MC

IF 1(LL)

12

8 IF 2(LL)

200 -200

EF - MC

IF 1(RR)

Channels

0 5 10 15

2.4

2.0

1.6

1.2 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

2.2

1.8

1.4 IF 2(LL)

0 5 10 15

200 -200

ON - MC

IF 1(RR)

Channels

0 5 10 15

3.6

3.2

2.8 IF 2(RR)

0 5 10 15

200 -200

MC - NT

IF 1(LL)

3.4 3.0 2.6 2.2 IF 2(LL)

200 -200

Plot file version 66 created 02-JUL-2004 12:44:12 J0122+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/11:12:02 to 00/11:14:58

MC - NT

IF 1(RR)

2.0

1.6

1.2 IF 2(RR)

200 -200

Plot file version 67 created 02-JUL-2004 12:44:12 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed

Timerange: 00/11:15:02 to 00/11:16:58

JV - MC

IF 1(LL)

2.5

1.5 IF 2(LL)

200 -200

JV - MC

IF 1(RR)

5.0

4.0

3.0 IF 2(RR)

200 -200

JB - MC

IF 1(LL)

5.5

4.5

3.5

2.5 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

11

9

7 IF 2(RR)

200 -200

EF - MC

IF 1(LL)

12 10 8 6 IF 2(LL)

200 -200

EF - MC

IF 1(RR)

Channels

0 5 10 15

2.0

1.6

1.2 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

2.0

1.6

1.2 IF 2(LL)

0 5 10 15

200 -200

ON - MC

IF 1(RR)

Channels

0 5 10 15

3.0

2.6

2.2 IF 2(RR)

0 5 10 15

200 -200

MC - NT

IF 1(LL)

2.6

2.2

1.8 IF 2(LL)

200 -200

Plot file version 68 created 02-JUL-2004 12:44:12 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/11:15:02 to 00/11:16:58

MC - NT

IF 1(RR)

2.5

1.5 IF 2(RR)

200 -200

Plot file version 69 created 02-JUL-2004 12:44:12 J0122+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/11:17:02 to 00/11:19:58

JV - MC

IF 1(LL)

3.0

2.0 IF 2(LL)

200 -200

JV - MC

IF 1(RR)

7.0

6.0

5.0

4.0 IF 2(RR)

200 -200

JB - MC

IF 1(LL)

6.0 5.0 4.0 3.0 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

15 13 11 9 IF 2(RR)

200 -200

EF - MC

IF 1(LL)

12

8 IF 2(LL)

200 -200

EF - MC

IF 1(RR)

Channels

0 5 10 15

2.2

1.8

1.4 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

2.2

1.8

1.4 IF 2(LL)

0 5 10 15

200 -200

ON - MC

IF 1(RR)

Channels

0 5 10 15

3.4

3.0

2.6 IF 2(RR)

0 5 10 15

200 -200

MC - NT

IF 1(LL)

3.0

2.0 IF 2(LL)

200 -200

Plot file version 70 created 02-JUL-2004 12:44:13 J0122+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/11:17:02 to 00/11:19:58

MC - NT

IF 1(RR)

2.5

1.5 IF 2(RR)

200 -200

Plot file version 71 created 02-JUL-2004 12:44:13 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/11:20:02 to 00/11:21:58

JV - MC

IF 1(LL)

2.8 2.4 2.0 1.6 IF 2(LL)

200 -200

JV - MC

IF 1(RR)

1.4

1.2

1.0 IF 2(RR)

200 -200

JB - MC

IF 1(LL)

1.4

1.2

1.0 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

11

9

7 IF 2(RR)

200 -200

EF - MC

IF 1(LL)

12

10

8

6 IF 2(LL)

200 -200

EF - MC

IF 1(RR)

Channels

0 5 10 15

2.0

1.6

1.2 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

2.0

1.6

1.2 IF 2(LL)

0 5 10 15

200 -200

ON - MC

IF 1(RR)

Channels

0 5 10 15

3.0

2.6

2.2 IF 2(RR)

0 5 10 15

200 -200

MC - NT

IF 1(LL)

2.6

2.2

1.8 IF 2(LL)

200 -200

Plot file version 72 created 02-JUL-2004 12:44:13 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/11:20:02 to 00/11:21:58

MC - NT

IF 1(RR)

2.0

1.6

1.2 IF 2(RR)

200 -200

Plot file version 75 created 02-JUL-2004 12:44:13 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed

Timerange: 00/11:25:02 to 00/11:29:58

JV - MC

IF 1(LL)

2.8 2.4 2.0 1.6 IF 2(LL)

200 -200 JV - MC

IF 1(RR)

5.5

4.5

3.5 IF 2(RR)

200 -200 JB - MC

IF 1(LL)

4.5

3.5

2.5 IF 2(LL)

200 -200 JB - MC

IF 1(RR)

11

9

7 IF 2(RR)

200 -200 EF - MC

IF 1(LL)

12

10

8

6 IF 2(LL)

200 -200 EF - MC

IF 1(RR)

Channels

0 5 10 15

2.0

1.6

1.2 IF 2(RR)

0 5 10 15

200 -200 ON - MC

IF 1(LL)

Channels

0 5 10 15

1.8

1.4 IF 2(LL)

0 5 10 15

200 -200 ON - MC

IF 1(RR)

Channels

0 5 10 15

2.6

2.2 IF 2(RR)

0 5 10 15

200 -200 MC - NT

IF 1(LL)

2.6

2.2

1.8 IF 2(LL)

200 -200

Plot file version 76 created 02-JUL-2004 12:44:13 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/11:25:02 to 00/11:29:58

MC - NT

IF 1(RR)

2.4 2.0 1.6 1.2 IF 2(RR)

200 -200

Plot file version 77 created 02-JUL-2004 12:44:13 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/11:33:02 to 00/11:34:58

JV - MC

IF 1(LL)

2.5

1.5 IF 2(LL)

200 -200 JV - MC

IF 1(RR)

1.5 1.3 1.1 0.9 IF 2(RR)

200 -200 JB - MC

IF 1(LL)

1.4

1.0 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

11

9

7 IF 2(RR)

200 -200 EF - MC

IF 1(LL)

12

10

8

6 IF 2(LL)

200 -200 EF - MC

IF 1(RR)

Channels

0 5 10 15

2.0

1.6

1.2 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

2.0

1.6

1.2 IF 2(LL)

0 5 10 15

200 -200 ON - MC

IF 1(RR)

Channels

0 5 10 15

2.8

2.4

2.0 IF 2(RR)

0 5 10 15

200 -200 MC - NT

IF 1(LL)

2.6

2.2

1.8 IF 2(LL)

200 -200

Plot file version 78 created 02-JUL-2004 12:44:13 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/11:33:02 to 00/11:34:58

MC - NT

IF 1(RR)

2.0

1.6

1.2 IF 2(RR)

200 -200

Plot file version 79 created 02-JUL-2004 12:44:13 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed

Timerange: 00/11:38:02 to 00/11:39:58

JV - MC

IF 1(LL)

2.5

1.5 IF 2(LL)

200 -200

JV - MC

IF 1(RR)

5.5

4.5

3.5 IF 2(RR)

200 -200

JB - MC

IF 1(LL)

4.5

3.5

2.5 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

11

9

7 IF 2(RR)

200 -200

EF - MC

IF 1(LL)

10

8

6 IF 2(LL)

200 -200

EF - MC

IF 1(RR)

Channels

0 5 10 15

2.0

1.6

1.2 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

2.0

1.6

1.2 IF 2(LL)

0 5 10 15

200 -200

ON - MC

IF 1(RR)

Channels

0 5 10 15

2.8

2.4

2.0 IF 2(RR)

0 5 10 15

200 -200

MC - NT

IF 1(LL)

2.6

2.2

1.8 IF 2(LL)

200 -200

Plot file version 80 created 02-JUL-2004 12:44:13 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/11:38:02 to 00/11:39:58

MC - NT

IF 1(RR)

2.0

1.0 IF 2(RR)

200 -200

Plot file version 81 created 02-JUL-2004 12:44:13 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed

Timerange: 00/11:43:02 to 00/11:44:58

JV - MC

IF 1(LL)

2.5

1.5 IF 2(LL)

200 -200

JV - MC

IF 1(RR)

1.4

1.2

1.0 IF 2(RR)

200 -200

JB - MC

IF 1(LL)

1.4

1.2

1.0 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

11

9

7 IF 2(RR)

200 -200

EF - MC

IF 1(LL)

10

8

6 IF 2(LL)

200 -200

EF - MC

IF 1(RR)

Channels

0 5 10 15

2.0

1.6

1.2 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

2.0

1.6

1.2 IF 2(LL)

0 5 10 15

200 -200

ON - MC

IF 1(RR)

Channels

0 5 10 15

3.0

2.6

2.2 IF 2(RR)

0 5 10 15

200 -200

MC - NT

IF 1(LL)

2.4

2.0 IF 2(LL)

200 -200

Plot file version 82 created 02-JUL-2004 12:44:13 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/11:43:02 to 00/11:44:58

MC - NT

IF 1(RR)

2.0

1.0 IF 2(RR)

200 -200

Plot file version 83 created 02-JUL-2004 12:44:13 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed

Timerange: 00/11:48:02 to 00/11:52:57

JV - MC

IF 1(LL)

2.5

1.5 IF 2(LL)

200 -200

JV - MC

IF 1(RR)

5.5

4.5

3.5 IF 2(RR)

200 -200

JB - MC

IF 1(LL)

4.5

3.5

2.5 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

11

9

7 IF 2(RR)

200 -200

EF - MC

IF 1(LL)

10

8

6 IF 2(LL)

200 -200

EF - MC

IF 1(RR)

Channels

0 5 10 15

2.0

1.6

1.2 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

1.8

1.4 IF 2(LL)

0 5 10 15

200 -200

ON - MC

IF 1(RR)

Channels

0 5 10 15

2.6

2.2 IF 2(RR)

0 5 10 15

200 -200

MC - NT

IF 1(LL)

2.6

2.2

1.8 IF 2(LL)

200 -200

Plot file version 84 created 02-JUL-2004 12:44:13 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/11:48:02 to 00/11:52:57

MC - NT

IF 1(RR)

2.0

1.0 IF 2(RR)

200 -200

Plot file version 85 created 02-JUL-2004 12:44:13 J0122+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/11:53:01 to 00/11:55:57

JV - MC

IF 1(LL)

3.0

2.0 IF 2(LL)

200 -200

JV - MC

IF 1(RR)

7.0

6.0

5.0

4.0 IF 2(RR)

200 -200

JB - MC

IF 1(LL)

6.0 5.0 4.0 3.0 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

15 13 11 9 IF 2(RR)

200 -200

EF - MC

IF 1(LL)

12

8 IF 2(LL)

200 -200

EF - MC

IF 1(RR)

Channels

0 5 10 15

2.2

1.8

1.4 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

2.2

1.8

1.4 IF 2(LL)

0 5 10 15

200 -200

ON - MC

IF 1(RR)

Channels

0 5 10 15

3.4

3.0

2.6 IF 2(RR)

0 5 10 15

200 -200

MC - NT

IF 1(LL)

3.2

2.8

2.4 IF 2(LL)

200 -200

Plot file version 86 created 02-JUL-2004 12:44:13 J0122+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/11:53:01 to 00/11:55:57

MC - NT

IF 1(RR)

2.4 2.0 1.6 1.2 IF 2(RR)

200 -200

Plot file version 87 created 02-JUL-2004 12:44:13 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/11:56:01 to 00/11:57:57

JV - MC

IF 1(LL)

2.8 2.4 2.0 1.6 IF 2(LL)

200 -200

JV - MC

IF 1(RR)

1.5

1.3

1.1 IF 2(RR)

200 -200

JB - MC

IF 1(LL)

1.4

1.2

1.0 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

11

9

7 IF 2(RR)

200 -200

EF - MC

IF 1(LL)

10

8

6 IF 2(LL)

200 -200

EF - MC

IF 1(RR)

Channels

0 5 10 15

2.2

1.8

1.4 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

2.0

1.6

1.2 IF 2(LL)

0 5 10 15

200 -200

ON - MC

IF 1(RR)

Channels

0 5 10 15

2.6

2.2 IF 2(RR)

0 5 10 15

200 -200

MC - NT

IF 1(LL)

3.0

2.0 IF 2(LL)

200 -200

Plot file version 90 created 02-JUL-2004 12:44:13 J0122+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/11:58:01 to 00/12:00:57

MC - NT

IF 1(RR)

2.0

1.6

1.2 IF 2(RR)

200 -200

Plot file version 91 created 02-JUL-2004 12:44:13 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed

Timerange: 00/12:01:01 to 00/12:02:57

JV - MC

IF 1(LL)

2.5

1.5 IF 2(LL)

200 -200 JV - MC

IF 1(RR)

5.5

4.5

3.5 IF 2(RR)

200 -200 JB - MC

IF 1(LL)

4.5

3.5

2.5 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

11

9

7 IF 2(RR)

200 -200 EF - MC

IF 1(LL)

10

8

6 IF 2(LL)

200 -200 EF - MC

IF 1(RR)

Channels

0 5 10 15

2.0

1.6

1.2 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

2.2

1.8

1.4 IF 2(LL)

0 5 10 15

200 -200 ON - MC

IF 1(RR)

Channels

0 5 10 15

3.0

2.6

2.2 IF 2(RR)

0 5 10 15

200 -200 MC - NT

IF 1(LL)

2.8

2.4

2.0 IF 2(LL)

200 -200

Plot file version 92 created 02-JUL-2004 12:44:13 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/12:01:01 to 00/12:02:57

MC - NT

IF 1(RR)

2.2

1.8

1.4

1.0 IF 2(RR)

200 -200

Plot file version 93 created 02-JUL-2004 12:44:13 J0122+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/12:03:01 to 00/12:05:57

JV - MC

IF 1(LL)

2.5

1.5 IF 2(LL)

200 -200

JV - MC

IF 1(RR)

7.0

6.0

5.0

4.0 IF 2(RR)

200 -200 JB - MC

IF 1(LL)

6.0 5.0 4.0 3.0 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

15 13 11 9 IF 2(RR)

200 -200

EF - MC

IF 1(LL)

12

8 IF 2(LL)

200 -200 EF - MC

IF 1(RR)

Channels

0 5 10 15

2.2

1.8

1.4 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

2.2

1.8

1.4 IF 2(LL)

0 5 10 15

200 -200

ON - MC

IF 1(RR)

Channels

0 5 10 15

3.4

3.0

2.6 IF 2(RR)

0 5 10 15

200 -200 MC - NT

IF 1(LL)

3.0

2.0 IF 2(LL)

200 -200

Plot file version 94 created 02-JUL-2004 12:44:13 J0122+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/12:03:01 to 00/12:05:57

MC - NT

IF 1(RR)

1.8

1.4

1.0 IF 2(RR)

200 -200

Plot file version 95 created 02-JUL-2004 12:44:13 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/12:06:01 to 00/12:07:57

JV - MC

IF 1(LL)

2.2

1.8

1.4 IF 2(LL)

200 -200

JV - MC

IF 1(RR)

1.4

1.2

1.0 IF 2(RR)

200 -200

JB - MC

IF 1(LL)

1.6 1.4 1.2 1.0 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

11

9

7 IF 2(RR)

200 -200

EF - MC

IF 1(LL)

10

8

6 IF 2(LL)

200 -200

EF - MC

IF 1(RR)

Channels

0 5 10 15

2.0

1.6

1.2 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

2.2

1.8

1.4 IF 2(LL)

0 5 10 15

200 -200

ON - MC

IF 1(RR)

Channels

0 5 10 15

2.6

2.2 IF 2(RR)

0 5 10 15

200 -200

MC - NT

IF 1(LL)

2.6

2.2

1.8 IF 2(LL)

200 -200

Plot file version 96 created 02-JUL-2004 12:44:14 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/12:06:01 to 00/12:07:57

MC - NT

IF 1(RR)

2.4 2.0 1.6 1.2 IF 2(RR)

200 -200

Plot file version 97 created 02-JUL-2004 12:44:14 J0122+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/12:08:01 to 00/12:10:57

JV - MC

IF 1(LL)

2.5

1.5 IF 2(LL)

200 -200

JV - MC

IF 1(RR)

7.0

6.0

5.0

4.0 IF 2(RR)

200 -200

JB - MC

IF 1(LL)

6.0 5.0 4.0 3.0 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

15 13 11 9 IF 2(RR)

200 -200

EF - MC

IF 1(LL)

12

8 IF 2(LL)

200 -200

EF - MC

IF 1(RR)

Channels

0 5 10 15

2.2

1.8

1.4 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

2.4

2.0

1.6

1.2 IF 2(LL)

0 5 10 15

200 -200

ON - MC

IF 1(RR)

Channels

0 5 10 15

3.4

3.0

2.6 IF 2(RR)

0 5 10 15

200 -200

MC - NT

IF 1(LL)

3.2 2.8 2.4 2.0 IF 2(LL)

200 -200

Plot file version 98 created 02-JUL-2004 12:44:14 J0122+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/12:08:01 to 00/12:10:57

MC - NT

IF 1(RR)

2.0

1.0 IF 2(RR)

200 -200

Plot file version 99 created 02-JUL-2004 12:44:14 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/12:11:01 to 00/12:15:58

JV - MC

IF 1(LL)

2.5

1.5 IF 2(LL)

200 -200

JV - MC

IF 1(RR)

5.5

4.5

3.5 IF 2(RR)

200 -200

JB - MC

IF 1(LL)

4.5

3.5

2.5 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

11

9

7 IF 2(RR)

200 -200

EF - MC

IF 1(LL)

10

8

6 IF 2(LL)

200 -200

EF - MC

IF 1(RR)

Channels

0 5 10 15

2.0

1.6

1.2 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

1.8

1.4 IF 2(LL)

0 5 10 15

200 -200

ON - MC

IF 1(RR)

Channels

0 5 10 15

2.6

2.2 IF 2(RR)

0 5 10 15

200 -200

MC - NT

IF 1(LL)

2.6

2.2

1.8 IF 2(LL)

200 -200

Plot file version 100 created 02-JUL-2004 12:44:14 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/12:11:01 to 00/12:15:58

MC - NT

IF 1(RR)

2.0

1.6

1.2 IF 2(RR)

200 -200

Plot file version 101 created 02-JUL-2004 12:44:14 J0122+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed

Timerange: 00/12:16:02 to 00/12:18:58

JV - MC

IF 1(LL)

3.0

2.0 IF 2(LL)

200 -200

JV - MC

IF 1(RR)

7.0 6.0 5.0 4.0 IF 2(RR)

200 -200

JB - MC

IF 1(LL)

6.5 5.5 4.5 3.5 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

13

11

9 IF 2(RR)

200 -200

EF - MC

IF 1(LL)

12

8 IF 2(LL)

200 -200

EF - MC

IF 1(RR)

Channels

0 5 10 15

2.4

2.0

1.6 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

2.2

1.8

1.4 IF 2(LL)

0 5 10 15

200 -200

ON - MC

IF 1(RR)

Channels

0 5 10 15

3.6

3.2

2.8

2.4 IF 2(RR)

0 5 10 15

200 -200

MC - NT

IF 1(LL)

3.0 2.6 2.2 IF 2(LL)

200 -200

Plot file version 102 created 02-JUL-2004 12:44:14 J0122+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/12:16:02 to 00/12:18:58

MC - NT

IF 1(RR)

2.4 2.0 1.6 1.2 IF 2(RR)

200 -200

Plot file version 105 created 02-JUL-2004 12:44:14 J0122+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/12:21:02 to 00/12:23:58

JV - MC

IF 1(LL)

2.5

1.5 IF 2(LL)

200 -200 JV - MC

IF 1(RR)

7.0

6.0

5.0

4.0 IF 2(RR)

200 -200 JB - MC

IF 1(LL)

6.0 5.0 4.0 3.0 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

14 12 10 8 IF 2(RR)

200 -200 EF - MC

IF 1(LL)

12

8 IF 2(LL)

200 -200 EF - MC

IF 1(RR)

Channels

0 5 10 15

2.2

1.8

1.4 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

2.6 2.2 1.8 1.4 IF 2(LL)

0 5 10 15

200 -200 ON - MC

IF 1(RR)

Channels

0 5 10 15

3.4

3.0

2.6 IF 2(RR)

0 5 10 15

200 -200 MC - NT

IF 1(LL)

3.0

2.0 IF 2(LL)

200 -200

Plot file version 106 created 02-JUL-2004 12:44:14 J0122+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/12:21:02 to 00/12:23:58

MC - NT

IF 1(RR)

2.2

1.8

1.4

1.0 IF 2(RR)

200 -200

Plot file version 107 created 02-JUL-2004 12:44:14 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/12:24:02 to 00/12:25:58

JV - MC

IF 1(LL)

2.6 2.2 1.8 1.4 IF 2(LL)

200 -200 JV - MC

IF 1(RR)

5.5

4.5

3.5 IF 2(RR)

200 -200 JB - MC

IF 1(LL)

5.0

4.0

3.0 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

11

9

7 IF 2(RR)

200 -200 EF - MC

IF 1(LL)

10

8

6 IF 2(LL)

200 -200 EF - MC

IF 1(RR)

Channels

0 5 10 15

2.0

1.6

1.2 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

2.0

1.6

1.2 IF 2(LL)

0 5 10 15

200 -200 ON - MC

IF 1(RR)

Channels

0 5 10 15

2.8 2.6 2.4 2.2 IF 2(RR)

0 5 10 15

200 -200 MC - NT

IF 1(LL)

2.6

2.2

1.8 IF 2(LL)

200 -200

Plot file version 108 created 02-JUL-2004 12:44:14 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/12:24:02 to 00/12:25:58

MC - NT

IF 1(RR)

2.5

1.5 IF 2(RR)

200 -200

Plot file version 109 created 02-JUL-2004 12:44:14 J0122+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/12:26:02 to 00/12:28:58

JV - MC

IF 1(LL)

2.5

1.5 IF 2(LL)

200 -200

JV - MC

IF 1(RR)

7.0

6.0

5.0

4.0 IF 2(RR)

200 -200

JB - MC

IF 1(LL)

6.0 5.0 4.0 3.0 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

13

11

9 IF 2(RR)

200 -200

EF - MC

IF 1(LL)

12

8 IF 2(LL)

200 -200

EF - MC

IF 1(RR)

Channels

0 5 10 15

2.2

1.8

1.4 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

2.2

1.8

1.4 IF 2(LL)

0 5 10 15

200 -200

ON - MC

IF 1(RR)

Channels

0 5 10 15

3.4

3.0

2.6 IF 2(RR)

0 5 10 15

200 -200

MC - NT

IF 1(LL)

3.0 2.6 2.2 IF 2(LL)

200 -200

Plot file version 110 created 02-JUL-2004 12:44:14 J0122+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/12:26:02 to 00/12:28:58

MC - NT

IF 1(RR)

2.2

1.8

1.4

1.0 IF 2(RR)

200 -200

Plot file version 111 created 02-JUL-2004 12:44:14 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/12:29:02 to 00/12:30:58

JV - MC

IF 1(LL)

2.6 2.2 1.8 1.4 IF 2(LL)

200 -200

JV - MC

IF 1(RR)

1.5 1.3 1.1 0.9 IF 2(RR)

200 -200

JB - MC

IF 1(LL)

1.4

1.2

1.0 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

11

9

7 IF 2(RR)

200 -200

EF - MC

IF 1(LL)

10

8

6 IF 2(LL)

200 -200

EF - MC

IF 1(RR)

Channels

0 5 10 15

2.0

1.6

1.2 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

2.0

1.6

1.2 IF 2(LL)

0 5 10 15

200 -200

ON - MC

IF 1(RR)

Channels

0 5 10 15

2.6

2.2 IF 2(RR)

0 5 10 15

200 -200

MC - NT

IF 1(LL)

2.6

2.2

1.8 IF 2(LL)

200 -200

Plot file version 112 created 02-JUL-2004 12:44:14 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/12:29:02 to 00/12:30:58

MC - NT

IF 1(RR)

2.0

1.6

1.2 IF 2(RR)

200 -200

Plot file version 113 created 02-JUL-2004 12:44:14 J0122+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed

Timerange: 00/12:31:02 to 00/12:33:58

JV - MC

IF 1(LL)

2.5

1.5 IF 2(LL)

200 -200

JV - MC

IF 1(RR)

7.0 6.0 5.0 4.0 IF 2(RR)

200 -200

JB - MC

IF 1(LL)

6.0 5.0

4.0 3.0 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

14

12

10

8 IF 2(RR)

200 -200

EF - MC

IF 1(LL)

12

8 IF 2(LL)

200 -200

EF - MC

IF 1(RR)

Channels

0 5 10 15

2.2

1.8

1.4 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

2.2

1.8

1.4 IF 2(LL)

0 5 10 15

200 -200

ON - MC

IF 1(RR)

Channels

0 5 10 15

3.4

3.0

2.6 IF 2(RR)

0 5 10 15

200 -200

MC - NT

IF 1(LL)

3.0

2.6

2.2 IF 2(LL)

200 -200

Plot file version 114 created 02-JUL-2004 12:44:14 J0122+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/12:31:02 to 00/12:33:58

MC - NT

IF 1(RR)

2.4 2.0 1.6 1.2 IF 2(RR)

200 -200

Plot file version 115 created 02-JUL-2004 12:44:14 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/12:34:02 to 00/12:38:58

JV - MC

IF 1(LL)

2.5

1.5 IF 2(LL)

200 -200

JV - MC

IF 1(RR)

5.5

4.5

3.5 IF 2(RR)

200 -200

JB - MC

IF 1(LL)

5.0

4.0

3.0 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

11

9

7 IF 2(RR)

200 -200

EF - MC

IF 1(LL)

10

8

6 IF 2(LL)

200 -200

EF - MC

IF 1(RR)

Channels

0 5 10 15

2.0

1.6

1.2 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

2.0

1.6

1.2 IF 2(LL)

0 5 10 15

200 -200

ON - MC

IF 1(RR)

Channels

0 5 10 15

2.8

2.4

2.0 IF 2(RR)

0 5 10 15

200 -200

MC - NT

IF 1(LL)

2.6

2.2

1.8 IF 2(LL)

200 -200

Plot file version 116 created 02-JUL-2004 12:44:14 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/12:34:02 to 00/12:38:58

MC - NT

IF 1(RR)

2.0

1.6

1.2 IF 2(RR)

200 -200

Plot file version 117 created 02-JUL-2004 12:44:14 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/12:42:02 to 00/12:43:58

JV - MC

IF 1(LL)

2.6 2.2 1.8 1.4 IF 2(LL)

200 -200

JV - MC

IF 1(RR)

1.5

1.3

1.1

0.9 IF 2(RR)

200 -200

JB - MC

IF 1(LL)

1.3

1.1

0.9 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

11

9

7 IF 2(RR)

200 -200

EF - MC

IF 1(LL)

10

8

6 IF 2(LL)

200 -200

EF - MC

IF 1(RR)

Channels

0 5 10 15

1.6

1.2 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

1.6

1.2 IF 2(LL)

0 5 10 15

200 -200

ON - MC

IF 1(RR)

Channels

0 5 10 15

3.0

2.6

2.2

1.8 IF 2(RR)

0 5 10 15

200 -200

MC - NT

IF 1(LL)

2.6

2.2

1.8 IF 2(LL)

200 -200

Plot file version 120 created 02-JUL-2004 12:44:15 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/12:47:02 to 00/12:48:58

MC - NT

IF 1(RR)

1.8

1.4

1.0 IF 2(RR)

200 -200

Plot file version 121 created 02-JUL-2004 12:44:15 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/12:57:02 to 00/13:01:58

JV - MC

IF 1(LL)

2.5

1.5 IF 2(LL)

200 -200 JV - MC

IF 1(RR)

5.0

4.0

3.0 IF 2(RR)

200 -200 JB - MC

IF 1(LL)

4.5

3.5

2.5 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

11

9

7 IF 2(RR)

200 -200 EF - MC

IF 1(LL)

10

8

6 IF 2(LL)

200 -200 EF - MC

IF 1(RR)

Channels

0 5 10 15

1.6

1.2 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

1.6

1.2 IF 2(LL)

0 5 10 15

200 -200 ON - MC

IF 1(RR)

Channels

0 5 10 15

2.8

2.4

2.0 IF 2(RR)

0 5 10 15

200 -200 MC - NT

IF 1(LL)

2.6

2.2

1.8 IF 2(LL)

200 -200

Plot file version 122 created 02-JUL-2004 12:44:15 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/12:57:02 to 00/13:01:58

MC - NT

IF 1(RR)

2.0

1.0 IF 2(RR)

200 -200

Plot file version 123 created 02-JUL-2004 12:44:15 J0122+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/13:02:02 to 00/13:04:58

JV - MC

IF 1(LL)

2.5

1.5 IF 2(LL)

200 -200

JV - MC

IF 1(RR)

6.0

5.0

4.0 IF 2(RR)

200 -200

JB - MC

IF 1(LL)

5.0

4.0

3.0 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

14

12

10

8 IF 2(RR)

200 -200

EF - MC

IF 1(LL)

12

8 IF 2(LL)

200 -200

EF - MC

IF 1(RR)

Channels

0 5 10 15

1.6

1.2 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

1.6

1.2 IF 2(LL)

0 5 10 15

200 -200

ON - MC

IF 1(RR)

Channels

0 5 10 15

3.0

2.6 IF 2(RR)

0 5 10 15

200 -200

MC - NT

IF 1(LL)

3.0

2.6

2.2 IF 2(LL)

200 -200

Plot file version 124 created 02-JUL-2004 12:44:15 J0122+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/13:02:02 to 00/13:04:58

MC - NT

IF 1(RR)

2.0

1.6

1.2 IF 2(RR)

200 -200

Plot file version 125 created 02-JUL-2004 12:44:15 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed

Timerange: 00/13:05:02 to 00/13:06:58

JV - MC

IF 1(LL)

2.5

1.5 IF 2(LL)

200 -200

JV - MC

IF 1(RR)

1.4

1.2

1.0 IF 2(RR)

200 -200

JB - MC

IF 1(LL)

1.4

1.2

1.0 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

10

8

6 IF 2(RR)

200 -200

EF - MC

IF 1(LL)

10

8

6 IF 2(LL)

200 -200

EF - MC

IF 1(RR)

Channels

0 5 10 15

1.4

1.0 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

1.4

1.0 IF 2(LL)

0 5 10 15

200 -200

ON - MC

IF 1(RR)

Channels

0 5 10 15

2.8

2.4

2.0 IF 2(RR)

0 5 10 15

200 -200

MC - NT

IF 1(LL)

2.4

2.0 IF 2(LL)

200 -200

Plot file version 126 created 02-JUL-2004 12:44:15 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/13:05:02 to 00/13:06:58

MC - NT

IF 1(RR)

2.0

1.6

1.2 IF 2(RR)

200 -200

Plot file version 127 created 02-JUL-2004 12:44:15 J0122+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/13:07:02 to 00/13:09:58

JV - MC

IF 1(LL)

3.0 2.6 2.2 1.8 IF 2(LL)

200 -200

JV - MC

IF 1(RR)

6.0

5.0

4.0 IF 2(RR)

200 -200

JB - MC

IF 1(LL)

5.0

4.0

3.0 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

12

10

8 IF 2(RR)

200 -200

EF - MC

IF 1(LL)

13 11 9 7 IF 2(LL)

200 -200

EF - MC

IF 1(RR)

Channels

0 5 10 15

1.6

1.2 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

1.6

1.2 IF 2(LL)

0 5 10 15

200 -200

ON - MC

IF 1(RR)

Channels

0 5 10 15

3.2

2.8

2.4 IF 2(RR)

0 5 10 15

200 -200

MC - NT

IF 1(LL)

3.2

2.8 2.4

2.0 IF 2(LL)

200 -200

Plot file version 128 created 02-JUL-2004 12:44:15 J0122+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/13:07:02 to 00/13:09:58

MC - NT

IF 1(RR)

2.2 1.8 1.4 1.0 IF 2(RR)

200 -200

Plot file version 129 created 02-JUL-2004 12:44:15 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/13:10:02 to 00/13:11:58

JV - MC

IF 1(LL)

2.5

1.5 IF 2(LL)

200 -200

JV - MC

IF 1(RR)

6.0

5.0

4.0

3.0 IF 2(RR)

200 -200

JB - MC

IF 1(LL)

4.5

3.5

2.5 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

11

9

7 IF 2(RR)

200 -200

EF - MC

IF 1(LL)

10

8

6 IF 2(LL)

200 -200

EF - MC

IF 1(RR)

Channels

0 5 10 15

1.8 1.6 1.4 1.2 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

1.8

1.4

1.0 IF 2(LL)

0 5 10 15

200 -200

ON - MC

IF 1(RR)

Channels

0 5 10 15

2.8

2.4

2.0 IF 2(RR)

0 5 10 15

200 -200

MC - NT

IF 1(LL)

2.6

2.2

1.8 IF 2(LL)

200 -200

Plot file version 130 created 02-JUL-2004 12:44:15 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/13:10:02 to 00/13:11:58

MC - NT

IF 1(RR)

2.4 2.0 1.6 1.2 IF 2(RR)

200 -200

Plot file version 131 created 02-JUL-2004 12:44:15 J0122+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/13:12:02 to 00/13:14:58

JV - MC

IF 1(LL)

2.8 2.4 2.0 1.6 IF 2(LL)

200 -200

JV - MC

IF 1(RR)

5.5

4.5

3.5 IF 2(RR)

200 -200

JB - MC

IF 1(LL)

5.0

4.0

3.0 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

12

10

8 IF 2(RR)

200 -200

EF - MC

IF 1(LL)

13 11 9 7 IF 2(LL)

200 -200

EF - MC

IF 1(RR)

Channels

0 5 10 15

2.0

1.6

1.2 IF 2(RR) 0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

2.0

1.6

1.2 IF 2(LL)

0 5 10 15

200 -200

ON - MC

IF 1(RR)

Channels

0 5 10 15

3.2

2.8

2.4 IF 2(RR)

0 5 10 15

200 -200

MC - NT

IF 1(LL)

3.2

2.8

2.4

2.0 IF 2(LL)

200 -200

Plot file version 132 created 02-JUL-2004 12:44:15 J0122+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/13:12:02 to 00/13:14:58

MC - NT

IF 1(RR)

2.0

1.6

1.2 IF 2(RR)

200 -200

Plot file version 135 created 02-JUL-2004 12:44:15 J0122+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/13:17:02 to 00/13:19:58

JV - MC

IF 1(LL)

2.5

1.5 IF 2(LL)

200 -200 JV - MC

IF 1(RR)

6.0

5.0

4.0 IF 2(RR)

200 -200 JB - MC

IF 1(LL)

5.0

4.0

3.0 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

12

10

8 IF 2(RR)

200 -200 EF - MC

IF 1(LL)

13 11 9 7 IF 2(LL)

200 -200 EF - MC

IF 1(RR)

Channels

0 5 10 15

2.0

1.6

1.2 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

1.6

1.2 IF 2(LL)

0 5 10 15

200 -200 ON - MC

IF 1(RR)

Channels

0 5 10 15

3.0

2.6

2.2 IF 2(RR)

0 5 10 15

200 -200 MC - NT

IF 1(LL)

3.2

2.8

2.4

2.0 IF 2(LL)

200 -200

Plot file version 136 created 02-JUL-2004 12:44:15 J0122+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/13:17:02 to 00/13:19:58

MC - NT

IF 1(RR)

1.8

1.4

1.0 IF 2(RR)

200 -200

Plot file version 137 created 02-JUL-2004 12:44:15 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/13:20:02 to 00/13:21:58

JV - MC

IF 1(LL)

2.4

2.0

1.6 IF 2(LL)

200 -200 JV - MC

IF 1(RR)

5.5

4.5

3.5 IF 2(RR)

200 -200 JB - MC

IF 1(LL)

4.5

3.5

2.5 IF 2(LL)

200 -200 JB - MC

IF 1(RR)

11

9

7 IF 2(RR)

200 -200 EF - MC

IF 1(LL)

10

8

6 IF 2(LL)

200 -200 EF - MC

IF 1(RR)

Channels

0 5 10 15

1.6

1.2 IF 2(RR)

0 5 10 15

200 -200 ON - MC

IF 1(LL)

Channels

0 5 10 15

1.6

1.2 IF 2(LL)

0 5 10 15

200 -200 ON - MC

IF 1(RR)

Channels

0 5 10 15

2.4

2.0 IF 2(RR)

0 5 10 15

200 -200 MC - NT

IF 1(LL)

2.4

2.0

1.6 IF 2(LL)

200 -200

Plot file version 138 created 02-JUL-2004 12:44:15 J0126+25 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/13:20:02 to 00/13:21:58

MC - NT

IF 1(RR)

3.0

2.6 IF 2(RR)

200 -200

Plot file version 139 created 02-JUL-2004 12:44:15 DA193 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/13:32:12 to 00/13:53:58

JV - MC

IF 1(LL)

14

10 IF 2(LL)

200 -200

JV - MC

IF 1(RR)

35

25 IF 2(RR)

200 -200 JB - MC

IF 1(LL)

30

20 IF 2(LL)

200 -200

JB - MC

IF 1(RR)

70

50 IF 2(RR)

200 -200

EF - MC

IF 1(LL)

80

60

40 IF 2(LL)

200 -200 EF - MC

IF 1(RR)

Channels

0 5 10 15

10

8

6 IF 2(RR)

0 5 10 15

200 -200

ON - MC

IF 1(LL)

Channels

0 5 10 15

10

8

6 IF 2(LL)

0 5 10 15

200 -200

ON - MC

IF 1(RR)

Channels

0 5 10 15

20

16 IF 2(RR)

0 5 10 15

200 -200 MC - NT

IF 1(LL)

18

14 IF 2(LL)

200 -200

Plot file version 140 created 02-JUL-2004 12:44:16 DA193 f04c4.MSORT.1 Freq = 4.9825 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Milli Ampl Jy Top frame: Phas deg Scalar averaged cross-power spectrum Several baselines displayed Timerange: 00/13:32:12 to 00/13:53:58

MC - NT