IF 1(RR)

1.2

0.8

0.4

0.0

Plot file version 1 created 24-MAY-2005 14:28:55 J2031+12 ig002b.MSORT.1 Freq = 1.6505 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Real Jy Total-power spectrum Antenna: * Timerange: 00/12:45:38 to 00/12:55:34

CM

IF 1(LL)

1.2 0.8 0.4 0.0

CM

IF 1(RR)

1.0

0.8

0.6

WB

IF 1(LL)

1.1 0.9 0.7 0.5

WB

IF 1(RR)

1.2 1.0 0.8 0.6 0.4

ON

IF 1(LL)

1.3 1.1 0.9 0.7 0.5

ON

IF 1(RR) FREQ MHz

1652 1654 1656 1658

1.5 1.3 1.1 0.9

TR

IF 1(LL) FREQ MHz

1652 1654 1656 1658

1.00

0.90

0.80

TR

IF 1(RR) FREQ MHz

1652 1654 1656 1658

1.10

1.00

0.90

AR

IF 1(LL)

1.00

0.90

0.80

Plot file version 2 created 24-MAY-2005 14:28:56 J2031+12 ig002b.MSORT.1 Freq = 1.6505 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Real Jy Total-power spectrum Antenna: * Timerange: 00/12:45:38 to 00/12:55:34

AR

IF 1(RR)

1.2

0.8

0.4

0.0

Plot file version 3 created 24-MAY-2005 14:28:56 J2031+12 ig002b.MSORT.1 Freq = 1.6505 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Real Jy Total-power spectrum Antenna: * Timerange: 00/12:55:38 to 00/13:05:38

CM

IF 1(LL)

1.2

0.8

0.4

0.0

CM

IF 1(RR)

1.0

0.8

0.6

WB

IF 1(LL)

1.1

0.9

0.7

0.5

WB

IF 1(RR)

1.2

1.0

0.8

0.6

0.4

ON

IF 1(LL)

1.3 1.1 0.9 0.7 0.5

ON

IF 1(RR)

FREQ MHz

1652 1654 1656 1658

1.5 1.3 1.1 0.9

TR

IF 1(LL)

FREQ MHz

1652 1654 1656 1658

1.10

1.00

0.90

0.80

TR

IF 1(RR)

FREQ MHz

1652 1654 1656 1658

1.10

1.00

0.90

AR

IF 1(LL)

1.05

0.95

0.85

0.75

Plot file version 4 created 24-MAY-2005 14:28:56 J2031+12 ig002b.MSORT.1 Freq = 1.6505 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Real Jy Total-power spectrum Antenna: * Timerange: 00/12:55:38 to 00/13:05:38

AR

IF 1(RR)

1.2

0.8

0.4

0.0

Plot file version 5 created 24-MAY-2005 14:28:56 J2031+12 ig002b.MSORT.1 Freq = 1.6505 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Real Jy Total-power spectrum Antenna: * Timerange: 00/13:05:42 to 00/13:15:42

CM

IF 1(LL)

1.2

0.8

0.4

0.0

CM

IF 1(RR)

1.0

0.8

0.6

WB

IF 1(LL)

1.1

0.9

0.7

0.5

WB

IF 1(RR)

1.2

1.0

0.8

0.6

0.4

ON

IF 1(LL)

1.3 1.1 0.9 0.7 0.5

ON

IF 1(RR)

FREQ MHz

1652 1654 1656 1658

1.5

1.3

1.1

0.9

TR

IF 1(LL)

FREQ MHz

1652 1654 1656 1658

1.10

1.00

0.90

0.80

TR

IF 1(RR)

FREQ MHz

1652 1654 1656 1658

1.10

1.00

0.90

AR

IF 1(LL)

1.05

0.95

0.85

0.75

Plot file version 6 created 24-MAY-2005 14:28:56 J2031+12 ig002b.MSORT.1 Freq = 1.6505 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Real Jy Total-power spectrum Antenna: * Timerange: 00/13:05:42 to 00/13:15:42

AR

IF 1(RR)

1.2

0.8

0.4

0.0

Plot file version 7 created 24-MAY-2005 14:28:56 J2031+12 ig002b.MSORT.1 Freq = 1.6505 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Real Jy Total-power spectrum Antenna: * Timerange: 00/13:15:46 to 00/13:18:54

CM

IF 1(LL)

1.2

0.8

0.4

0.0

CM

IF 1(RR)

1.0

0.8

0.6

WB

IF 1(LL)

1.1

0.9

0.7

0.5

WB

IF 1(RR)

1.2

1.0

0.8

0.6

0.4

ON

IF 1(LL)

1.3 1.1 0.9 0.7 0.5

ON

IF 1(RR)

FREQ MHz

1652 1654 1656 1658

1.5

1.3

1.1

0.9

TR

IF 1(LL)

FREQ MHz

1652 1654 1656 1658

1.00

0.90

0.80

TR

IF 1(RR)

FREQ MHz

1652 1654 1656 1658

1.10

1.00

0.90

AR

IF 1(LL)

1.05

0.95

0.85

0.75

Plot file version 8 created 24-MAY-2005 14:28:56 J2031+12 ig002b.MSORT.1 Freq = 1.6505 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Real Jy Total-power spectrum Antenna: * Timerange: 00/13:15:46 to 00/13:18:54

AR

IF 1(RR)

1.0

0.8

0.6

Plot file version 9 created 24-MAY-2005 14:28:56 SN2001EM ig002b.MSORT.1 Freq = 1.6505 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Real Jy Total-power spectrum Antenna: * Timerange: 00/14:39:19 to 00/14:46:55

WB

IF 1(LL)

1.1

0.9

0.7

0.5

WB

IF 1(RR)

1.2 1.0 0.8 0.6 0.4

ON

IF 1(LL)

1.1

0.9

0.7

0.5

ON

IF 1(RR)

1.5

1.3

1.1

0.9

TR

IF 1(LL)

1.10

1.00

0.90

0.80

TR

IF 1(RR)

FREQ MHz

1652 1654 1656 1658

1.10

1.00

0.90

AR

IF 1(LL)

FREQ MHz

1652 1654 1656 1658

1.05

0.95

0.85

0.75

AR

IF 1(RR)

1.0

0.8

0.6

Plot file version 10 created 24-MAY-2005 14:28:56 J2145+11 ig002b.MSORT.1 Freq = 1.6505 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Real Jy Total-power spectrum Antenna: * Timerange: 00/14:47:03 to 00/14:49:55

WB

IF 1(LL)

1.1

0.9

0.7

0.5

WB

IF 1(RR)

1.2 1.0 0.8 0.6 0.4

ON

IF 1(LL)

1.1

0.9

0.7

0.5

ON

IF 1(RR)

1.7 1.5 1.3 1.1 0.9

TR

IF 1(LL)

1.10

1.00

0.90

0.80

TR

IF 1(RR)

FREQ MHz

1652 1654 1656 1658

1.10

1.00

0.90

AR

IF 1(LL)

FREQ MHz

1652 1654 1656 1658

1.05

0.95

0.85

0.75

AR

IF 1(RR)

1.0

0.8

0.6

Plot file version 11 created 24-MAY-2005 14:28:56 SN2001EM ig002b.MSORT.1 Freq = 1.6505 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Real Jy Total-power spectrum Antenna: * Timerange: 00/14:50:03 to 00/14:57:55

WB

IF 1(LL)

1.1

0.9

0.7

0.5

WB

IF 1(RR)

1.2 1.0 0.8 0.6 0.4

ON

IF 1(LL)

1.1

0.9

0.7

0.5

ON

IF 1(RR)

1.7 1.5 1.3 1.1 0.9

TR

IF 1(LL)

1.10

1.00

0.90

0.80

TR

IF 1(RR)

FREQ MHz

1652 1654 1656 1658

1.10

1.00

0.90

AR

IF 1(LL)

FREQ MHz

1652 1654 1656 1658

1.05

0.95

0.85

0.75

AR

IF 1(RR)

1.0

0.8

0.6

Plot file version 12 created 24-MAY-2005 14:28:56 J2145+11 ig002b.MSORT.1 Freq = 1.6505 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Real Jy Total-power spectrum Antenna: * Timerange: 00/14:58:03 to 00/15:00:55

WB

IF 1(LL)

1.1

0.9

0.7

0.5

WB

IF 1(RR)

1.2 1.0 0.8 0.6 0.4

ON

IF 1(LL)

1.1

0.9

0.7

0.5

ON

IF 1(RR)

1.7 1.5 1.3 1.1 0.9

TR

IF 1(LL)

1.15

1.05

0.95

0.85

0.75

TR

IF 1(RR)

1.0

0.8

0.6

Plot file version 15 created 24-MAY-2005 14:28:56 SN2001EM ig002b.MSORT.1 Freq = 1.6505 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Real Jy Total-power spectrum Antenna: * Timerange: 00/15:12:03 to 00/15:19:55

WB

IF 1(LL)

1.1

0.9

0.7

0.5

WB

IF 1(RR)

1.2 1.0 0.8 0.6 0.4

ON

IF 1(LL)

1.1

0.9

0.7

0.5

ON

IF 1(RR)

1.6

1.2

0.8

TR

IF 1(LL)

1.10

1.00

0.90

0.80

TR

IF 1(RR)

FREQ MHz

1652 1654 1656 1658

1.10

1.00

0.90

AR

IF 1(LL)

FREQ MHz

1652 1654 1656 1658

1.05

0.95

0.85

0.75

AR

IF 1(RR)

1.0

0.8

0.6

Plot file version 16 created 24-MAY-2005 14:28:56 J2145+11 ig002b.MSORT.1 Freq = 1.6505 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Real Jy Total-power spectrum Antenna: * Timerange: 00/15:20:03 to 00/15:22:55

WB

IF 1(LL)

1.1

0.9

0.7

0.5

WB

IF 1(RR)

1.2 1.0 0.8 0.6 0.4

ON

IF 1(LL)

1.3 1.1 0.9 0.7 0.5

ON

IF 1(RR)

1.6

1.2

0.8

TR

IF 1(LL)

1.00

0.90

0.80

TR

IF 1(RR)

FREQ MHz

1652 1654 1656 1658

1.10

1.00

0.90

AR

IF 1(LL)

FREQ MHz

1652 1654 1656 1658

1.05

0.95

0.85

0.75

AR

IF 1(RR)

1.0

0.8

0.6

Plot file version 17 created 24-MAY-2005 14:28:56 SN2001EM ig002b.MSORT.1 Freq = 1.6505 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Real Jy Total-power spectrum Antenna: * Timerange: 00/15:23:03 to 00/15:30:55

WB

IF 1(LL)

1.1

0.9

0.7

0.5

WB

IF 1(RR)

1.2 1.0 0.8 0.6 0.4

ON

IF 1(LL)

1.3 1.1 0.9 0.7 0.5

ON

IF 1(RR)

1.5

1.3

1.1

0.9

TR

IF 1(LL)

1.00

0.90

0.80

TR

IF 1(RR)

FREQ MHz

1652 1654 1656 1658

1.10

1.00

0.90

AR

IF 1(LL)

FREQ MHz

1652 1654 1656 1658

1.05

0.95

0.85

0.75

AR

IF 1(RR)

1.0

0.8

0.6

Plot file version 18 created 24-MAY-2005 14:28:56 J2145+11 ig002b.MSORT.1 Freq = 1.6505 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Real Jy Total-power spectrum Antenna: * Timerange: 00/15:31:03 to 00/15:33:55

WB

IF 1(LL)

1.1

0.9

0.7

0.5

WB

IF 1(RR)

1.2 1.0 0.8 0.6 0.4

ON

IF 1(LL)

1.3 1.1 0.9 0.7 0.5

ON

IF 1(RR)

1.5

1.3

1.1 0.9

TR

IF 1(LL)

1.00

0.90

0.80

TR

IF 1(RR)

FREQ MHz

1652 1654 1656 1658

1.8

1.4

1.0

AR

IF 1(LL)

FREQ MHz

1652 1654 1656 1658

1.6

1.2

0.8

AR

IF 1(RR)

1.0

0.8

0.6

Plot file version 19 created 24-MAY-2005 14:28:56 SN2001EM ig002b.MSORT.1 Freq = 1.6505 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Real Jy Total-power spectrum Antenna: * Timerange: 00/15:34:03 to 00/15:41:55

WB

IF 1(LL)

1.1

0.9

0.7

0.5

WB

IF 1(RR)

1.2 1.0 0.8 0.6 0.4

ON

IF 1(LL)

1.3 1.1 0.9 0.7

0.5

ON

IF 1(RR)

1.5

1.3

1.1

0.9

TR

IF 1(LL)

1.10

1.00

0.90

0.80

TR

IF 1(RR)

FREQ MHz

1652 1654 1656 1658

1.3

1.1

0.9

AR

IF 1(LL)

FREQ MHz

1652 1654 1656 1658

1.2

1.0

0.8

AR

IF 1(RR)

1.0

0.8

0.6

Plot file version 20 created 24-MAY-2005 14:28:56 J2145+11 ig002b.MSORT.1 Freq = 1.6505 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Real Jy Total-power spectrum Antenna: * Timerange: 00/15:42:03 to 00/15:44:55

WB

IF 1(LL)

1.1 0.9 0.7 0.5

WB

IF 1(RR)

1.2 1.0 0.8 0.6 0.4

ON

IF 1(LL)

1.1 0.9 0.7 0.5

ON

IF 1(RR)

1.5 1.3 1.1 0.9

TR

IF 1(LL)

1.10

1.00

0.90

0.80

TR

IF 1(RR) FREQ MHz

1652 1654 1656 1658

1.10

1.00

0.90

AR

IF 1(LL) FREQ MHz

1652 1654 1656 1658

1.05

0.95

0.85

0.75

AR

IF 1(RR)

1.0

0.8

0.6

Plot file version 21 created 24-MAY-2005 14:28:57 SN2001EM ig002b.MSORT.1 Freq = 1.6505 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Real Jy Total-power spectrum Antenna: * Timerange: 00/15:45:03 to 00/15:52:55

WB

IF 1(LL)

1.1 0.9 0.7 0.5

WB

IF 1(RR)

1.2 1.0 0.8 0.6 0.4

ON

IF 1(LL)

1.1 0.9 0.7 0.5

ON

IF 1(RR)

1.5 1.3 1.1 0.9

TR

IF 1(LL)

1.10 1.00 0.90 0.80

TR

IF 1(RR) FREQ MHz

1652 1654 1656 1658

1.10

1.00

0.90

AR

IF 1(LL) FREQ MHz

1652 1654 1656 1658

1.00

0.90

0.80

AR

IF 1(RR)

1.0

0.8

0.6

Plot file version 22 created 24-MAY-2005 14:28:57 J2145+11 ig002b.MSORT.1 Freq = 1.6505 GHz, Bw = 8.000 MH No calibration applied and no bandpass applied

Lower frame: Real Jy Total-power spectrum Antenna: * Timerange: 00/15:53:03 to 00/15:55:55

WB

IF 1(LL)

1.1

0.9

0.7

0.5

WB

IF 1(RR)

1.2 1.0 0.8 0.6 0.4

ON

IF 1(LL)

1.1

0.9

0.7

0.5

ON

IF 1(RR)

1.5

1.3

1.1

0.9

TR

IF 1(LL)

1.10

1.00

0.90

0.80

TR